{"text_format":"1","workbook":"xlsx","n_sheets":9,"sheets":[" 432.1 MHz Table","144.1 MHz Table","50.15 MHz Table","NF Calculator","Convergence Correction","Charts432MHz_GT","Charts144MHz_GT","Charts50MHz_Gain","Charts50MHz_GT"],"not_rendered":{"charts":28,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":" 432.1 MHz Table","index":0,"n_rows":317,"n_cols":23,"rows_kept":317,"cut":false,"hidden":false,"merged":[[7,1,7,2],[7,5,7,6],[8,5,8,7]]}
[]
["Issue: July 2, 2024",null,null,null,null,"VE7BQH Antenna Table"]
[]
[null,"Old Reference: Tsky=20K Tearth=350K",null,null,null,"Reference: Estimated Values for man made noise (Tearth) on 432.1 MHz:"]
[null,"New Reference: Tsky=27K",null,null,null,"Rural =",null,760,null,null,null,"Man-Made Noise in Our Living Environments"]
[null,null,null,null,null,"Residential =",null,1800,null,null,null,"U.R.S.I. Radio Science Bulletins No. 334, 09.2010"]
[null,null,null,null,null,"City =                                   7900",null,8200]
[null,"Enter Tsky > ",null,27,"K","       Enter Tearth, K >",null,1800,"                 Enter Receive System NF >",null,null,null,0.75,"dB",null,null,"K"]
[null,null,null,null,null,"            DL6WU Optimal Stacking",null,null,null,null,null," ","1 Ant.",null,null,null,null,null,null,"         Internal use only"]
[null,null,"1  Ant.",null,null,null,"    4 Antennas",null,null,null,"<","H Plane","          >",null,null,null,null,null,null,"      archive"]
["TYPE OF","Length","GAIN","E","H","GA","Tloss","TA"," G/T","S/N","F/R","1st SL","2nd SL","Z","e","VSWR","Feed","Convergence",null,"Ta",null,"    New"]
["ANTENNA","(m)","(dBi)","(m)","(m)","(dBi)","(K)","(K)","(dB/K)","(dB)","(dB)","(dB)","(dB)","(ohms)","(%)","Bandwidth","System","Correction req.",null,"          Old","Tpat","     \"S\"","avg gain"]
[]
["F5FOD Isotropic Lossless Radiator",0,0,"-","-","-",{"$f":"290*(1/W14-1)","v":7.0001689696130853E-3},{"$f":"\n\nS14/350*H$8+(1-S14/350)*D$8+290*(1/W14-1)","v":913.5044355979428},{"$f":"\nC14-10*LOG((S14/350*H$8+(1-S14/350)*D$8)+290*(10^(0.1*M$8)/W14-1))+10*LOG(1/W14)","v":-29.859417667356968},{"$f":"10*LOG(10^(C14/10)*5E-22/W14/1.380649E-23/2500/(S14/350*H$8+(1-S14/350)*D$8+290*(10^(M$8/10)/W14-1)))","v":-48.249950537499487},"-","-","    -","-",null,"      -","          -","         No",174.99949373950403,185.00299999999999,185.00046552847826,{"$f":"(U14-20)*1.0606","v":174.99949373950403},0.99997586206896549]
["KF2YN Boxkite 4",0.30527331999999996,13.24,1.2,0.85,19.3,{"$f":"290*(1/W15-1)","v":5.0152594099695058},186.74673442232233,{"$f":"\nF15-10*LOG((S15/350*H$8+(1-S15/350)*D$8)+290*(10^(0.1*M$8)/W15-1))+10*LOG(1/W15)","v":-4.4701046193764977},{"$f":"10*LOG(10^(F15/10)*5E-22/W15/1.380649E-23/2500/(S15/350*H$8+(1-S15/350)*D$8+290*(10^(M$8/10)/W15-1)))","v":-22.860637489519018},26.1,21.5,"none",52.5,{"$f":"(1-((P15-1)/(P15+1))^2)*10^2","v":99.773242630385482},1.1000000000000001,"Bent Dipole","Yes",30.544848423194299,52.9,48.799593082400811,30.544848423194299,0.98299999999999998]
["KF2YN Boxkite 7",0.92969601999999996,15.64,1.4,1.17,21.56,{"$f":"290*(1/W16-1)","v":8.3750798268643685},116.53165728558243,-0.69118926413943604,-19.081722134281957,27.6,27.5,21.3,51.7,{"$f":"(1-((P16-1)/(P16+1))^2)*10^2","v":99.940511600237954},1.05,"Bent Dipole","Yes",16.020756971546152,42.26,35.105371461009007,16.020756971546152,0.97193103448275864]
["DG7YBN GTV70-8n",1.2765975199999999,13.6,1.07,0.93,19.559999999999999,4.9842160645387672,126.19014437240065,-2.9618193300874514,-21.352352200229969,24.8,16.5,21.7,49.8,91.398319369701213,1.83,"Bent Dipole","Yes",18.59677095755875,41.8,37.534198526832689,18.59677095755875,0.98310344827586205]
["DG7YBN GTV70-9w",1.3779999999999999,13.5,0.99939999999999996,0.88370000000000004,19.373999999999999,{"$f":"290*(1/W18-1)","v":2.191435768261969},{"$f":"\n\nS18/350*H$8+(1-S18/350)*D$8+290*(1/W18-1)","v":93.959292936833393},{"$f":"\nF18-10*LOG((S18/350*H$8+(1-S18/350)*D$8)+290*(10^(0.1*M$8)/W18-1))+10*LOG(1/W18)","v":-2.3262761511382184},{"$f":"10*LOG(10^(F18/10)*5E-22/W18/1.380649E-23/2500/(S18/350*H$8+(1-S18/350)*D$8+290*(10^(M$8/10)/W18-1)))","v":-20.716809021280742},25.05,18.93,25.05,48.96,{"$f":"(1-((P18-1)/(P18+1))^2)*10^2","v":99.90385193197524},1.0640000000000001,"Bent Dipole","Yes",12.785532999999999,36.35,32.055,12.785532999999999,0.99250000000000005]
["DG7YBN GTV70-10w",1.552,14.07,1.075,0.97640000000000005,20.010000000000002,{"$f":"290*(1/W19-1)","v":2.1619987910537763},{"$f":"\n\nS19/350*H$8+(1-S19/350)*D$8+290*(1/W19-1)","v":108.40390052305378},{"$f":"\nF19-10*LOG((S19/350*H$8+(1-S19/350)*D$8)+290*(10^(0.1*M$8)/W19-1))+10*LOG(1/W19)","v":-2.0923116410793243},{"$f":"10*LOG(10^(F19/10)*5E-22/W19/1.380649E-23/2500/(S19/350*H$8+(1-S19/350)*D$8+290*(10^(M$8/10)/W19-1)))","v":-20.482844511221849},24.87,15.49,21.3,48.87,{"$f":"(1-((P19-1)/(P19+1))^2)*10^2","v":99.844880550641747},1.0820000000000001,"Bent Dipole","Yes",15.642789400000002,36.35,34.749000000000002,15.642789400000002,0.99260000000000004]
["KF2YN Boxkite 10",1.6443131099999999,16.55,1.5,1.3,22.46,9.0009599317381941,92.404054595635117,0.86769726553379312,-17.52283560460873,28.3,19.2,28,48.7,99.852071005917168,1.08,"Bent Dipole","Yes",11.134282646567359,38.31,30.498097913037299,11.134282646567359,0.96989655172413791]
["InnoV 10 LFA",1.6859412899999999,14.43,1.1200000000000001,1.03,20.36,3.7170397792756815,101.09330409248075,-1.5287112739858335,-19.919244144128353,23.8,17.2,23.3,50.7,99.627498953029601,1.1299999999999999,"LFA-LOOP","Yes",13.892663570006638,36.35,33.098871930988722,13.892663570006638,0.9873448275862069]
["InnoV 10 LFA 2018",1.7139986833199998,14.35,1.1100000000000001,1.0089999999999999,20.27,3.6965252313602415,97.305954594826531,-1.5124835444649289,-19.90301641460745,22.06,18.57,21.42,48.8,98.76543209876543,1.25,"LFA-LOOP","Yes",13.149069530295096,35.64,32.397764972935221,13.149069530295096,0.98741379310344823]
["YU7EF EF7010-5",1.7969497699999997,14.64,1.1399999999999999,1.05,20.56,5.0877192982456299,99.576328862155407,-1.273414367448892,-19.663947237591412,22.5,16.899999999999999,24.1,50,99.915166368177964,1.06,"Dipole","No",13.32262456140351,37,32.561403508771932,13.32262456140351,0.98275862068965514]
["+DG7YBN GTV 70-11w",1.9495864299999999,14.97,1.179,1.0900000000000001,20.9,2.7253741733379844,85.509411321167505,-0.54197142272597965,-18.932504292868497,27.8,15.9,23.4,50.01,99.915166368177964,1.06,"Bent Dipole","No",11.01207727114514,32.799999999999997,30.382875043508523,11.01207727114514,0.99068965517241381]
["YU7EF EF7011B-5",1.9912146099999999,15.07,1.2,1.1100000000000001,21,4.7774272695408264,95.805356967603032,-0.72948056446733611,-19.120013434609856,25.39,16.93,20.14,48.95,95.21484375,1.56,"Dipole","No",12.639467227479848,36.1,31.917280056081321,12.639467227479848,0.98379310344827586]
["Innov 11 LFA",1.9912146099999999,15.05,1.2,1.1000000000000001,20.98,4.0045446600244583,85.813374812395438,-0.4598286403754468,-18.85036151051797,25.6,16.399999999999999,23.8,50.4,99.885644939205122,1.07,"LFA-LOOP","Yes",10.819566019926587,33.74,30.201363398007341,10.819566019926587,0.98637931034482762]
["*Innov 11 LFA",1.9912146099999999,15.05,1.19,1.1000000000000001,20.96,4.0045446600244583,85.268686119609455,-0.46304707111930021,-18.853579941261824,25.61,16.399999999999999,23.8,50.44,99.885644939205122,1.07,"LFA-LOOP","Yes",10.712041461282993,33.64,30.099982520538369,10.712041461282993,0.98637931034482762]
["EAntenna 432LFA11",2.0376994109999997,15.09,1.1990000000000001,1.1100000000000001,21.02,3.9839899325340244,87.90561320196359,-0.48387935973642987,-18.874412229878956,25.35,17,24.9,47.91,98.491843644198212,1.28,"LFA-LOOP","Yes",11.236643059391058,34.11,30.594609710909918,11.236643059391058,0.98644827586206896]
["*YU7EF EF7011V6",2.09,15.128,1.18,1.1000000000000001,21.016999999999999,4.3286611720650452,68.621739531184005,0.14351060035224567,-18.247022269790278,28.05,18.77,22.42,50.39,99.978160110655438,1.03,"Bent Dipole","Yes",7.3618598001644893,30.81,26.941221761422298,7.3618598001644893,0.98529310344827581]
["*KF2YN Polly 12 CR",2.1993555099999997,15.7,1.3,1.3,21.74,3.2254802831142682,80.747298396648873,0.45197890079133224,-17.938553969351187,25.4,16.100000000000001,22.1,48.3,99.386268555288922,1.17,"Multi-Pol loop","No",9.973286147623865,32.270000000000003,29.403437815975735,9.973286147623865,0.98899999999999999]
["+*InnoV 12Y",2.2687358099999999,15.59,1.26,1.17,21.52,3.1437136184600512,77.41722595858046,0.33891956106778404,-18.051613309074739,27.6,15.9,21.8,49.7,96.868702264221241,1.43,"LFA-Loop","Yes",9.3320526334135039,31.6,28.79884276203423,9.3320526334135039,0.98927586206896556]
["+InnoV 12Y",2.2715110219999999,15.59,1.274,1.1930000000000001,21.54,3.4300966470116556,78.778929545474966,0.31706522756932537,-18.073467642573195,27.6,15.9,21.8,49.7,96.868702264221241,1.43,"LFA-Loop","Yes",9.544326855308606,32.049999999999997,28.998988172080526,9.544326855308606,0.98831034482758617]
["InnoV 12 LFA",2.2826118699999998,15.48,1.24,1.1599999999999999,21.4,4.0045446600244583,71.814875407795839,0.4134813086063911,-17.977051561536136,28.34,16.8,23.3,50.1,99.885644939205122,1.07,"LFA-LOOP","Yes",8.0561848627862283,31.17,27.595874847054713,8.0561848627862283,0.98637931034482762]
["*InnoV 12 LFA",2.2826118699999998,15.48,1.23,1.1499999999999999,21.37,4.0559440559440478,70.584713725874138,0.42610016802483763,-17.964432702117684,28.3,16.8,23.3,50.12,99.885644939205122,1.07,"LFA-LOOP","Yes",7.8031976223776249,30.98,27.357342657342659,7.8031976223776249,0.98620689655172411]
["YU7EF EF7012B-5",2.2895498999999999,15.58,1.26,1.17,21.5,4.9842160645387672,79.73733115398106,0.25966544704507277,-18.130867423097452,23.95,17.62,21.3,48.57,97.222222222222214,1.4,"Dipole","No",9.4267288670641864,33.299999999999997,28.888109435285863,9.4267288670641864,0.98310344827586205]
["EAntenna 432LFA12",2.2930189149999998,15.32,1.228,1.1399999999999999,21.24,4.385326239148684,81.386685712885523,-5.8185850507024614E-2,-18.448718720649548,28.58,16.100000000000001,24.5,50.1,96.626405664306532,1.45,"LFA-LOOP","Yes",9.8705447353682434,33.19,29.30656678801456,9.8705447353682434,0.98510344827586205]
["InnoV 12 LFA-430",2.3019689736999998,15.59,1.274,1.1930000000000001,21.54,3.1437136184600512,78.503413700024424,0.32350948413813635,-18.067023386004387,26.35,15.51,21.66,49.93,97.33723149104533,1.39,"LFA-LOOP","Yes",9.5464720973195316,31.8,29.001010840391789,9.5464720973195316,0.98927586206896556]
["WD5AGO 12B",2.31,15.59,1.266,1.179,21.52,4.7454009553816405,82.753782204524498,0.18183065264884424,-18.208702217493677,24.94,15.43,22.95,39.200000000000003,97.994068780047527,1.33,"Dipole","No",10.069336399999999,33.299999999999997,29.494,10.069336399999999,0.9839]
["WD5AGO 12C",2.3199999999999998,15.5,1.24,1.1499999999999999,21.398,4.2967322914552453,68.121194592026669,0.54180270995193125,-17.848730160190591,29.22,16.57,24.98,35.83,97.781801720235393,1.35,"Dipole","yes",7.2693523999999989,27.376999999999999,26.853999999999999,7.2693523999999989,0.98540000000000005]
["KF2YN Boxkite 13",2.3381161100000001,17.38,1.63,1.5,23.3,9.5867768595041642,97.307128606847726,1.5722505906017596,-16.818282279540764,28,18,29,50.9,99.814564684874426,1.0900000000000001,"Bent Dipole","Yes",11.986533057851238,39.58,31.301652892561982,11.986533057851238,0.96799999999999997]
["+DG7YBN GTV70-13m",2.4879775579999999,15.75,1.25,1.173,21.567,2.6846244866708524,56.25697876576281,1.1370491521351733,-17.253483718007352,29.22,17.13,22.37,49.21,99.572015023146136,1.1399999999999999,"Bent Dipole","Yes",5.2455296095218191,27.376999999999999,24.945813322196699,5.2455296095218191,0.99082758620689659]
["Innov 13 LFA",2.58094716,15.92,1.31,1.23,21.85,4.5709281961470882,68.137256420115065,0.99546725203601227,-17.395065618106507,29.54,16.5,23.2,50.06,99.51325040562466,1.1499999999999999,"LFA-LOOP","Yes",7.2183953064798585,30.89,26.805954465849386,7.2183953064798585,0.98448275862068968]
["*InnoV 13 LFA",2.58094716,15.92,1.3,1.22,21.83,4.5709281961470882,67.591518414610917,0.99467530742216781,-17.395857562720355,29.54,16.5,23.2,50.06,99.51325040562466,1.1499999999999999,"LFA-LOOP","Yes",7.1106636077057761,30.79,26.704378283712781,7.1106636077057761,0.98448275862068968]
["WD5AGO 13",2.6429999999999998,15.88,1.2809999999999999,1.2,21.76,{"$f":"290*(1/W44-1)","v":4.5657694261045982},64.178037614676029,1.0467437841789844,-17.343789085963536,25.81,17.14,21.35,33.590000000000003,97.105766085294675,1.41,"Dipole","No",6.4378419999999998,32.9,26.07,6.4378419999999998,0.98450000000000004]
["YU7EF EF7013M-6",2.6572654899999999,16.11,1.33,1.25,22.01,4.7774272695408264,78.329498508837801,0.81329595699509971,-17.577236913147424,26.41,18.670000000000002,21.8,49.44,99.915166368177964,1.06,"Dipole","No",9.1896361724500526,32.9,28.664563617245005,9.1896361724500526,0.98379310344827586]
["M2 432-12EME",2.7613359399999999,16.22,1.39,1.32,22.11,3.9737136465324019,122.85493815036747,-0.34166881762481072,-18.732201687767333,19.71,12.3,16,200.43,96.127481814809428,1.49,"Folded Dipole","Yes",18.137861577181205,40.520000000000003,37.101510067114091,18.137861577181205,0.98648275862068968]
["*M2 432-12EME",2.7613359399999999,16.22,1.42,1.37,22.17,3.9737136465324019,125.03346444471072,-0.33441967494982439,-18.72495254509235,19.71,12.3,16,200.43,96.127481814809428,1.49,"Folded Dipole","Yes",18.567914709172257,40.92,37.506991051454136,18.567914709172257,0.98648275862068968]
["F9FT 19",2.7890880599999996,15.96,1.3320000000000001,1.2589999999999999,21.88,6.1997675483393344,{"$f":"\n\nS48/350*H$8+(1-S48/350)*D$8+290*(1/W48-1)","v":106.78033535730634},-0.13972956762310448,-18.530262437765625,21.53,14.05,17.46,55.71,99.572015023146136,1.1399999999999999,"Folded Dipole","Yes",14.525210791392244,39.06,33.695277004895573,14.525210791392244,0.97906896551724143]
["DG7YBN Tonna 19 mod",2.7890880599999996,16.170000000000002,1.35,1.27,22.07,6.1997675483393344,76.214643912835612,{"$f":"\nF49-10*LOG((S49/350*H$8+(1-S49/350)*D$8)+290*(10^(0.1*M$8)/W49-1))+10*LOG(1/W49)","v":0.95451730803532309},{"$f":"10*LOG(10^(F49/10)*5E-22/W49/1.380649E-23/2500/(S49/350*H$8+(1-S49/350)*D$8+290*(10^(M$8/10)/W49-1)))","v":-17.436015562107205},22.36,14.3,18.7,44.74,99.51325040562466,1.1499999999999999,"Folded Dipole","Yes",8.4913743528334447,33.49,28.006198710949882,8.4913743528334447,0.97906896551724143]
["InnoV 14 LFA",2.7960260899999998,16.46,1.38,1.32,22.31,4.5709281961470882,67.536944614060516,1.4766007936951457,-16.913932076447377,30.78,16,22.3,52.59,99.572015023146136,1.1399999999999999,"LFA-LOOP","Yes",7.0998904378283703,30.78,26.694220665499124,7.0998904378283703,0.98448275862068968]
["*InnoV 14 LFA",2.7960260899999998,16.46,1.36,1.29,22.26,4.5709281961470882,66.500042403602691,1.4633481735870657,-16.927184696555454,30.6,16,22.3,52.59,99.572015023146136,1.1399999999999999,"LFA-LOOP","Yes",6.8952002101576184,30.59,26.50122591943958,6.8952002101576184,0.98448275862068968]
["+DG7YBN GTV70-14m",2.8189215889999995,16.38,1.38,1.31,22.31,3.8504542278127318,75.285020211640216,1.2053092316047713,-17.185223638537753,26.9,15.88,20.6,49.4,95.871494103268205,1.51,"Bent Dipole","No",8.7716289308176076,31.7,28.270440251572325,{"$f":"(U52-20)*1.0606","v":8.7716289308176076},0.98689655172413793]
["YU7EF EF7014M-6",2.9417247199999998,16.5,1.39,1.32,22.39,4.5709281961470882,81.289542352764528,1.0965239821335235,-17.294008888008999,23.76,17.91,20.48,49.47,99.72821814424654,1.1100000000000001,"Dipole","No",9.8147292469351974,33.299999999999997,29.253940455341503,9.8147292469351974,0.98448275862068968]
["RA3AQ AQ70-14f",2.9833528999999999,16.649999999999999,1.41,1.34,22.54,7.1101533243835107,73.349097795924109,1.5273619639481688,-16.863170906194348,26.11,15.9,20,53.3,99.814564684874426,1.0900000000000001,"Folded Dipole","Yes",7.7459845262488507,33.590000000000003,27.303398572740761,7.7459845262488507,0.97606896551724143]
["KF2YN Boxkite 16",3.03191911,18.02,1.74,1.61,23.85,10.539613336668685,103.08217233994107,1.9710483865486641,-16.419484483593855,27.4,17,25,49.09,99.915166368177964,1.06,"Bent Dipole","Yes",12.938463424221846,41.24,32.199192366794122,12.938463424221846,0.96493103448275863]
["*KF2YN Polly 15 CR",3.0804853200000002,16.760000000000002,1.4,1.4,22.66,3.542757417102933,68.292279924208373,1.7916445492425943,-16.598888320899928,26.7,16.3,20.3,47.4,99.097070084560102,1.21,"Multi-pol loop","No",7.4519643979057575,30.2,27.026178010471202,7.4519643979057575,0.98793103448275865]
["I0JXX 16JXX70 old ver",3.0943613799999996,16.53,1.41,1.33,22.44,4.9428350985480884,81.368101201214458,1.1472872060047097,-17.243245664137813,23.43,16.600000000000001,21.3,201.8,99.940511600237954,1.05,"T Match","Yes",9.7568207196464911,33.57,29.199340674756261,9.7568207196464911,0.98324137931034483]
["I0JXX 32JXX70 XPOL H new ver",3.0943613799999996,16.28,1.37,1.37,22.17,6.0642117862423728,123.29131776505972,-0.27107867442727529,-18.661611544569798,18.61,15,18,206.56,99.978160110655438,1.03,"T Match","Yes",17.811329437442794,41.98,36.793635147504048,17.811329437442794,0.97951724137931029]
["I0JXX 32JXX70 XPOL V new ver",3.0943613799999996,16.28,1.37,1.37,22.18,4.4471675652965237,124.95864853961804,-0.31777816199851039,-18.708311032141033,18.61,15,18,206.56,99.978160110655438,1.03,"T Match","Yes",18.459683215461101,41.22,37.404943631398361,18.459683215461101,0.98489655172413793]
["EAntenna 432LFA15",3.1747037674,15.66,1.22,1.1399999999999999,21.36,4.086792320872803,56.846502322221589,0.91765380176474498,-17.472879068377772,29.16,26.2,29.1,48.37,98.76543209876543,1.25,"LFA-LOOP","Yes",5.0851091373220951,28.48,24.794558869811517,5.0851091373220951,0.98610344827586205]
["InnoV 15 LFA",3.1845557699999998,16.68,1.42,1.34,22.57,4.8497703607615144,61.942748106841123,1.9408145460608985,-16.449718324081619,31.06,15.8,22.1,51.05,99.852071005917168,1.08,"LFA-LOOP","Yes",5.9405201416400795,29.95,25.60109385408267,5.9405201416400795,0.98355172413793102]
["YU7EF EF7015M-5",3.25393607,16.8,1.425,1.36,22.66,5.5024595924103759,79.433322827025378,1.4339141677329656,-16.95661870240956,24.25,18.96,21.1,49.45,99.978160110655438,1.03,"Dipole","No",9.2644118060435723,33.6,28.735066760365427,9.2644118060435723,0.98137931034482762]
["Konni F20",3.3059712949999995,16.690000000000001,1.444,1.3620000000000001,22.61,1.7505030181086312,82.477468732394343,1.2539592616483486,-17.136573608494171,21.93,14,16.399999999999999,210.667,99.915166368177964,1.06,"Folded Dipole","Yes",10.606,31.56,30,10.606,0.99399999999999999]
["WiMo 15 (YU7EF)",3.3926966699999994,17.059999999999999,1.46,1.3,22.87,4.3647182359117975,64.06727104555226,2.159175576954953,-16.231357293187571,22.3,17.2,20.8,174.5,74.378905654625811,3.05,"Folded Dipole","Yes",6.4556646832341578,30,26.086804340217007,6.4556646832341578,0.9851724137931035]
["InnoV 16 LFA",3.6008375699999999,17.27,1.5,1.43,23.15,4.8497703607615144,60.358609756537362,2.5797531268601821,-15.810779743282339,29.29,18.100000000000001,23.3,48.4,99.247305102062086,1.19,"LFA-LOOP","Yes",5.6278024751954581,29.66,25.306244083721911,5.6278024751954581,0.98355172413793102]
["+DG7YBN GTV70-17w",3.6285896900000001,17.29,1.51,1.44,23.2,3.0313588850173967,65.899256553509176,2.4124172359047735,-15.978115634237746,31.5,14.7,20.8,49.9,99.978160110655438,1.03,"Bent Dipole","No",7.0805212543553999,29.4,26.675958188153309,7.0805212543553999,0.98965517241379308]
["InnoV 17 LFA",3.6979699899999998,17.25,1.49,1.42,23.11,4.3441131177376651,61.964647546249097,2.4760740997146202,-15.914458770427904,27.36,18.100000000000001,23.5,49.85,99.978160110655438,1.03,"LFA-LOOP","Yes",6.0446627467450647,29.6,25.699286014279714,6.0446627467450647,0.98524137931034483]
["*InnoV 17 LFA",3.6979699899999998,17.25,1.45,1.45,23.11,4.3441131177376651,61.419329750604994,2.4962853978467523,-15.894247472295769,27.36,18.100000000000001,23.5,49.85,99.978160110655438,1.03,"LFA-LOOP","Yes",5.9370139997200031,29.5,25.597788044239113,5.9370139997200031,0.98524137931034483]
["YU7EF EF7017M-5",3.8575446799999993,17.41,1.52,1.44,23.22,5.7102672292545442,77.558304010448026,2.05637122444063,-16.33416164570189,25,18.45,22.33,50.66,99.915166368177964,1.06,"Dipole","No",8.8532503516174383,33.4,28.347398030942333,8.8532503516174383,0.9806896551724138]
["*KF2YN Polly 18 CR",3.9477390699999999,17.79,1.95,1.95,23.96,3.7478169752008395,74.040904611546324,2.8959866968913017,-15.494546173251223,28.3,14.8,20,48.1,99.318239205454091,1.18,"Multi-Pol loop","No",8.546294795668878,31.4,28.057981138665735,8.546294795668878,0.98724137931034484]
["YU7EF EF7017XM-5",3.9796540079999994,17.61,1.5529999999999999,1.486,23.451000000000001,6.5036542929568881,68.141985359357676,2.6119275712259862,-15.778605298916533,27.46,21.58,23.98,52.16,99.247305102062086,1.19,"Dipole","Yes",6.8377980108518202,32.228000000000002,26.447103536537639,6.8377980108518202,0.97806551724137936]
["RA3AQ AQ70-18f",3.9824292199999998,17.760000000000002,1.59,1.53,23.64,6.2102000563539246,71.346278530572022,2.6877444558765138,-15.70278841426601,27.24,16.100000000000001,20.5,51.7,99.852071005917168,1.08,"Folded Dipole","Yes",7.5282726824457589,32.61,27.098126232741617,7.5282726824457589,0.97903448275862071]
["InnoV 18 LFA",3.9963052799999996,17.489999999999998,1.52,1.45,23.33,4.3441131177376651,58.201954756304886,2.837485529109526,-15.553047341032995,28.2,18.5,24.8,49.8,99.940511600237954,1.05,"LFA-LOOP","Yes",5.301886392272154,28.91,24.99895002099958,5.301886392272154,0.98524137931034483]
["+DG7YBN GTV70-19m",4.1159862975000001,17.8,1.6,1.54,23.68,3.6452513966480127,64.093289060255344,2.9625310804817344,-15.428001789660787,29.6,15.4,20.2,49.3,98.491843644198212,1.28,"Bent Dipole","No",6.6028275139664778,29.5,26.225558659217874,6.6028275139664778,0.98758620689655174]
["+Konni F20 Mod YBN",4.1204960169999998,17.57,1.58,1.5,23.42,1.7505030181086312,85.720545133659087,1.962696256031671,-16.427836614110856,24.66,14.25,16.12,223.4,99.627498953029601,1.1299999999999999,"Folded Dipole","Yes",11.246201207243461,32.159999999999997,30.603621730382294,11.246201207243461,0.99399999999999999]
["YU7EF EF7018M-5",4.1628179999999997,17.579999999999998,1.53,1.46,23.33,5.6063268892794298,69.73364309113731,2.4282396471950021,-15.962293222947521,26.49,17.489999999999998,22.43,49.17,99.915166368177964,1.06,"Dipole","No",7.3291374340949025,31.9,26.9103690685413,7.3291374340949025,0.98103448275862071]
["K1FO 22",4.2321982999999994,17.850000000000001,1.63,1.56,23.75,4.8290972830850221,81.794704521247027,2.4427840401203622,-15.94774883002216,20.55,15.4,21.2,200.8,97.888815837533784,1.34,"T Match","Yes",9.86348704645048,33.57,29.299912357581068,9.86348704645048,0.98362068965517246]
["*InnoV 18 LFA 2019",4.2439929510000001,17.84,1.56,1.53,23.71,5.1705741962656031,55.304170131365197,3.3356935998304866,-15.054839270312035,30.7,16.489999999999998,28.5,48.24,99.386268555288922,1.17,"LFA-LOOP","Yes",4.5666997051804037,28.96,24.305770040713185,4.5666997051804037,0.98248275862068968]
["EAntenna 432LFA18",4.2537061930000002,17.88,1.6140000000000001,1.5529999999999999,23.76,5.7102672292545442,57.452252811533043,3.3064385977096133,-15.084094272432907,30.35,16,26.2,47.58,96.987910661840033,1.42,"LFA-LOOP","Yes",4.8842047116737017,29.73,24.605133614627288,4.8842047116737017,0.9806896551724138]
["YU7EF EF7019B-5",4.4611532899999995,17.91,1.6,1.54,23.72,5.8142806894125831,{"$f":"\n\nS80/350*H$8+(1-S80/350)*D$8+290*(1/W80-1)","v":73.331556275564054},2.6971774799133361,-15.693355390229186,25.7,17.8,23.4,50.5,99.67960128159487,1.1200000000000001,"Dipole","No",7.9983341540626141,32.700000000000003,27.541329581428073,7.9983341540626141,0.98034482758620689]
["KF2YN Polly 20 CR",4.5097194999999992,18.3,1.9,1.9,24.43,3.8504542278127318,72.018600912448861,{"$f":"\nF81-10*LOG((S81/350*H$8+(1-S81/350)*D$8)+290*(10^(0.1*M$8)/W81-1))+10*LOG(1/W81)","v":3.4352462756384403},{"$f":"10*LOG(10^(F81/10)*5E-22/W81/1.380649E-23/2500/(S81/350*H$8+(1-S81/350)*D$8+290*(10^(M$8/10)/W81-1)))","v":-14.955286594504077},28.7,14.4,19.5,48.75,99.097070084560102,1.21,"Multi-Pol loop","No",8.1268197064989529,31.1,27.662473794549268,8.1268197064989529,0.98689655172413793]
["InnoV 19 LFA",4.5374716199999998,18.18,1.68,1.63,24.1,5.1084286616604953,56.800058599199986,3.6670660161172419,-14.723466854025277,34.299999999999997,15,20.100000000000001,47.6,{"$f":"(1-((P82-1)/(P82+1))^2)*10^2","v":99.814564684874426},1.0900000000000001,"LFA-LOOP","Yes",4.8742642290687082,29.19,24.595761106042531,4.8742642290687082,0.9826896551724138]
["InnoV 19 LFA 2019",4.5548166949999995,18.12,1.71,1.6539999999999999,24.05,{"$f":"290*(1/W83-1)","v":7.1941479963248618},60.700691509546402,3.4848785939823701,-14.905654276160147,26.97,15.19,30,50.1,68.374758797025621,3.57,"LFA-LOOP","Yes",5.2325382005795484,31.35,24.933564209484771,5.2325382005795484,0.97579310344827586]
["Tonna 21 DX",4.5846502239999998,17.91,1.6679999999999999,1.609,23.8,6.8060702311628845,117.10514666646503,1.5189376114146407,-16.871595258727886,20.48,14.48,18.18,58.39,84.192190448541155,2.3199999999999998,"Folded Dipole","Yes",16.443698111875776,41.34,35.504146814893247,{"$f":"(U84-20)*1.0606","v":16.443698111875776},0.97706896551724143]
["KF2YN Boxkite 22",4.6484800999999996,19.260000000000002,1.99,1.9,25.14,11.163831692032254,95.138465020488553,3.4882268893791997,-14.902305980763321,29,16.2,21.2,52.1,99.386268555288922,1.17,"Bent Dipole","Yes",11.247107538048342,40.22,30.604476275738584,11.247107538048342,0.96293103448275863]
["DG7YBN GTV70-21n",4.6949649009999996,18.82,1.6819999999999999,1.6279999999999999,24.081,7.2477193924977339,53.366026296996239,3.7981161343932328,-14.592416735749286,32.35,14.82,21.14,48.3,96.253902185223723,1.48,"Bent Dipole","Yes",3.7740594566127901,30.055,23.558419250059202,3.7740594566127901,0.97561724137931038]
["InnoV 20 LFA",4.8496829699999999,18.28,1.73,1.67,24.31,5.1084286616604953,50.895333474028284,4.1113643680632732,-14.279168502079244,35.15,15.1,20.7,50.46,99.814564684874426,1.0900000000000001,"LFA-LOOP","Yes",3.708638851849253,28.11,23.496736613095656,3.708638851849253,0.9826896551724138]
["InnoV 20 LFA 2019",4.8559271969999998,18.440000000000001,1.7549999999999999,1.696,24.38,5.980854508340947,49.947563291134152,4.2262379535559731,-14.164294916586551,30,14.67,22.37,48,95.61155462513085,1.53,"LFA-LOOP","Yes",3.349322094742031,28.55,23.157950306187093,3.349322094742031,0.97979310344827586]
["+YU7XL QY721104D14",4.8843731199999993,18.420000000000002,1.88,1.82,24.47,3.4403349616189849,52.373534503040574,4.1995574569819487,-14.190975413160574,27.68,18.54,22.82,201.1,98.491843644198212,"1.28","LFA 200 Ώ","Yes",4.3297348220516385,27.2,24.082344731332867,4.3297348220516385,0.98827586206896556]
["RA3AQ AQ70-21f",4.9537534199999991,18.54,1.73,1.67,24.41,7.1101533243835107,58.817420783680369,3.9148929551431402,-14.475639914999386,27.87,16.8,21.3,52.3,99.885644939205122,1.07,"Folded Dipole","Yes",4.8773511622977441,30.95,24.598671659718786,4.8773511622977441,0.97606896551724143]
["BVO70-7.2 WL modified",4.9690170859999991,18.489999999999998,1.7549999999999999,1.696,24.42,3.8504542278127318,81.817858810022955,3.1034474391852909,-15.287085430957228,22.56,14.9,19.100000000000001,49.51,99.915166368177964,1.06,"Dipole","No",10.061247379454922,32.9,29.486373165618446,10.061247379454922,0.98689655172413793]
["Directive DSEFO432-25",5.1269960290999999,18.57,1.74,1.6890000000000001,24.47,5.1809343301393307,66.584597328680232,3.6752364690333477,-14.715296401109175,25.39,15.9,20.5,198.196,97.45074500388391,1.38,"T Match","Yes",6.791473237162613,31.03,26.403425643185567,6.791473237162613,0.98244827586206895]
["*Directive DSEFO432-25 ",5.1269960290999999,18.57,1.778,1.6759999999999999,24.47,4.9842160645387672,66.347990873377782,3.6820767744904681,-14.708456095652053,25.39,15.9,20.5,198.196,97.45074500388391,1.38,"T Match","Yes",6.7835990880392867,30.85,26.396001403016488,6.7835990880392867,0.98310344827586205]
["Directive DSEFO432-25XPOL H",5.1272041699999997,18.57,1.7270000000000001,1.7270000000000001,24.48,5.2016567798097224,66.068372013659385,3.7037832396237529,-14.686749630518769,25.4,15.9,20.5,198.2,97.45074500388391,1.38,"T Match","Yes",6.6854767805117765,30.95,26.303485555828566,6.6854767805117765,0.98237931034482762]
["Directive DSEFO432-25XPOL V",5.1272041699999997,18.57,1.7270000000000001,1.7270000000000001,24.48,5.5024595924103759,65.856220317638773,3.7137565415895688,-14.676776328552956,25.4,15.9,20.5,198.2,97.45074500388391,1.38,"T Match","Yes",6.5842167252283899,31.12,26.208011243851018,6.5842167252283899,0.98137931034482762]
["InnoV 22 LFA 2019-2",5.1847898189999997,18.84,1.8180000000000001,1.7549999999999999,24.74,6.8479757156471504,45.954606230630738,4.7591455824291851,-13.631387287713338,31.15,14,28.03,46.2,79.29378048689945,2.67,"LFA Loop","Yes",2.3899157812996359,28.43,22.253362041579894,2.3899157812996359,0.97693103448275864]
["InnoV 21 LFA 2019",5.2069915149999995,18.53,1.8180000000000001,1.7549999999999999,24.58,6.5758013894276583,48.979413593015572,4.4702593560280999,-13.920273514114424,28.19,14.13,26.35,47.9,95.61155462513085,1.53,"LFA Loop","Yes",3.0407581902175798,28.79,22.867016962302074,3.0407581902175798,0.97782758620689658]
["+DG7YBN GTV70-23m",5.2382126499999995,18.649999999999999,1.76,1.7,24.51,3.8504542278127318,54.053294766896286,4.1753339554835227,-14.215198914659002,32.299999999999997,15.7,21.8,48.4,95.21484375,1.56,"Bent Dipole","Yes",4.5803689727463306,27.8,24.318658280922431,4.5803689727463306,0.98689655172413793]
["YU7EF EF7021B-5",5.2659647699999992,18.66,1.74,1.68,24.5,8.0155917788802356,62.831005282980655,3.8626626179860093,-14.527870252156511,29.6,20.260000000000002,21.74,50.2,97.994068780047527,1.33,"Dipole","No",5.4909163713678213,32.299999999999997,25.17717930545712,5.4909163713678213,0.97310344827586204]
["EA1DDO 22 Quad V3",5.4379999999999997,17.54,1.5189999999999999,1.496,22.925999999999998,3.7601296596434142,76.444168606500554,1.7821813416158712,-16.608351528526651,22.22,14.75,20.78,50.88,98.936234390395953,1.23,"Dipole","Yes",9.0182818000000005,28.28,28.503,9.0182818000000005,0.98719999999999997]
["I0JXX 25JXX70",5.4879817299999996,18.53,1.74,1.68,24.41,5.7206652835894278,73.519833734157828,3.3800663069355448,-15.010466563206977,23.91,21.3,24.8,198.6,99.67960128159487,1.1200000000000001,"T Match","Yes",8.0539813636203821,32.67,27.593797250254934,8.0539813636203821,0.98065517241379307]
["InnoV 22 LFA 2019",5.5178152589999998,18.84,1.851,1.8009999999999999,24.77,6.9213387939556874,44.847314027478006,4.837068517458559,-13.553464352683964,32,13.91,28.46,46.2,79.429066260563161,2.66,"LFA Loop","Yes",2.1568479028385839,28.28,22.033611071882504,2.1568479028385839,0.9766896551724138]
["KF2YN Polly 24 CR",5.6544944499999996,19.149999999999999,1.9,1.9,25.11,3.7478169752008395,71.864052350681092,4.1196606163211333,-14.270872253821388,29.5,13.1,19.14,51.8,99.572015023146136,1.1399999999999999,"Multi-Pol loop","No",8.1165721271393636,31,27.65281173594132,8.1165721271393636,0.98724137931034484]
["*Antennas-Amplifiers PA432-23-6A",5.6947350239999999,18.88,1.9,1.9,24.9,6.8584539357571384,47.949218328879041,4.8350369938997346,-13.555495876242791,36.26,16.96,26.91,49.14,99.814564684874426,1.0900000000000001,"Hair Pin","Yes",2.7815947758559867,28.8,22.622661489587014,2.7815947758559867,0.97689655172413792]
["+YU7XL QY724104D17",5.7932550499999991,19.010000000000002,2,1.9,24.99,3.4403349616189849,51.829891095603656,4.7415376203337543,-13.648995249808769,31.67,18.71,22.77,199,98.936234390395953,"1.23","LFA 200 Ώ","Yes",4.222416608513611,27.1,23.981158408932313,4.222416608513611,0.98827586206896556]
["+DG7YBN GTV70-25m",5.8210071699999997,18.97,1.8009999999999999,1.74,24.84,3.2357043235704408,48.819089954174146,4.7139034405794771,-13.676629429563047,32.6,16.3,22.1,41.2,98.76543209876543,"1.25","Bent Dipole","No",3.668463040446305,26.4,23.458856345885636,3.668463040446305,0.98896551724137927]
["InnoV 23 LFA ",5.8279451999999994,19.16,1.87,1.82,25.08,5.6998699061214042,48.836283574115797,4.9701958233882886,-13.420337046754231,31.75,15.9,21.7,45.2,98.936234390395953,1.23,"LFA-LOOP","Yes",3.1854172497450848,28.15,23.003410569248619,3.1854172497450848,0.98072413793103452]
["*InnoV 23 LFA",5.8279451999999994,19.16,1.89,1.85,25.06,5.6998699061214042,48.836283574115797,4.950195823388289,-13.440337046754234,31.8,15.9,21.7,45.2,98.936234390395953,1.23,"LFA-LOOP","Yes",3.1854172497450848,28.15,23.003410569248619,3.1854172497450848,0.98072413793103452]
["DJ9BV BVO70-8.5wl",5.8473716840000005,19.14,1.9490000000000001,1.903,25.13,5.0877192982456299,100.12302430275695,3.2813144943332033,-15.10921837580932,24.25,14.85,17.75,203.9,96.626405664306532,1.45,"Folded Dipole","Yes",13.430545263157901,37.1,32.663157894736848,13.430545263157901,0.98275862068965514]
["InnoV 23 LFA 2019",5.8487592899999994,19.02,1.8680000000000001,1.8180000000000001,24.94,6.5444287729195949,43.990496789441863,5.041707054247329,-13.348825815895189,32.19,14.4,27.59,47.4,98.097502972651611,1.32,"LFA-LOOP","Yes",2.0621115655853326,27.86,21.944287729196052,2.0621115655853326,0.97793103448275864]
["DJ9BV OPT70-8.5wl",5.8556973199999991,19.04,1.8,1.754,24.87,4.9635241301907662,83.039190715688619,3.524802871986199,-14.865729998156322,23.22,15.8,20.12,186.1,95.21484375,1.56,"Folded Dipole","Yes",10.0826188973064,33.89,29.506523569023571,10.0826188973064,0.98317241379310349]
["EAntenna 432LFA23",5.8584725320000004,18.96,1.9019999999999999,1.8420000000000001,24.89,8.2798368505054416,{"$f":"\n\nS112/350*H$8+(1-S112/350)*D$8+290*(1/W112-1)","v":47.078998819040883},4.8710282293351028,-13.519504640807419,31.99,14.2,30.9,47.84,64.096128127999478,3.99,"LFA-LOOP","Yes",2.3292197907430379,29.63,22.196134066323815,2.3292197907430379,0.97224137931034482]
["YU7EF EF7023B-5",5.87651141,18.98,1.79,1.73,24.78,6.5339727090017856,56.666442591486287,{"$f":"\nF113-10*LOG((S113/350*H$8+(1-S113/350)*D$8)+290*(10^(0.1*M$8)/W113-1))+10*LOG(1/W113)","v":4.3627787823350426},{"$f":"10*LOG(10^(F113/10)*5E-22/W113/1.380649E-23/2500/(S113/350*H$8+(1-S113/350)*D$8+290*(10^(M$8/10)/W113-1)))","v":-14.02775408780748},30.47,19.600000000000001,21.9,48.6,99.097070084560102,1.21,"Dipole","No",4.5664774161700938,30.16,24.30556045273439,4.5664774161700938,0.97796551724137926]
["RA3AQ AQ70-24f",5.9112015599999994,19.22,1.87,1.82,24.82,6.1997675483393344,51.46576268939522,4.6058667520689118,-13.784666118073609,30,15.1,21,52.04,99.627498953029601,1.1299999999999999,"Folded Dipole","Yes",3.6058084034797298,28.98,23.39978163631881,3.6058084034797298,0.97906896551724143]
["InnoV 24 LFA",6.1679086700000001,19.32,1.92,1.87,25.25,5.9912716010276927,46.946327630712304,5.2213567398530296,-13.169176130289488,33.42,15.3,22.1,46.38,99.247305102062086,1.19,"LFA-LOOP","Yes",2.7548051948051966,28.01,22.597402597402599,2.7548051948051966,0.97975862068965514]
["*InnoV 24 LFA",6.1679086700000001,19.32,1.89,1.84,25.22,5.9912716010276927,46.397958220331731,5.2145987604694932,-13.17593410967303,33.4,15.3,22.1,46.4,99.247305102062086,1.19,"LFA-LOOP","Yes",2.6465540421637974,27.91,22.495336641678104,2.6465540421637974,0.97975862068965514]
["YU7EF EF7024B-5",6.1748466999999998,19.190000000000001,1.84,1.79,25.02,7.6991150442477991,59.06167896637168,4.520076551433144,-13.870456318709376,30.3,20.5,22.4,50.1,94.674556213017752,1.6,"Dipole","No",4.8093047787610592,31.4,24.53451327433628,{"$f":"(U117-20)*1.0606","v":4.8093047787610592},0.97413793103448276]
["Innov 24 LFA 2019-b",6.2053740319999999,19.2,1.885,1.8340000000000001,25.11,6.2936865839910201,44.079208379368694,5.2062317429785026,-13.184301127164016,33.229999999999997,30.61,29.43,50.1,94.674556213017752,1.6,"LFA-LOOP","Yes",2.1291216178128529,27.7,22.007468996617813,2.1291216178128529,0.97875862068965513]
["M2 432-9WLA",6.3760495699999993,19.399999999999999,2.02,1.96,25.33,7.404342598486453,121.99993023875197,2.9337974049942517,-15.456735465148268,23.24,15.8,18.100000000000001,167.2,87.556686670646528,2.09,"Folded Dipole","Yes",17.291853172077232,42.62,36.303840441332483,17.291853172077232,0.97510344827586204]
["*M2 432-9WLA",6.3760495699999993,19.399999999999999,1.8280000000000001,1.879,25.23,7.152144724754419,104.57125974035149,3.2787562231523064,-15.11177664699021,23.24,15.8,18.100000000000001,167.2,87.556686670646528,2.09,"Folded Dipole","Yes",13.901122535509858,39.29,33.106847572609709,13.901122535509858,0.97593103448275864]
["+YU7XL QY728107D21",6.9449680299999992,19.64,2.2200000000000002,2.06,25.65,3.4403349616189849,52.373534503040574,5.3795574569819484,-13.010975413160573,28.6,19.14,24.07,198.1,98.396292976869248,"1.29","LFA 200","Yes",4.3297348220516385,27.2,24.082344731332867,4.3297348220516385,0.98827586206896556]
["Antennas-Amplifiers PA432-26-7BGP",6.9588440899999986,19.600000000000001,1.95,1.95,25.49,7.5569197020892309,45.416558803140823,5.5367734325160205,-12.853759437626495,36.299999999999997,16.23,28.18,47.92,99.885644939205122,1.07,"HairPin","No",2.1437527836255263,28.827000000000002,22.021264174642209,2.1437527836255263,0.97460344827586209]
["YU7EF EF7027B-5",7.0629145399999995,19.670000000000002,1.94,1.89,25.47,8.0155917788802356,62.278885507745287,4.8528580089619613,-13.537674861180559,25.6,20,23.16,50.25,94.123048668503216,1.64,"Dipole","No",5.3819248759744873,32.200000000000003,25.074415308291993,5.3819248759744873,0.97310344827586204]
["Hy-Gain UB-7031DX",7.2294272599999996,19.54,1.92,1.86,25.33,5.3364236550077386,77.429641823691099,4.1673699201507066,-14.223162949991814,26.23,18.3,21.1,199.5,98.676482105098287,1.26,"T Match","Yes",8.9016505127124521,33.119999999999997,28.393032729315909,8.9016505127124521,0.98193103448275865]
["WiMo 27 (YU7EF)",7.2363652899999993,19.43,1.851,1.8,25.08,4.3647182359117975,50.160693815690763,4.9062196036101557,-13.484313266532364,27.09,20.5,22.62,191.8,78.621805989131687,2.72,"Folded Dipole","Yes",3.7104294714735699,27.45,23.498424921246059,3.7104294714735699,0.9851724137931035]
["+DG7YBN GTV70-30m",7.2752182579999998,19.739999999999998,1.94,1.885,25.58,3.9531632296399688,43.85439547211265,5.6708302407499875,-12.719702629392533,32.86,18.899999999999999,26,42.5,98.491843644198212,1.28,"Bent Dipole","No",2.5467745543516287,26,22.401258301293257,2.5467745543516287,0.98655172413793102]
["K1FO 33",7.3612498299999993,20.03,2.08,2.04,25.95,6.2623736217282939,66.594025194430088,5.1635467366370627,-13.226986133505461,22.03,15.5,22.2,200.5,99.247305102062086,1.19,"T Match","Yes",6.5798522563145125,31.78,26.203896149645967,6.5798522563145125,0.9788620689655172]
["Directive DSEFO432-33",7.3612498299999993,20.03,2.08,2.04,25.95,6.2623736217282939,66.594025194430088,5.1635467366370627,-13.226986133505461,22.03,15.5,22.2,200.5,99.247305102062086,1.19,"T Match","Yes",6.5798522563145125,31.78,26.203896149645967,6.5798522563145125,0.9788620689655172]
["RA3AQ AQ70-30f",7.9024161699999995,20.329999999999998,2.08,2.04,26.08,5.6375013182409255,46.611762903645356,6.0631572880484867,-12.32737558209404,30.57,16.8,22.1,51.59,99.773242630385482,1.1000000000000001,"Folded Dipole","Yes",2.7585964776602077,27.7,22.600977255949658,2.7585964776602077,0.98093103448275865]
["InnoV 30 LFA ",8.0758669199999993,20.45,2.27,2.2200000000000002,26.42,6.8270214943705092,57.968411411024988,5.9550177686430201,-12.435515101499499,36.6,13.9,20.3,49.6,83.330415601694625,2.38,"LFA-LOOP","Yes",4.7656438075742065,30.6,24.493346980552712,4.7656438075742065,0.97699999999999998]
["*YU7EF EF7032-5",8.6655994700000001,19.97,1.94,1.9,25.58,6.7966431276225414,52.766864365396131,5.3177673899037243,-13.0727654802388,27.7,23.1,24.2,51.27,69.799529258988713,3.44,"Dipole","No",3.7448265274792747,29.632999999999999,23.530856616518268,3.7448265274792747,0.97709999999999997]
["InnoV 33 LFA",9.0402530899999984,20.85,2.3199999999999998,2.29,26.81,5.4297959040292447,53.379292494065822,6.5135708725279979,-11.876961997614522,36.549999999999997,13.3,19.2,50.07,99.386268555288922,1.17,"LFA-LOOP","Yes",4.1355464221730402,28.79,23.899251765201811,4.1355464221730402,0.98162068965517246]
["DJ9BV OPT70-13wl",9.2171728549999994,20.85,2.3460000000000001,2.2930000000000001,26.8,5.2431104089871772,79.530762065046758,5.5685408469230016,-12.821992023219519,25.93,14.75,19.670000000000002,183,96.748185971513038,1.44,"Folded Dipole","Yes",9.3348438125329114,33.44,28.801474460242233,9.3348438125329114,0.98224137931034483]
["M2 432-13WLA",9.2206418699999979,20.81,2.3199999999999998,2.2799999999999998,26.69,7.341253005232633,119.2512857950987,4.3607333497012091,-14.029799520441316,22.36,19.2,20.9,199.9,83.760302962797951,2.35,"Folded Dipole","Yes",16.76170980059398,42.08,35.803988120492157,16.76170980059398,0.97531034482758616]
["*M2 432-13WLA",9.2206418699999979,20.81,2.0819999999999999,2.0819999999999999,26.4,7.983913829146438,129.0322791393038,3.8414701439525532,-14.54906272618997,22.36,19.2,20.9,199.9,83.760302962797951,2.35,"Folded Dipole","Yes",18.565667150905291,44.27,37.504871912978778,18.565667150905291,0.9732068965517241]
["InnoV 34 A LFA 2019",9.3524644400000003,20.98,2.403,2.375,26.95,6.5862604034419299,53.93945075831769,6.6396632625704344,-11.750869607572088,37.81,12.89,18.04,50.12,94.261880322109619,1.63,"LFA-LOOP","Yes",4.0178322753561844,29.7,23.788263506841584,4.0178322753561844,0.97779310344827586]
["I0JXX 39JXX70",9.387154589999998,20.16,2,1.97,25.86,6.439901304194537,60.869628882823861,5.2828470941282095,-13.107685776014311,26.05,26.7,27,194,99.247305102062086,1.19,"T Match","Yes",5.4147798378568899,30.86,25.105393020796615,5.4147798378568899,0.97827586206896555]
["InnoV 34 LFA B 2019",9.3940926199999986,20.89,2.403,2.375,26.89,7.3727944556416318,54.954738041390762,6.545404598584514,-11.845128271558007,37.25,12.71,17.93,50.12,88.29639889196676,2.04,"LFA-LOOP","Yes",4.0629894275308498,30.43,23.830840493617622,4.0629894275308498,0.9752068965517241]
["*InnoV 34 LFA B 2019",9.3940926199999986,20.89,2.2000000000000002,2.2000000000000002,26.72,7.0786675615528232,48.589825845188003,6.6298406883485423,-11.760692181793978,37.25,12.71,17.91,50.12,88.29639889196676,2.04,"LFA-LOOP","Yes",2.8645828535094835,29.07,22.70090783849659,2.8645828535094835,0.97617241379310349]
["InnoV 35 LFA 2019",9.6716138199999993,20.95,2.46,2.4300000000000002,26.93,7.6569689247540174,59.386889966528123,6.417515211393626,-11.973017658748898,36.67,12.7,18.100000000000001,49.1,79.024096474027075,2.69,"LFA-LOOP","Yes",4.8818231046931384,31.43,24.602888086642597,4.8818231046931384,0.97427586206896555]
["InnoV 38 LFA",10.69150423,21.45,2.2999999999999998,2.35,27.23,7.0576807601285712,47.514567266433524,7.1845795473293874,-11.205953322813134,36.9,12.7,17,49.3,90.810863310225926,1.87,"LFA-LOOP","Yes",2.6564637773303632,28.86,22.504680159655255,2.6564637773303632,0.97624137931034483]
["*InnoV 38 LFA",10.69150423,21.45,2.59,2.56,27.26,6.4712518066767828,46.359890072468495,7.2594088988997116,-11.131123971242813,36.9,12.7,17,49.3,90.810863310225926,1.87,"LFA-LOOP","Yes",2.5442884337434282,28.24,22.398914231325126,2.5442884337434282,0.97817241379310349]
["InnoV 39 LFA 2019",10.957924581999999,21.59,2.524,2.4929999999999999,27.54,6.2832481944689178,46.809156138604401,7.5191118832629789,-10.871420986879542,39.54,12.9,18.899999999999999,49.22,99.51325040562466,1.1499999999999999,"LFA-LOOP","Yes",2.6700889906640821,28.19,22.517526862779636,2.6700889906640821,0.97879310344827586]
["InnoV 40 LFA 2019",11.273604946999999,21.82,2.589,2.556,27.63,7.1731448763250754,46.135463285007575,7.6435931874141776,-10.746939682728341,35.64,12.74,19.16,51.8,95.347943098808159,1.55,"LFA-LOOP","Yes",2.3614277738515934,28.69,22.226501766784455,2.3614277738515934,0.97586206896551719]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-",null,null,1]
["Only Antennas that have actually been built are posted in these Tables, except for the F5FOD Isotropic Lossless Radiator."]
[]
["Thanks to Vladimir, UR5EAZ for establishing the Interactive Mode in the 144 and 432 Tables"]
["Thanks to Hartmut,  DG7YBN for his ongoing support and many inputs to the Tables"]
[]
["Legend:"]
[]
["1. L      = Length in Wavelengths"]
[]
["2. Gain  = Gain in dBi of a single antenna"]
[]
["3. E      = E plane (Horizontal) stacking in Meters. "]
[]
["4. H      = H plane (Vertical) stacking in Meters."]
[]
["5. Ga     = Gain in dBi of a 4 bay array"]
[]
["6. Tloss = Noise temperature due to ohmic losses in the antenna (K) at an actual antenna temperature of 290 K."]
[]
["7. Ta     = Noise temperature of the antenna array (K) is the mixture of the antenna array pattern, the sky temperature, "]
["               ground and the ohmic losses in the antenna array."]
[]
["8. F/R    = Front to Rear in dB over the rear 180 degrees of an antenna using either E or H plane. "]
[]
["9. Z ohms = The natural impedence of a single antenna in free space.  "]
[]
["10. VSWR  = VSWR Bandwidth is based a single antenna over 432.000 - 435.000 MHz with a "]
["                    reference at 432.300 MHz. This parameter gives an indicator of the"]
["                    antenna \"Q\" and what to expect with with stacking and wet weather.  "]
[" "]
["11. G/T = Figure of merit; a system parameter used to determine the receive capability of the antenna or array"]
["               as part of the radio receiving system. The more positive value thebetter.",null,null,null,"value the"," better."]
[]
["12. S/N = Figure of merit; a system parameter used to determine the receive capability of the antenna or array"]
["               as part of the radio receiving system. The more positive value the better."]
[]
["13. e   = Radiation Efficiency; a system parameter which describes how efficiently an antenna transmits and receives signals."]
[]
["   Notes:"]
["        "]
["1. The programs used to calculate E/H Stacking,G,Ta,Tlos and G/T are"]
["   EZNEC 5+ by Roy Lewallen W7EL,4NEC2 by Arie Voors and Tant.exe by Sinisa, YT1NT/VE3EA or AGTC_lite by F5FOD/DG7YBN "]
["   This combination of software provides excellent accuracy. Segment Density is"]
["   25 segments per half wave."]
[]
["2. Temperatures initially used: Tsky=20 degrees;Tearth=350 degrees"]
["    Temperatures now adjustable to Tsky=27 Kelvin. Tearth: Rural = 460K Kelvin, Residential = 1800K Kelvin, City = 7900 Kelvin"]
[]
["3. Dipole Z is measured at 432.1 MHz"]
[]
["4. F/R, 1st and 2nd Side Lobes (SL) have been calculated on a single antenna"]
[]
["5. No stacking harness losses or H frame effects are included in the 4 bay gain figures."]
[]
["6. All stacking dimensions EXCEPT those marked with a \"*\" and \"#\" are"]
["    calculated from the DL6WU stacking formula:"]
["    D = W/(2* sin(B/2))"]
["    Where:"]
["    D = stacking distance,vertical or horizontal"]
["    W = wavelength, in the same units as D"]
["    B = beamwidth between -3dB points."]
["    Use vertical beamwidth for vertical stacking (as above),"]
["    Use horizontal beamwidth for horizontal stacking."]
[]
["7. Antennas marked with a \"*\" have stacking dimensions recommended by "]
["   the manufacturer or designer."]
[]
["8. Antennas marked with a \"#\" have stacking dimensions for XPOL"]
["   antennas by VE7BQH."]
[]
["9. Antennas marked with a \"+\" have some or all elements over 6mm. All others"]
["   are 4MM to 6MM."]
[]
["10. FD = Folded Dipole    "]
[]
["11.  Convergence Correction: NEC2 and NEC 4 are incapable of handling complex "]
["      feed systems accurately like Folded Dipoles, T Matches, LFAs etc."]
["      Convergence Correction using the KF2YN Excel program is required. "]
["      See DUBUS 4/2010 \"The Correction of Convergence Errors in Antenna"]
["      Temperature Calculations by Brian Cake, KF2YN for details."]
[]
["12.Earth Temperature Definition"]
["       Rural: Open countryside with largely agricultural activity, building density < 1/ha, no major roads, no electrified railways."]
["       Residential: Villages and pure residential areas with no commercial or industrial activities. No electrified railways and no major roads and no high voltage overhead lines or facilities within 1 km."]
["       City: Dense commercial or industrial buildings and offices. Major roads and railways can be in the vicinity, but should not be dominating."]
[]
["13. Manufacturer/Designer Legend: Single click on Sites in blue"]
[]
["   Antennas-Ampifiers=Antenna-Amplifiers",null,null,"K1FO = K1FO"]
["   AF9Y = AF9Y",null,null,"K2GAL = K2GAL"]
["   BVO = Eagle/DJ9BV",null,null,"K5GW = Texas Towers/K5GW"]
["  BQH = VE7BQH",null,null,"KF2YN = KF2YN"]
["   CC = Cushcraft",null,null,"M2 = M²"]
["   CC MOD = VE7BQH",null,null,"MBI = F/G8MBI/F5VHX"]
["   CD = CUE DEE ",null,null,"OZ5HF = Vargarda"]
["   CD MOD = VE7BQH",null,null,"RA3AQ = RA3AQ"]
["   CT1FFU = CT1FFU",null,null,"RU1AA = RU1AA"]
["   DD0VF = DD0VF",null,null,"SHARK = SHARK (Italian)"]
["   DG7YBN = DG7YBN",null,null,"SM2CEW = SM2CEW/VE7BQH"]
["   DJ9BV = DJ9BV",null,null,"SV = Svenska Antennspecialisten AB "]
["   DJ9BV OPT = DJ9BV",null,null,"Tonna = F9FT"]
["   DK7ZB = DK7ZB",null,null,"UA9TC = UA9TC"]
["   Dual = Antennas-Amplifiers",null,null,"UR5CSZ = UR5CSZ"]
["   Eantenna = EAntenna",null,null,"Vine = G0KSC Design"]
["   EKM MOD = SM2EKM",null,null,"WiMo = WiMo"]
["   F9FT = F9FT",null,null,"W1JR = VE7BQH (Mininec error)"]
["   Flexa = FlexaYagi",null,null,"WB9UWA = WB9UWA"]
["   G0KSC LFA = G0KSC",null,null,"YU7EF = YU7EF"]
["   G4CQM = G4CQM",null,null,"YU7XL = YU7XL"]
["   HG = HYGAIN"]
["   I0JXX = I0JXX"]
["   IK0BZY = IK0BZY"]
["   InnoVAntennas = G0KSC"]
[]
["Using this Chart:"]
[]
["Programmable Tsky and Tearth: Tsky and Tearth may be changed to meet a Stations individual characteristics."]
["                                                    Click on the Red number to change then click on the green to set."]
[]
["Antennas with good G/T can provide significant benefit with today's high noise levels. "]
["Other factors like ease of matching and wet weather performance should be considered in the the decision making. ",null,null,null,"Lionel H. Edwards"]
["Antennas with 50 ohm feed systems and good VSWR bandwidth (Q) may be the best feed system choice. "]
[" "]
[null,null,null,null,"Lionel H. Edwards"]
[null,null,null,null,"VE7BQH"]
[null,null,null,null,"Issue 26, July 2, 2024"]
[]
[]
[]
["Issue 1: Add YU7EF 32,InnoV 34 LFA,InnoV 38 LFA,InnoV 40 LFA,DG7YBN 19,KF2YN Boxkite 4,KF2YN Boxkite 4,KF2YN Boxkite 7,"]
["Issue 1: Add KF2YN Boxkite 10,KF2YN Boxkite 13,KF2YN Boxkite 16,KF2YN Boxkite 22,WiMo 27 (YU7EF),DG7YBN 14,DG7YBN 23,"]
["Issue 1: Add DJ9BV OPT70 8.5wl,WiMo 15 (YU7EF),InnoV 24 LFA,InnoV30 LFA,"]
["Issue 2: Add DJ9BV OPT70 13wl,K1FO 22,K1FO 33,YU7EF 23B,DJ9BV BVO70 8.5wl,Tonna 21 DX,Konni F20,"]
["Issue 2: Add YU7EF 27,24,21,19,18,15,14,13,12,11,10,I0JXX 30,I0JXX 25,I0JXX 16,RA3AQ 14,RA3AQ 30,RA3AQ 24,"]
["Issue 2: Add RA3AQ 21,RA3AQ 18,InnoV 20 LFA,InnoV 19 LFA,InnoV 18 LFA,InnoV 17 LFA,InnoV 16 LFA,InnoV 10 LFA,"]
["Issue 2: Add KF2YN Polly 15 CR,18 CR,20 CR,24 CR,InnoV 1111 LFA,12 LFA,13 LFA,15 LFA,20 LFA,23 LFA, 33 LFA,"]
["Issue 3: Add YU7XL QY721104D14,YU7XL QY724104D17, YU7XL QY728107D21"]
["Issue 4: Add DG7YBN Tonna 19 mod,"]
["Issue 5: Add EAntenna 432LFA11,EAntenna 432LFA12,EAntenna 432LFA15,EAntenna 432LFA18,EAntenna 432LFA23,"]
["Issue 6: Add Hy-Gain UB-7031DX,M2 432-13WLA,M2 432-12EME,M2 432-9WLA,"]
["Issue 7: Add Directive DSEFO432-33,Directive DSEFO432-25,Konni F20,Directive DSEFO432-25XPOL,I0JXX 32JXX70 XPOL new ver,"]
["Issue 8: Add BVO70-7.2 modified,DG7YBN GTV 70-11W"]
["Issue 9: Add DG7YBN GTV70-25,DG7YBN GTV70-30"]
["Issue 10: Add Programmable Tsky and Tearth"]
["Issue 11: Add DG7YBN GTV70-8n,DG7YBN GTV70-17w"]
["Issue 12: Revised Konni F20 mod YBN,"]
["Issue 13: Add Revised YU7EF EF7018M-5,InnoV 12Y,"]
["Issue 14: Add InnoV 10 LFA 2018,Innov 12 LFA-430, InnoV 24 LFA 2019"]
["Issue 15: Add Innov 18 LFA 2019,Innov 19 LFA 2019,Innov 20 LFA 2019,Innov 21 LFA 2019,"]
["Issue 15: Add Innov 22 LFA 2019,Innov 22 LFA 2019-2,Innov 23 LFA 2019"]
["Issue 16: Tearth Kelvin updated,"]
["Issue 17: Update InnoV 18LFA 2019,Add Antennas-Amplifiers PA432-23-6A, Update InnoV 34 LFA B 2019,"]
["Issue 17: Update InnoV 40 LFA 2019,Add Innov 39 LFA 2019, Add InnoV 34 LFA A 2019,"]
["Issue 18: Add YU7EF EF7017XM-5, Antennas-Amplifiers PA432-26-7BGP,"]
["Issue 19: Add DG7YBN GTV70 21n,DG7YBN GTV70 13,"]
["Issue 20: Add YU7EF EF7011V6,"]
["Issue 21: Add WD5AGO 12B,"]
["Issue 22: Add Receive System NF Thanks to Vladimir UR5EAZ"]
["Issue 22: Charts for all 3 bands have been revised to be more readable.Thanks to Hartmut,DG7YBN"]
["Issue 23: Add EA1DDO 22 Quad,"]
["Issue 24: Add WD5AGO 13,"]
["Issue 24: Add Signal to Noise (S/N)"]
["Issue 25: Add DG7YBN GTV70-9w,DG7YBN GTV70-10w,"]
["Issue 26: Add Radiation Efficiency. Thanks to Vladimir UR5EAZ"]

{"sheet":"144.1 MHz Table","index":1,"n_rows":678,"n_cols":24,"rows_kept":678,"cut":false,"hidden":false,"merged":[[7,1,7,2],[7,5,7,6],[9,5,9,7]]}
[]
["Issue: July 2, 2024",null,null,null,null,"VE7BQH Antenna Table"]
[]
[null,"Old Reference: Tsky=200K Tearth=1000K",null,null,null,"Reference: Estimated Values for man-made noise (Tearth) on 144.1 MHz acc. ITU-R P.372-16: Part 6, Man-made noise, p.98-100"]
[null,"New Reference: Tsky=290K",null,null,null,"Rural =",null,1600]
[null,null,null,null,null,"Residential =",null,5400]
[null,null,null,null,null,"City =",null,14550]
[null,"Enter Tsky > ",null,290,"K","Enter Tearth > ",null,5400,"                 Enter Receive System NF >",null,null,null,0.75,"dB"]
[null,null,null,null,null,"                DL6WU Optimal Stacking",null,null,null,null,null,null,"1 Ant",null,null,null,null,null,null,null,"    Internal use only"]
[null,null,"   1 Ant",null,null,"4 Antennas",null,null,null,null,"<"," H Plane","          > ",null,null,null,null,"KF2YN",null,null,"  archive"]
["TYPE OF","Length","GAIN","E","H","GA","Tloss","TA","G/T","S/N","F/R","1st SL","2nd SL","Z","e","VSWR","Feed","Convergence","Polarity",null,"Ta",null,"    New"]
["ANTENNA","(m)","(dBi)","(m)","(m)","(dBi)","(K)","(K)","(dB/K)","(dB)","(dB)","(dB)","(dB)","(ohms)","(%)","Bandwidth","System","Correction req.",null,null,"      Old","Tpat","     \"S\""," avg gain"]
[]
["F5FOD Isotropic Lossless Radiator",0,0,"       -","        -","        -",{"$f":"290*(1/X14-1)","v":7.0001689696130853E-3},{"$f":"T14/1000*H$8+(1-T14/1000)*D$8+290*(1/X14-1)","v":2845.0036962099089},{"$f":"C14-10*LOG((T14/1000*H$8+(1-T14/1000)*D$8)+290*(10^(0.1*M$8)/X14-1))+10*LOG(1/X14)","v":-34.623381913806476},{"$f":"10*LOG(10^(C14/10)*5E-22/X14/1.380649E-23/2500/(T14/1000*H$8+(1-T14/1000)*D$8+290*(10^(M$8/10)/X14-1)))","v":-53.013914783949005},"     -","     -","-","      -",null,"-","         -","          No",null,499.99935343266912,599.99199999999996,599.9994827461353,{"$f":"(V14-200)*1.25","v":499.99935343266912},0.99997586206896549]
["+KF2YN Boxkite 4",0.89459349999999993,13.25,3.5,2,18.95,{"$f":"290*(1/X15-1)","v":3.9531632296399688},452.51319468717247,{"$f":"F15-10*LOG((T15/1000*H$8+(1-T15/1000)*D$8)+290*(10^(0.1*M$8)/X15-1))+10*LOG(1/X15)","v":-8.0491861185411917},{"$f":"10*LOG(10^(F15/10)*5E-22/X15/1.380649E-23/2500/(T15/1000*H$8+(1-T15/1000)*D$8+290*(10^(M$8/10)/X15-1)))","v":-26.439718988683715},23.4,22,"none",50.4,{"$f":"(1-((P15-1)/(P15+1))^2)*10^2","v":99.67960128159487},1.1200000000000001,"Dipole","Yes",null,31.029360363509291,225.70000000000002,224.82348829080743,31.029360363509291,0.98655172413793102]
["I0JXX 4JXX2",1.0840000000000001,9.23,2.1320000000000001,1.5649999999999999,15.22,1.6038210155857158,701.92404601558565,-13.546387114985745,-31.936919985128263,14.65,"none","none",196.8,{"$f":"(1-((P16-1)/(P16+1))^2)*10^2","v":99.572015023146136},1.1399999999999999,"Folded Dipole","Yes",null,80.297499999999999,250.67999999999998,264.238,80.297499999999999,0.99450000000000005]
["+Eantenna 144LFA4",1.2233045999999999,10.06,2.68,1.744,16.14,2.0341690395166312,613.99096291409114,-12.084164484763143,-30.474697354905661,17.739999999999998,"none","none",49.4,99.097070084560102,1.21,"LFA Loop","Yes",null,63.005243419681882,250.67999999999998,250.40419473574551,63.005243419681882,0.99303448275862072]
["+G4CQM WA26075",1.5644984,10.33,2.2909999999999999,1.77,16.329999999999998,1.9125303713988329,509.94333564734461,-11.161702616916212,-29.552235487058734,21.48,"none","none",49.65,99.572015023146136,1.1399999999999999,"Dipole","No",null,42.667476570635188,234.5,234.13398125650815,42.667476570635188,0.99344827586206896]
["+Eantenna 144LFA5",1.7995892499999999,11.09,2.4430000000000001,1.9850000000000001,17.09,3.2050343408987825,526.38229961998388,-10.50889876686548,-28.899431637008,18.89,18.3,"none",53.4,99.814564684874426,1.0900000000000001,"LFA Loop","Yes",null,45.631558763030355,237.08999999999997,236.50524701042428,45.631558763030355,0.98906896551724133]
["G4CQM 6",2.0804499999999999,11.61,2.6,2.17,17.59,8.1212336051045888,608.37123360510452,-10.515443504833037,-28.905976374975559,18.899999999999999,17.100000000000001,"none",56.7,90.368608799048758,1.9,"Dipole","No",null,60.714285714285694,249.7,248.57142857142856,60.714285714285694,0.97275862068965513]
["+KF2YN Boxkite 6",2.1636679999999999,14.62,3.9,3,20.399999999999999,4.7051196692013892,695.22825191856168,-8.2852348860197971,-26.675767756162323,26.5,22.9,24.8,49.9,99.173553719008268,1.2,"Dipole","Yes"," ",78.380260714160528,263.14,262.70420857132842,78.380260714160528,0.98403448275862071]
["Vine 6 OWL",2.2884950000000002,11.84,2.64,2.21,17.82,8.4386089425124062,534.12783889283162,-9.7667770349533107,-28.157309905095836,24.1,18.399999999999999,"none",48.3,99.318239205454091,1.18,"Folded Dipole","Yes",null,46.123136976579104,238.39999999999998,236.89850958126328,46.123136976579104,0.97172413793103452]
["InnoV 6 LFA-3 2022",2.2999999999999998,11.71,2.5779999999999998,2.1459999999999999,17.68,4.2503962408725009,504.12175659789165,-9.7354980906345485,-28.126030960777069,23.11,19.68,"none",50.16,99.51325040562466,1.1499999999999999,"LFA Loop","Yes",null,41.070716312528219,233.68199999999999,232.85657305002258,41.070716312528219,0.98555517241379309]
["*InnoV 6 LFA-3 2022",2.2999999999999998,11.71,2.2429999999999999,1.879,17.27,4.1608545705111499,385.81463625139048,-9.1151221974128891,-27.505655067555416,23.11,19.68,"none",50.16,99.51325040562466,1.1499999999999999,"LFA Loop","Yes",null,17.936160798606515,215.41900000000001,214.34892863888521,17.936160798606515,0.98585517241379306]
["G0KSC 6 LFA",2.3509084999999996,11.84,2.6,2.19,17.79,4.0970765141977878,524.6801082319206,-9.7842367812783912,-28.174769651420913,24.44,19.8,"none",49.5,99.978160110655438,1.03,"LFA Loop","Yes",null,45.123880962372382,236.85,236.09910476989791,45.123880962372382,0.98606896551724132]
["DG7YBN GTV 2-6m",2.3509084999999996,11.9,2.6509999999999998,2.194,17.88,3.542757417102933,522.51178010471187,-9.6853817133183711,-28.075914583460889,22.73,18.350000000000001,"none",49.83,97.994068780047527,1.33,"Bent Dipole","No",null,44.808027923211142,236.5,235.84642233856891,44.808027923211142,0.98793103448275865]
["+I5MZY 5",2.3925174999999999,12.36,2.915,2.5470000000000002,18.329999999999998,7.4885037141846151,856.63764591439713,-11.162629469584822,-29.553162339727344,16.489999999999998,12.13,"none",11.85,65.972222222222214,3.8,"Dipole","No",null,109.42253272019812,287.60000000000002,287.5380261761585,109.42253272019812,0.97482758620689658]
["+G4CQM WA27116",2.3987588500000001,11.7,2.5569999999999999,2.1120000000000001,17.649999999999999,2.3183872088981872,486.67422662495659,-9.6536234283998805,-28.044156298542408,24.36,20.2,"none",48.71,99.318239205454091,1.18,"Dipole","No",null,38.034410844629818,230.9,230.42752867570385,38.034410844629818,0.99206896551724133]
["DD0VF 6",2.4133219999999995,11.88,2.63,2.2200000000000002,17.86,5.6063268892794298,545.58321616871694,-9.847795698689005,-28.238328568831527,23.7,16.399999999999999,"none",27.2,99.885644939205122,1.07,"Dipole","No",null,48.919156414762739,240.1,239.13532513181019,48.919156414762739,0.98103448275862071]
["*DD0VF 6",2.4133219999999995,11.88,2.2999999999999998,2.2999999999999998,17.73,5.6063268892794298,578.13813708260113,-10.206780221069391,-28.597313091211912,23.7,16.399999999999999,"none",27.2,99.885644939205122,1.07,"Dipole","No",null,55.289982425307578,245.10000000000002,244.23198594024606,55.289982425307578,0.98103448275862071]
["EA1DDO 6 Quad V3",2.4655,12.41,2.8130000000000002,2.6560000000000001,18.369,17.822948731557158,784.15798623155717,-10.626036279855184,-29.016569149997707,19.86,13.42,"none",47.86,99.451303155006855,1.1599999999999999,"Dipole","Yes",null,93.216250000000002,244.97,274.57299999999998,93.216249999999974,0.94210000000000005]
["M2 2M7",2.662976,12.09,2.65,2.2599999999999998,17.91,3.7067821470978402,577.27617954180346,-10.046410562896153,-28.436943433038671,18.399999999999999,16.100000000000001,"none",204.9,99.572015023146136,1.1399999999999999,"T Match","Yes",null,55.493032758259417,244.97,244.39442620660753,55.493032758259417,0.98737931034482762]
["*M2 2M7",2.662976,12.09,2.21,2.0299999999999998,17.32,3.7067821470978402,544.73637982817627,-10.407082012967933,-28.797614883110455,18.399999999999999,16.100000000000001,"none",204.9,99.572015023146136,1.1399999999999999,"T Match","Yes",null,49.125165886708118,239.94,239.30013270936649,49.125165886708118,0.98737931034482762]
["+KF2YN Boxkite 7",2.746194,15.49,4.17,3.4,21.45,5.2949438202246757,580.73635007022472,-6.5087222951147821,-24.899255165257301,26.8,23.6,24.5,52.7,99.915166368177964,1.06,"Dipole","Yes",null,55.859375,245.5,244.6875,55.859375,0.98206896551724143]
["+DG7YBN YBN 2-7mz",2.758,12.24,2.718,2.331,18.213999999999999,3.314453322544757,564.74487832254476,-9.6608095399895753,-28.051342410132097,22.68,15.78,"none",27.2,99.017936855774693,1.22,"Dipole","Yes",null,53.1175,251.62,242.494,53.1175,0.98870000000000002]
["+YU7XL 8 Hybrid",2.7878030000000003,12.64,2.79,2.5,18.55,3.1845912497821249,620.215238800767,-9.6987011439273587,-28.089234014069881,19.8,17.100000000000001,"none",199.9,99.627498953029601,1.1299999999999999,"Horiz Dipole","Yes",null,63.998169775143801,251.62,251.19853582011504,63.998169775143801,0.98913793103448278]
["*YU7XL 8 Hybrid",2.7878030000000003,12.64,3,2.4300000000000002,18.579999999999998,3.4915372535334122,594.98688710521731,-9.4992331177034579,-27.889765987845976,19.8,17.100000000000001,"none",199.9,99.627498953029601,1.1299999999999999,"Horiz Dipole","Yes",null,59.001046937707216,247.70999999999998,247.20083755016577,59.001046937707216,0.98810344827586205]
["+G0KSC 7LFA",2.8918254999999995,12.75,2.84,2.4900000000000002,18.66,3.7580774738901512,606.1340249397465,-9.4894333184574116,-27.879966188599937,20.399999999999999,16.100000000000001,"none",48,99.67960128159487,1.1200000000000001,"LFA Loop","Yes",null,61.130322400363291,249.43,248.90425792029063,61.130322400363291,0.98720689655172411]
["+*G0KSC 7 LFA",2.8918254999999995,12.75,2.6,2.2000000000000002,18.34,3.7580774738901512,503.70957333473052,-9.0788495324859078,-27.46938240262843,20.399999999999999,16.100000000000001,"none",48,99.247305102062086,1.19,"LFA Loop","Yes",null,41.086398407209472,233.6,232.86911872576758,41.086398407209472,0.98720689655172411]
["+EAntenna 144LFA7",2.8918254999999995,12.73,2.8380000000000001,2.4889999999999999,18.649999999999999,4.3338116403597997,586.87608056556883,-9.3633542653396358,-27.753887135482156,22.54,15.2,"none",48.63,99.51325040562466,1.1499999999999999,"LFA Loop","Yes",null,57.248976306303128,246.45,245.7991810450425,57.248976306303128,0.98527586206896556]
["+DG7YBN GTV 2-7n",2.9958479999999996,12.74,2.88,2.4700000000000002,18.7,4.5709281961470882,562.55507880910693,-9.1425446016178231,-27.533077471760343,23.17,17.399999999999999,"none",47.2,98.936234390395953,1.23,"Bent Dipole","No",null,52.443082311733811,242.70000000000002,241.95446584938705,52.443082311733811,0.98448275862068968]
["Vine 7 FD",3.0166524999999997,12.71,2.83,2.46,18.62,8.4386089425124062,535.44251242015605,-8.9764371971627703,-27.366970067305296,22.8,17.899999999999999,"none",47.9,99.572015023146136,1.1399999999999999,"Folded Dipole","Yes",null,46.380411639460597,238.6,237.10432931156848,46.380411639460597,0.97172413793103452]
["+*InnoV 7 FD",3.0374569999999999,13,2.96,2.6059999999999999,18.96,3.8196555217832007,606.14057750759878,-9.1886422624978579,-27.579175132640373,22.4,14.8,"none",47.7,98.676482105098287,1.26,"Folded Dipole","Yes",null,61.119554204660602,249.43,248.89564336372848,61.119554204660602,0.98699999999999999]
["+InnoV 7 FD",3.0416178999999999,13,2.97,2.6240000000000001,18.97,3.8196555217832007,623.41983282674744,-9.290625002970863,-27.681157873113381,22.35,14.8,"none",47.69,98.676482105098287,1.26,"Folded Dipole","Yes",null,64.501013171225907,252.1,251.60081053698073,64.501013171225907,0.98699999999999999]
["+PY1MHZ 7",3.0416178999999999,12.86,2.8759999999999999,2.5179999999999998,18.78,3.0446326837103688,582.58286960733403,-9.2216401813591578,-27.612173051501671,22.2,15.1,"none",49.9,96.379222737628879,1.47,"Folded Dipole","Yes",null,56.661103116169009,245.79300000000001,245.32888249293521,56.661103116169009,0.98961034482758625]
["G4CQM 7",3.1206749999999999,12.91,2.89,2.5299999999999998,18.84,8.1212336051045888,544.02073732718907,-8.8231356379933175,-27.213668508135839,23.5,17.899999999999999,"none",50.7,84.336579622310865,2.31,"Dipole","No",null,48.121233605104585,239.9,238.49698688408367,48.121233605104585,0.97275862068965513]
["InnoV/G0KSC 7 LFA3 2020",3.15,12.45,2.71,1.88,17.920000000000002,3.8083642804490125,348.57188086262965,-8.0866727350187126,-26.477205605161235,30.2,20.9,"none",50.4,98.491843644198212,1.28,"LFA Loop","Yes",null,10.716930838000138,209.62899999999999,208.57354467040011,10.716930838000138,0.98703793103448279]
["+CT1FFU 7",3.2038929999999999,12.97,2.863,2.4980000000000002,18.850000000000001,2.8272980501392975,530.37913474930372,-8.7837099145352244,-27.174242784677745,20.3,18.399999999999999,20.399999999999999,28,99.990197039505929,1.02,"Dipole","No",null,46.487639275766028,237.70000000000002,237.19011142061282,46.487639275766028,0.9903448275862069]
["DK7ZB 7",3.2663064999999998,13.26,3.16,2.84,19.28,5.9183673469387816,757.38265306122457,-9.734041788585456,-28.12457465872798,16.899999999999999,11.9,16.899999999999999,28.4,94.123048668503216,1.64,"Dipole","No",null,90.306122448979593,272.60000000000002,272.24489795918402,90.30612244898002,0.98]
["+G4CQM WA9UXO",3.3620071999999999,12.96,2.8380000000000001,2.4609999999999999,18.829999999999998,2.0138888888888817,506.06167534722215,-8.6304013310489651,-27.020934201191487,22.01,19.7,22.1,48.07,99.51325040562466,1.1499999999999999,"Dipole","No",null,41.888020833333321,233.89999999999998,233.510416666667,41.888020833333748,0.99310344827586206]
["IK0BZY 6",3.3911334999999996,13.26,3.1,2.77,19.190000000000001,4.880785413744773,717.12320301542763,-9.6176743092029557,-28.008207179345483,17.8,11.9,17.7,19.5,84.916159320670729,2.27,null,null,null,82.630610098176689,266.5,266.10448807854135,82.630610098176689,0.98344827586206895]
["G4CQM 10 UZ2",3.4743514999999996,12.89,2.89,2.5099999999999998,18.829999999999998,5.8142806894125831,518.19723883221968,-8.6725964854902884,-27.06312935563281,25.3,19.5,25.3,45.1,98.676482105098287,1.26,"Dipole","No",null,43.519169890960292,235.9,234.81533591276823,43.519169890960292,0.98034482758620689]
["+DG7YBN YBN 2-8m",3.4951559999999997,13.09,2.91,2.56,18.989999999999998,3.542757417102933,537.38250436300177,-8.6857325585265066,-27.076265428669032,19.7,15.5,20.2,47.5,99.451303155006855,1.1599999999999999,"Dipole","No",null,47.718150087260049,238.8,238.17452006980804,47.718150087260049,0.98793103448275865]
["+PY1MHZ 8",3.4949479549999998,13.09,2.915,2.5670000000000002,19.03,3.0711838890999044,550.57250157686951,-8.7476638722529145,-27.138196742395436,20.7,16.7,21.3,50.03,98.936234390395953,1.23,"Folded Dipole","Yes",null,50.391647297019482,240.834,240.31331783761559,50.391647297019482,0.98952068965517237]
["I4GBZ 7",3.5159604999999998,13.56,3.18,2.86,19.41,5.8142806894125831,798.3665142455153,-9.8190190484980313,-28.209551918640553,12.7,13.9,19.7,48.4,84.916159320670729,2.27,"Dipole","No",null,98.346816742877223,278.89999999999998,278.67745339430178,98.346816742877223,0.98034482758620689]
["EA1DDO 8 Circular V2",3.6150000000000002,13.62,3.1160000000000001,2.9769999999999999,19.489999999999998,{"$f":"290*(1/X56-1)","v":3.3737986848760926},771.49733618487596,-9.6337659044173538,-28.024298774559874,18.29,13.47,18.2,53.79,93.562040543550907,1.68,"Dipole","No",null,93.566249999999997,214.33500000000001,274.85300000000001,93.566250000000011,0.98850000000000005]
["EA1DDO 8 Quad V3",3.6402000000000001,12.9,3.4590000000000001,3.339,18.96,25.388798259923892,1019.3615607599238,-11.004979255861651,-29.395512126004174,17.75,9.1999999999999993,16.600000000000001,50.64,98.936234390395953,1.23,"Dipole","Yes",null,137.76374999999999,214.33500000000001,310.21100000000001,137.76375000000002,0.91949999999999998]
["*InnoV/G0KSC 8 LFA3 2020",3.6428679499999994,13.08,2.89,2.13,18.649999999999999,5.0152594099695058,378.22170651068166,-7.6487584163070768,-26.0392912864496,25.63,18.5,25.63,50.6,99.097070084560102,1.21,"LFA Loop","Yes",null,16.283062054933879,214.33500000000001,213.0264496439471,16.283062054933879,0.98299999999999998]
["+DG7YBN GTV 2-8w",3.703201,13.36,2.98,2.63,19.25,3.6452513966480127,510.20469622905028,-8.2205176657622605,-26.611050535904784,22.78,16.239999999999998,22.78,49.06,99.72821814424654,1.1100000000000001,"Bent Dipole","No",null,42.379539106145252,234.6,233.9036312849162,42.379539106145252,0.98758620689655174]
["G0KSC 8LFA",3.7240055000000001,13.25,2.94,2.6,19.14,4.9842160645387672,487.16932655208694,-8.1321866203182367,-26.522719490460759,24.8,19.3,25.1,50,98.852040816326536,1.24,"LFA Loop","Yes",null,37.60961066292527,231.1,230.08768853034022,37.60961066292527,0.98310344827586205]
["*G0KSC 8LFA",3.7240055000000001,13.25,3.15,2.4,19.02,4.6741415557112553,475.51380080588615,-8.1619999777570378,-26.552532847899563,24.8,19.3,25.1,50,98.852040816326536,1.24,"LFA Loop","Yes",null,35.389365802382571,229.28999999999996,228.31149264190606,35.389365802382571,0.98413793103448277]
["+G4CQM WAX8",3.7240055000000001,13.08,2.8380000000000001,2.508,18.95,2.9292929292929482,481.32828282828279,-8.3024224273925533,-26.692955297535079,24.43,19.7,24.7,44.62,98.852040816326536,1.24,"Dipole","No",null,36.868686868686851,230.1,229.49494949494948,36.868686868686851,0.99]
["EAntenna 144LFA8",3.7281664000000001,13.23,2.9289999999999998,2.577,19.11,4.9635241301907662,488.47484392536478,-8.1728935337879509,-26.563426403930471,25.38,19.399999999999999,25,51.33,99.386268555288922,1.17,"LFA Loop","Yes",null,37.869142817059505,231.3,230.2953142536476,37.869142817059505,0.98317241379310349]
["W1JR 8 MOD",3.7448099999999998,13.29,3.07,2.75,19.14,5.3986652616789588,653.6102037232173,-9.2881545540750228,-27.678687424217543,17.3,12.8,17.3,50,99.572015023146136,1.1399999999999999,"Dipole","No",null,70.100105374077941,256.7,256.08008429926235,70.100105374077941,0.98172413793103452]
["DJ9BV 1.8",3.7448099999999998,13.49,3.16,2.8,19.43,5.6063268892794298,682.96498242530765,-9.1714498372118491,-27.561982707354371,17.600000000000001,13.4,17.5,77.5,97.888815837533784,1.34,"Dipole","No",null,75.80404217926187,261.2,260.6432337434095,75.80404217926187,0.98103448275862071]
["+PY1MHZ 8",3.74,13.28,2.67,2.629,19.296999999999997,4.6256222696332667,569.09010976963327,-8.5904872192973087,-26.981020089439834,29.31,18.38,26.86,50.33,94.810751181407554,1.59,"Folded Dipole","No",null,53.71125,257.7,242.96899999999999,53.711249999999993,0.98429999999999995]
["K1FO 10",3.8280280000000002,13.48,3.1,2.78,19.420000000000002,4.3647182359117975,659.81825341267051,-9.0600451020574138,-27.45057797219993,16.5,14.5,18.5,29.4,96.868702264221241,1.43,null,null,null,71.517325866293291,257.7,257.21386069303463,71.517325866293291,0.9851724137931035]
["Vine 8 OWL",3.8488324999999999,13.33,3,2.63,19.21,8.7566607460035701,493.94413854351677,-8.0664868809222448,-26.457019751064763,24.2,20.5,22.3,51.4,99.67960128159487,1.1200000000000001,"Folded Dipole","Yes",null,38.19715808170514,232.29999999999998,230.55772646536411,38.19715808170514,0.97068965517241379]
["YU7EF EF0208",3.8904415000000001,13.46,3.04,2.71,19.38,3.8504542278127318,558.83127183787576,-8.4459752042754221,-26.836508074417939,20,15.1,20.100000000000001,48.5,99.097070084560102,1.21,"Dipole","No",null,51.855345911949691,242.12,241.48427672955975,51.855345911949691,0.98689655172413793]
["BQH8B",3.9112459999999998,13.75,3.28,2.97,19.77,7.3833097595473802,671.16951025459684,-8.7375135806993693,-27.128046450841889,18,12.6,16.5,50,98.396292976869248,1.29,"Dipole","No",null,73.147984441301261,259.3,258.51838755304101,73.147984441301261,0.97517241379310349]
["+UR5EAZ 9",3.9320504999999994,13.47,3.07,2.75,19.41,3.6452513966480127,607.86832227653622,-8.7523335441627967,-27.142866414305313,18.5,13.7,17.8,49.2,99.997524813742231,1.01,"Dipole","No",null,61.4917946927374,249.7,249.19343575418992,61.4917946927374,0.98758620689655174]
["G4CQM 8",3.9736594999999997,13.67,3.15,2.83,19.600000000000001,5.1912951912952039,600.23982098982117,-8.4912151288228213,-26.881747998965345,19.5,13.9,18.5,49.47,99.72821814424654,1.1100000000000001,"Dipole","No",null,59.696384696384719,248.5,247.75710775710778,59.696384696384719,0.98241379310344823]
["G4CQM 9 UZ22",3.9736594999999997,13.62,3.09,2.76,19.54,4.880785413744773,545.00561009817682,-8.1733055648710451,-26.563838435013565,22.34,15.13,21.17,48.12,99.67960128159487,1.1200000000000001,"Dipole","No",null,48.948106591865361,240,239.15848527349229,48.948106591865361,0.98344827586206895]
["+G4CQM WA9C4X",3.9799008499999999,13.51,2.97,2.6619999999999999,19.399999999999999,3.1334959916347116,500.63262460787729,-8.0032058492438587,-26.393738719386381,24.73,19.100000000000001,21.1,50.2,98.936234390395953,1.23,"Dipole","No",null,40.606483095155106,233.1,232.48518647612408,40.606483095155106,0.98931034482758617]
["+KF2YN Boxkite9",3.9944639999999998,16.13,4.45,3.7,22.1,5.7102672292545442,470.67027074542915,-5.0285763468978981,-23.419109217040418,24.4,21.5,26.3,49.2,98.491843644198212,1.28,"Dipole","Yes",null,34.238748241912837,228.60000000000002,227.39099859353027,34.238748241912837,0.9806896551724138]
["+CT1FFU 8",4.036073,13.43,2.96,2.62,19.25,2.9292929292929482,495.52272727272725,-8.115822497094868,-26.50635536723739,23.6,21.2,21.6,27.1,99.940511600237954,1.05,"Dipole","No",null,39.646464646464636,232.29999999999998,231.71717171717171,39.646464646464636,0.99]
["+InnoV 8 OWL G/T",4.0498039700000001,13.98,3.2440000000000002,2.9359999999999999,19.93,3.542757417102933,552.89978184991276,-7.8579678299918463,-26.248500700134372,21.99,15.1,19.7,48.85,99.097070084560102,1.21,"Folded Dipole","Yes",null,50.754799301919711,241.2,240.60383944153577,50.754799301919711,0.98793103448275865]
["G0KSC 8 OWL",4.0568774999999997,13.78,3.13,2.82,19.7,4.6741415557112553,{"$f":"T78/1000*H$8+(1-T78/1000)*D$8+290*(1/X78-1)","v":517.11759810791864},-7.8095610370934914,-26.20009390723601,25.5,17.100000000000001,22.1,48.9,98.676482105098287,1.26,"Folded Dipole","Yes",null,43.531009110021017,235.7,234.82480728801681,43.531009110021017,0.98413793103448277]
["+*InnoV 8 OWL G/T",4.0568774999999997,13.98,3.2290000000000001,2.9239999999999999,19.96,3.8504542278127318,561.93798043326342,{"$f":"F79-10*LOG((T79/1000*H$8+(1-T79/1000)*D$8)+290*(10^(0.1*M$8)/X79-1))+10*LOG(1/X79)","v":-7.8878862411097765},{"$f":"10*LOG(10^(F79/10)*5E-22/X79/1.380649E-23/2500/(T79/1000*H$8+(1-T79/1000)*D$8+290*(10^(M$8/10)/X79-1)))","v":-26.278419111252298},22,15.1,19.7,48.9,99.097070084560102,1.21,"Folded Dipole","Yes",null,52.46331236897273,242.6,241.97064989517818,52.46331236897273,0.98689655172413793]
["RA3RF 9",4.0693601999999993,13.96,3.2109999999999999,2.9020000000000001,19.89,{"$f":"290*(1/X80-1)","v":4.880785413744773},548.25311185133239,-7.8467253634779244,-26.237258233620445,20.57,15.92,18.899999999999999,48.88,{"$f":"(1-((P80-1)/(P80+1))^2)*10^2","v":99.885644939205122},1.07,"Dipole","No",null,49.58362552594668,240.5,239.66690042075734,49.58362552594668,0.98344827586206895]
["InnoV 9 LFA-4 2022",4.165,13.81,3.1160000000000001,2.8010000000000002,19.7,5.8840106532316554,478.8987973775038,-7.4936523585471075,-25.884185228689628,26.79,17.329999999999998,24.82,47.89,98.936234390395953,1.23,"LFA Loop","Yes",null,35.815026756217634,229.87200000000001,228.65202140497411,35.815026756217634,0.98011379310344826]
["*InnoV 9 LFA-4 2022",4.165,13.81,2.742,2.4649999999999999,19.3,5.8236454900085066,401.49798929617913,-7.2152966006621693,-25.605829470804689,26.79,17.329999999999998,24.82,47.89,98.936234390395953,1.23,"LFA Loop","Yes",null,20.679910725277999,217.99,216.5439285802224,20.679910725277999,0.98031379310344824]
["I0JXX 8JXX2",4.2441180000000003,14.26,3.46,3.17,20.25,8.3856661344687193,654.14346726982467,-8.1411677665885467,-26.53170063673107,19.5,13.2,17.5,203.77,93.420488937411037,1.69,"T Match","Yes",null,69.619921944296664,256.66000000000003,255.69593755543733,69.619921944296664,0.97189655172413791]
["#I0JXX 8x8JXX2 XPOL H",4.2441180000000003,14.18,3.32,3.32,20.22,7.5200764141932197,639.2344916333534,-8.0906499889707995,-26.481182859113321,18.98,13.6,16.399999999999999,49.6,81.632653061224488,2.5,"HairPin","Yes","XPOL",66.871705522340534,254.42000000000002,253.49736441787243,66.871705522340534,0.97472413793103452]
["#I0JXX 8x8JXX2 XPOL V",4.2441180000000003,14.18,3.32,3.32,20.22,7.5200764141932197,586.21962005165005,-7.7462154785438377,-26.136748348686361,18.98,13.6,16.399999999999999,49.69,81.77272764591423,2.4900000000000002,"HairPin","Yes","XPOL",56.496975271517975,246.32999999999998,245.19758021721438,56.496975271517975,0.97472413793103452]
["Antennas-Amplifiers +PA144-9-4.3AP",4.3002901500000004,13.82,3.2,2.5,19.55,5.6250307576577896,422.55504390435942,-7.1633994202299487,-25.553932290372469,26.3,16.89,23.37,53.11,99.852071005917168,1.08,"HairPin","No",null,24.839532905421073,221.20599999999999,219.87162632433686,24.839532905421073,0.9809724137931034]
["Ant-Amp +PA144-XPOL-18-5AP Horiz",4.3002901500000004,13.82,3.2,2.5,19.63,5.6447762977962039,429.58415945131702,-7.1465048090771788,-25.537037679219701,26.3,16.89,23.37,53.11,99.852071005917168,1.08,"HairPin","No","XPOL",26.211229579945368,222.28700000000001,220.96898366395629,26.211229579945368,0.98090689655172414]
["Ant-Amp +PA144-XPOL-18-5AP Vert",4.3002901500000004,13.82,3.2,2.5,19.579999999999998,5.5990538018396618,394.05753021894003,-6.8669375657353431,-25.257470435877867,26.3,16.89,23.37,53.11,99.852071005917168,1.08,"HairPin","No","XPOL",19.267803604129234,216.827,215.41424288330339,19.267803604129234,0.98105862068965521]
["*InnoV/G0KSC 9 LFA3 2020",4.3044510499999999,13.96,3.1789999999999998,2.5569999999999999,19.68,4.9945631204181318,448.15520274299371,-7.2680967936881045,-25.658629663830624,25.6,16.3,24.4,47.646000000000001,99.940511600237954,1.05,"LFA Loop","Yes",null,29.972727910484451,225.096,223.97818232838756,29.972727910484451,0.98306896551724132]
["*DG0OPK 9",4.3065314999999993,13.6,2.95,2.7,19.45,5.8142806894125831,484.96785965529392,-7.7935893376366998,-26.184122207779225,24.6,16.399999999999999,23.4,28.4,99.72821814424654,1.1100000000000001,"Dipole","No",null,37.016355962012,230.8,229.6130847696096,{"$f":"(V90-200)*1.25","v":37.016355962012},0.98034482758620689]
["DG0OPK 9",4.3065314999999993,13.6,3.04,2.72,19.489999999999998,5.8142806894125831,492.13498065423863,-7.8107749214465692,-26.201307791589095,24.6,16.399999999999999,23.4,28.4,99.72821814424654,1.1100000000000001,"Dipole","No",null,38.418923672177314,231.9,230.73513893774185,38.418923672177314,0.98034482758620689]
["+DG7YBN GTV 2-9n",4.3190141999999998,13.99,3.2109999999999999,2.8889999999999998,19.899999999999999,4.6741415557112553,517.76664330763845,-7.6144804483093651,-26.005013318451891,25.35,17.100000000000001,22.1,51.67,95.347943098808159,1.55,"Bent Dipole","No",null,43.658023826208847,235.8,234.92641906096708,43.658023826208847,0.98413793103448277]
["+7arrays GTV 2-9n XPOL H",4.3273359999999998,13.97,3.05,3.05,19.89,4.6741415557112553,545.67558689558496,-7.8309106524227339,-26.221443522565252,25.2,17.2,22.6,51.6,95.21484375,1.56,"Bent Dipole","No","XPOL",49.119656622284502,240.1,239.2957252978276,49.119656622284502,0.98413793103448277]
["+7arrays GTV 2-9n XPOL V",4.3273359999999998,14,3.05,3.05,19.89,4.6741415557112553,545.67558689558496,-7.8309106524227339,-26.221443522565252,24.82,17,21.6,53.22,95.61155462513085,1.53,"Bent Dipole","No","XPOL",49.119656622284502,240.1,239.2957252978276,49.119656622284502,0.98413793103448277]
["*InnoV/G0KSC 9 LFA3 2020",4.3398186999999995,13.96,3.1789999999999998,2.8769999999999998,19.88,4.9893895017450358,490.97526219330399,-7.4224646675622648,-25.812997537704785,25.7,16.100000000000001,24.3,49.6,99.940511600237954,1.05,"LFA Loop","Yes",null,38.353399743945005,231.68600000000001,230.682719795156,38.353399743945005,0.98308620689655168]
["DK7ZB 8",4.3481404999999995,14.16,3.4,3.1,20.170000000000002,4.880785413744773,633.3376577840113,-8.1392242340235388,-26.529757104166059,21.6,13,17.600000000000001,28,98.676482105098287,1.26,"Dipole","No",null,66.23422159887798,253.60000000000002,252.98737727910239,66.23422159887798,0.98344827586206895]
["G0KSC 9 OWA",4.3481404999999995,14.14,3.33,3.04,20.11,4.9842160645387672,590.47610487548241,-7.9188638156667643,-26.309396685809286,21.3,15,17.100000000000001,49.1,98.298676748582224,1.3,"Dipole","No",null,57.826201332865672,247,246.26096106629254,57.826201332865672,0.98310344827586205]
["YU7XL TWB21810XL",4.3689450000000001,15.54,3.3479999999999999,4.2690000000000001,21.47,3.6247468752182321,437.32231076740459,-5.4016254411873064,-23.792158311329832,24.66,17.3,20.2,203.8,99.852071005917168,1.08,"Dipole","Yes",null,28.12085399064312,223.33,222.4966831925145,28.12085399064312,0.98765517241379308]
["*YU7XL TWB21810XL",4.3689450000000001,15.54,3.9,4.4000000000000004,21.58,3.6247468752182321,434.15331506179763,-5.2636002058249396,-23.654133075967462,24.66,17.3,20.2,203.8,99.852071005917168,1.08,"Dipole","Yes",null,27.500698275260156,222.84000000000003,222.00055862020812,27.500698275260156,0.98765517241379308]
["+PY1MHZ 9",4.3879999999999999,13.91,3.1629999999999998,2.85,19.824999999999999,4.326601035217708,495.10488853521775,-7.5189373250819234,-25.90947019522444,24.48,16.68,22.32,49.94,95.21484375,1.56,"Folded Dipole","Yes",null,39.291249999999998,246.5,231.43299999999999,39.291249999999991,0.98529999999999995]
["+RA3AQ 9S",4.4105540000000003,14.19,3.35,3.06,20.170000000000002,4.7774272695408264,587.21880476691206,-7.8396951162018871,-26.23022798634441,20.7,14.5,17.399999999999999,47.1,99.852071005917168,1.08,"Dipole","No",null,57.229232386961115,246.5,245.78338590956889,57.229232386961115,0.98379310344827586]
["M2 9SSB",4.4105540000000003,14.16,3.33,3.04,20.12,7.5306021368428233,578.55258083917101,-7.7939226654822562,-26.184455535624775,20.2,14.7,17.100000000000001,200.6,98.676482105098287,1.26,"T Match","Yes",null,54.994516380103349,245.16000000000003,243.99561310408268,54.994516380103349,0.97468965517241379]
["Cushcraft LFA-2M9EL ",4.4105540000000003,13.89,3.1309999999999998,2.8250000000000002,19.77,5.2949438202246757,476.99554511938197,-7.4159150090329815,-25.806447879175508,25.6,16.899999999999999,24.6,47.4,99.852071005917168,1.08,"LFA Loop","Yes",null,35.557847612359552,229.55,228.44627808988764,35.557847612359552,0.98206896551724143]
["InnoV 9LFA XPOL H",4.4105540000000003,13.98,2.9,2.9,19.82,4.9842160645387672,493.66660820764633,-7.5038651410946002,-25.894398011237122,25.04,16.7,22.6,50.9,99.961553248750477,1.04,"LFA Loop","Yes","XPOL",38.881094352858625,232.1,231.1048754822869,38.881094352858625,0.98310344827586205]
["InnoV 9LFA XPOL V",4.4105540000000003,13.98,2.9,2.9,19.82,4.9842160645387672,439.34933356716959,-7.0516450998377103,-25.442177969980232,25.1,16.7,22.7,50.09,99.940511600237954,1.05,"LFA Loop","Yes","XPOL",28.251490705015811,223.74,222.60119256401265,28.251490705015811,0.98310344827586205]
["#WiMo WX220 XPOL H",4.4313585,13.36,2.94,2.94,19.29,1.973337036522711,840.0312152826001,-10.199112425009741,-28.589645295152263,14.43,13.4,17.600000000000001,190.63,99.915166368177964,1.06,"Folded Dipole","Yes","XPOL",107.25203096792121,285.83000000000004,285.80162477433697,107.25203096792121,0.99324137931034484]
["#WiMo WX220 XPOL V",4.4313585,13.33,2.94,2.94,19.27,1.7505030181086312,850.68888329979859,-10.273633210589159,-28.664166080731679,13.99,13.5,17.5,170.28399999999999,99.451303155006855,1.1599999999999999,"Folded Dipole","Yes","XPOL",109.38128772635814,287.52,287.50503018108651,109.38128772635814,0.99399999999999999]
["*WiMo WX220 XPOL H",4.4313585,13.36,3.4,3.4,19.57,2.0138888888888817,908.05277777777746,-10.236649917190533,-28.627182787333055,14.43,13.4,17.600000000000001,190.63,99.915166368177964,1.06,"Folded Dipole","Yes","XPOL",120.5555555555555,296.39999999999998,296.4444444444444,120.5555555555555,0.99310344827586206]
["*WiMo WX220 XPOL V",4.4313585,13.33,3.4,3.4,19.55,1.7505030181086312,911.35085513078457,-10.275192511003288,-28.665725381145812,13.99,13.5,17.5,170.28399999999999,99.451303155006855,1.1599999999999999,"Folded Dipole","Yes","XPOL",121.25251509054323,296.95999999999998,297.00201207243458,121.25251509054323,0.99399999999999999]
["Gulf Alpha 9",4.4313585,13.77,3.26,2.97,19.79,4.7154471544715708,715.03112296747963,-9.008160107145109,-27.398692977287631,18.91,14.9,12.8,203.35,99.51325040562466,1.1499999999999999,"T Match","Yes",null,82.253556910569117,266.19,265.80284552845529,82.253556910569117,0.98399999999999999]
["Gulf Alpha 9XPOL H",4.4313585,13.74,3.12,3.12,19.78,5.0359586037537323,732.59931590948975,-9.1116733028801704,-27.502206173022692,18.89,14.9,12.8,203.19,99.51325040562466,1.1499999999999999,"T Match","Yes","XPOL",85.628837046132276,268.87,268.50306963690582,85.628837046132276,0.98293103448275865]
["Gulf Alpha 9XPOL V",4.4313585,13.75,3.12,3.12,19.79,4.7154471544715708,661.34756097560967,-8.6945493839938521,-27.085082254136378,18.899999999999999,14.9,12.8,203.15899999999999,99.51325040562466,1.1499999999999999,"T Match","Yes","XPOL",71.74796747967477,257.91999999999996,257.39837398373982,71.74796747967477,0.98399999999999999]
["DJ9BV 2.1",4.4313585,14.04,3.33,3.04,20.02,5.9183673469387816,643.97193877551013,-8.3417097518731875,-26.732242622015711,20.2,13.2,17.399999999999999,44.9,98.298676748582224,1.3,"Dipole","No",null,68.112244897959187,255.20000000000002,254.48979591836735,68.112244897959187,0.98]
["EAntenna 144LFA9",4.4469618750000004,14.09,3.2269999999999999,2.9289999999999998,19.98,4.385326239148684,519.24911614393727,-7.5495432524987276,-25.940076122641248,22.19,16,20.100000000000001,51.26,99.451303155006855,1.1599999999999999,"LFA Loop","Yes",null,44.004655558667061,236.02,235.20372444693365,44.004655558667061,0.98510344827586205]
["*G0KSC 9LFA",4.4492000000000003,14.1,3.1,3,19.989999999999998,5.5959368739235789,516.61138448560678,-7.5034747310746948,-25.894007601217218,23.5,16.2,20.9,50.5,99.852071005917168,1.08,"LFA Loop","Yes",null,43.251555305613145,235.65,234.60124424449052,43.251555305613145,0.98106896551724143]
["G0KSC 9LFA",4.4521629999999996,14.1,3.26,2.94,20.02,5.5959368739235789,513.42111437207802,-7.4491987345981254,-25.839731604740646,23.5,16.2,20.9,50.5,99.852071005917168,1.08,"LFA Loop","Yes",null,42.627236301008686,235.15999999999997,234.10178904080695,42.627236301008686,0.98106896551724143]
["YU7EF EF0209V",4.4800000000000004,13.95,3.1629999999999998,2.8380000000000001,19.84,5.8944209300444106,470.92472635923224,-7.2882576308184612,-25.678790500960979,23.42,18.96,22.03,48.1,98.936234390395953,1.23,"Bent Dipole","Yes",null,34.252505954831278,228.649,227.40200476386502,34.252505954831278,0.98007931034482754]
["*YU7EF EF0209V",4.4800000000000004,13.95,3.05,2.85,19.809999999999999,5.8642331452373186,470.56388169652286,-7.3156773931910299,-25.706210263333553,23.42,18.96,22.03,48.1,98.936234390395953,1.23,"Bent Dipole","Yes",null,34.187798150936501,228.59200000000001,227.3502385207492,34.187798150936501,0.98017931034482764]
["*DG7YBN GTV2-9M",4.492,13.983000000000001,3.1629999999999998,2.851,19.855999999999998,4.3564758424685568,482.84521334246853,-7.3897465165678637,-25.780279386710383,26.18,17.43,20.76,48.1,98.852040816326536,1.24,"Bent Dipole","Yes",null,36.886249999999997,228.59200000000001,229.50899999999999,36.886249999999983,0.98519999999999996]
["*OZ5HF 9",4.4937719999999999,13.67,2.7,2.5,18.8,2.9292929292929482,771.66919191919214,-10.330813672351422,-28.72134654249394,18.2,11.9,16,38,99.51325040562466,1.1499999999999999,null,null,null,93.686868686868721,275.10000000000002,274.94949494949498,93.686868686868721,0.99]
["OZ5HF 9",4.4937719999999999,13.67,3.21,2.92,19.62,3.0313588850173967,755.60209059233466,-9.4241861092244061,-27.814718979366933,18.2,11.9,16,38,99.51325040562466,1.1499999999999999,null,null,null,90.522648083623736,272.60000000000002,272.41811846689899,90.522648083623736,0.98965517241379308]
["YU7EF EF0209",4.4937719999999999,13.99,3.2,2.89,19.89,5.3986652616789588,522.83135756937122,-7.6530384099421029,-26.043571280084628,22,16.7,19.8,49.8,99.386268555288922,1.17,"Dipole","No",null,44.507376185458369,236.60000000000002,235.6059009483667,44.507376185458369,0.98172413793103452]
["F9FT 11",4.5145764999999995,13.93,3.26,2.97,19.899999999999999,5.3986652616789588,616.52366526167873,-8.2949248159365379,-26.685457686079062,22.7,13.4,18.899999999999999,21.5,98.76543209876543,1.25,null,null,null,62.842465753424612,251,250.27397260273969,62.842465753424612,0.98172413793103452]
["*CC 13B2",4.5145764999999995,13.94,2.9,2.79,19.62,5.9183673469387816,604.2130102040818,-8.4876624837782391,-26.878195353920763,19.600000000000001,13.2,19,21.1,97.562712528262921,1.37,null,null,null,60.331632653061256,249.10000000000002,248.265306122449,60.331632653061256,0.98]
["CC 13B2",4.5145764999999995,13.94,3.33,3.01,19.93,6.0225272791270719,661.60066877859902,-8.5383556134800926,-26.928888483622618,19.600000000000001,13.2,19,21.1,97.562712528262921,1.37,null,null,null,71.541710665258691,257.89999999999998,257.23336853220695,71.541710665258691,0.97965517241379307]
["K1FO 11",4.5353810000000001,14.1,3.3,3,20.05,4.3647182359117975,596.92697759887983,-8.0303643477824114,-26.420897217924932,17.899999999999999,14.6,19.2,44,98.396292976869248,1.29,null,null,null,59.20983549177457,248,247.36786839341966,59.20983549177457,0.9851724137931035]
["CC 215WB",4.5561854999999998,13.93,3.36,3.07,19.93,6.7537050105857288,718.68031051517278,-8.8609001842859758,-27.251433054428496,19.100000000000001,12.7,17.7,17.399999999999999,96.379222737628879,1.47,null,null,null,82.568807339449535,266.60000000000002,266.05504587155963,82.568807339449535,0.97724137931034483]
["Vine 9 FD",4.6185990000000006,14.08,3.21,2.91,19.95,9.7148966500356515,478.50115823235927,-7.1904189534510392,-25.580951823593558,23.9,18.7,21.5,50,99.885644939205122,1.07,"Folded Dipole","Yes",null,34.987526728439065,230,227.99002138275125,34.987526728439065,0.96758620689655173]
["+G0KSC 9 OWL",4.7434259999999995,14.3,3.28,2.97,20.149999999999999,6.5444287729195949,476.25480430183359,-7.0134563271025847,-25.40398919724511,24.3,18.8,22.3,49,99.173553719008268,1.2,"Folded Dipole","Yes",null,35.168370944992944,229.5,228.13469675599436,35.168370944992944,0.97793103448275864]
["+KF2YN Boxkite 10",4.7642305,16.440000000000001,4.49,3.89,22.4,5.7102672292545442,453.08443213783391,-4.5810129538906441,-22.971545824033164,29.2,21.2,27,49,99.572015023146136,1.1399999999999999,"Dipole","Yes",null,30.797292545710242,225.89999999999998,224.63783403656819,30.797292545710242,0.9806896551724138]
["G4CQM CQM12UX",4.826643999999999,14.09,3.2,2.89,19.97,4.0559440559440478,490.68374125874112,-7.342512989804157,-25.733045859946682,23.3,15.8,20.9,50.2,99.915166368177964,1.06,"Dipole","No",null,38.479020979020966,231.6,230.78321678321677,38.479020979020966,0.98620689655172411]
["*Flexa 224",4.8682529999999993,13.68,3.5,3.3,19.79,31.544637736570415,667.73224048939039,-8.3849334548520069,-26.775466324994529,17.7,12.7,16.899999999999999,234.5,99.814564684874426,1.0900000000000001,"Folded Dipole","Yes",null,67.747084687440307,257.71000000000004,254.19766774995225,67.747084687440307,0.90189655172413796]
["Flexa 224",4.8682529999999993,13.68,3.3,3,19.62,30.833174379124866,634.45496509365569,-8.3606149814201505,-26.751147851562674,17.7,12.7,16.899999999999999,234.5,99.814564684874426,1.0900000000000001,"Folded Dipole","Yes",null,61.37412734139545,253.02999999999997,249.09930187311636,61.37412734139545,0.90389655172413796]
["+RA3AQ 9",4.8890574999999998,14.53,3.4,3.13,20.46,5.7102672292545442,507.79593002812942,-6.9645478051491576,-25.355080675291678,22.1,15.1,18.8,49.2,99.773242630385482,1.1000000000000001,"Folded Dipole","Yes",null,41.504043600562603,234.3,233.20323488045008,41.504043600562603,0.9806896551724138]
["+G4CQM WAXXX10",4.9009160649999997,14.28,3.1949999999999998,2.903,20.14,2.6235212247738349,454.35573242867071,-6.8924652241223674,-25.282998094264887,24.42,18.2,21.5,45.26,98.76543209876543,1.25,"Dipole","No",null,31.650139178844796,225.89999999999998,225.32011134307584,31.650139178844796,0.99103448275862072]
["+*InnoV 9 OWL G/T",4.9306665000000001,14.74,3.58,3.35,20.74,4.1587967820916827,551.55784365162663,-7.030101659727829,-25.420634529870352,20.89,14.8,19.899999999999999,48.67,97.888815837533784,1.34,"Folded Dipole","Yes",null,50.371633438265135,241,240.29730675061211,50.371633438265135,0.9858620689655172]
["+InnoV 9 OWL G/T",4.9306665000000001,14.74,3.54,3.26,20.7,4.1587967820916827,543.13501224204276,-7.0094169733323914,-25.399949843474914,20.9,14.8,19.899999999999999,48.7,97.888815837533784,1.34,"Folded Dipole","Yes",null,48.723329835606854,239.7,238.97866386848548,48.723329835606854,0.9858620689655172]
["+WiMo WY209",4.9514709999999997,14.39,3.5,3.24,20.440000000000001,2.6337033299697166,689.93491422805221,-8.2428648042686632,-26.633397674411185,19.149999999999999,11.5,14.9,209.7,99.814564684874426,1.0900000000000001,"Folded Dipole","Yes",null,77.749747729566039,262.45,262.19979818365283,77.749747729566039,0.99099999999999999]
["+*WiMo WY209",4.9514709999999997,14.39,3.56,3.22,20.45,2.6337033299697166,691.86856710393522,-8.2441208817344034,-26.634653751876925,19.2,11.5,14.9,209.7,99.814564684874426,1.0900000000000001,"Folded Dipole","Yes",null,78.128153380423768,262.75,262.50252270433901,78.128153380423768,0.99099999999999999]
["+CT1FFU 9",4.9514709999999997,14.38,3.26,2.97,20.23,3.6452513966480127,459.75593575419003,-6.8347391738154366,-25.225272043957958,22.7,20.2,21.2,28.1,99.51325040562466,1.1499999999999999,"Dipole","No",null,32.506983240223484,226.8,226.00558659217879,32.506983240223484,0.98758620689655174]
["ZL1RS 9",4.9514709999999997,14.39,3.3,3.01,20.28,5.7102672292545442,461.55168776371306,-6.7726881013644391,-25.163220971506959,25.2,18.7,23.4,48.7,86.377613470131067,2.17,"Dipole","No",null,32.454289732770754,227.2,225.9634317862166,32.454289732770754,0.9806896551724138]
["Eagle 10",4.9514709999999997,14.43,3.44,3.16,20.420000000000002,6.1267605633802731,{"$f":"T142/1000*H$8+(1-T142/1000)*D$8+290*(1/X142-1)","v":564.44674295774666},-7.4149922610481038,-25.805525131190624,22,15,19.2,23.6,97.994068780047527,1.33,null,null,null,52.508802816901436,243,242.00704225352115,52.508802816901436,0.97931034482758617]
["G4CQM CQM12UC",4.9722755000000003,14.3,3.3,3.01,20.2,5.2949438202246757,516.34550561797744,{"$f":"F143-10*LOG((T143/1000*H$8+(1-T143/1000)*D$8)+290*(10^(0.1*M$8)/X143-1))+10*LOG(1/X143)","v":-7.2954504672515901},{"$f":"10*LOG(10^(F143/10)*5E-22/X143/1.380649E-23/2500/(T143/1000*H$8+(1-T143/1000)*D$8+290*(10^(M$8/10)/X143-1)))","v":-25.685983337394113},21.4,14.5,19.8,49.4,99.978160110655438,1.03,"Dipole","No",null,43.258426966292127,235.6,234.6067415730337,43.258426966292127,0.98206896551724143]
["DK7ZB 9",4.9722755000000003,14.56,3.56,3.3,20.6,{"$f":"290*(1/X144-1)","v":6.3354474982381603},613.39222163495424,-7.5620414462372869,-25.95257431637981,20.399999999999999,12.2,16,27.5,{"$f":"(1-((P144-1)/(P144+1))^2)*10^2","v":98.936234390395953},1.23,"Dipole","No",null,62.046335447498251,250.5,249.6370683579986,62.046335447498251,0.97862068965517246]
["DG7YBN GTV 2-10LT",5.0554934999999999,14.42,3.33,3.0409999999999999,20.309999999999999,8.7566607460035701,463.67442273534635,-6.7207599332192194,-25.111292803361742,26.26,17.5,23.9,48.9,97.888815837533784,1.34,"Dipole","No",null,32.273534635879209,227.7,225.81882770870337,32.273534635879209,0.97068965517241379]
["+PY1MHZ 10",5.0783784499999998,14.46,3.44,3.1469999999999998,20.420000000000002,6.8877968877968643,511.74413438779686,-7.0193077640568058,-25.409840634199323,23.35,16.66,20.34,50.14,92.993079584775089,1.72,"Folded Dipole","Yes",null,42.046250000000001,218.29499999999999,233.637,42.046250000000001,0.9768]
["*InnoV/G0KSC 9 OWL 2020",5.0783784499999998,14.33,3.28,2.7,20.04,6.5099265600265044,403.08769254635382,-6.4815297091965123,-24.87206257933903,25.8,19,23.8,50.6,99.67960128159487,1.1200000000000001,"Folded Dipole","Yes",null,20.856705672471101,218.29499999999999,216.68536453797688,20.856705672471101,0.97804482758620692]
["*InnoV/G0KSC 9 OWL 2020",5.0783784499999998,14.33,3.28,2.65,20,6.5099265600265044,397.51031526655925,-6.4684324280691721,-24.858965298211693,25.8,19,23.8,50.6,99.67960128159487,1.1200000000000001,"Folded Dipole","Yes",null,19.765242408323438,217.441,215.81219392665875,19.765242408323438,0.97804482758620692]
["Vine 10 OWL ",5.0971025000000001,14.42,3.35,3.04,20.32,9.8217468805704282,456.67415329768255,-6.6381408562932833,-25.028673726435802,25,18,22.6,47.6,99.852071005917168,1.08,"Folded Dipole","Yes",null,30.695187165775373,226.7,224.5561497326203,30.695187165775373,0.96724137931034482]
["DD0VF 9",5.1179069999999998,14.62,3.48,3.18,20.59,4.4677871148459225,517.80663515406161,-6.9275310755678596,-25.318063945710378,20.3,15.8,17.5,25,99.451303155006855,1.1599999999999999,"Dipole","No",null,43.706232492997188,235.8,234.96498599439775,43.706232492997188,0.98482758620689659]
["*InnoV/G0KSC 10 LFA3 2020",5.1719987000000005,14.57,3.3660000000000001,3.0859999999999999,20.47,4.9893895017450358,454.49888326698124,-6.5325121755466089,-24.923045045689133,25.7,15.9,22.2,49.01,99.885644939205122,1.07,"LFA Loop","Yes",null,31.215165120398467,226.072,224.97213209631877,31.215165120398467,0.98308620689655168]
["+YU7EF EF0210LT",5.1803205000000005,13.99,3.1309999999999998,2.8130000000000002,19.84,5.3986652616789588,441.50122936424304,-7.0450708128566797,-25.435603682999201,29.4,22.8,25.3,45.7,99.627498953029601,1.1299999999999999,"Dipole","No",null,28.591499824376534,224.10000000000002,222.87319985950123,28.591499824376534,0.98172413793103452]
["K5GW 10",5.1803205000000005,14.58,3.42,3.13,20.5,6.6385665408627155,505.49456368382039,-6.8945176148978859,-25.285050485040408,21.33,16,20.6,202.6,96.379222737628879,1.47,"T Match","Yes",null,40.872015096469205,233.98,232.69761207717536,40.872015096469205,0.97762068965517246]
["+PY1MHZ 11",5.1898905700000002,14.7,3.4780000000000002,3.1949999999999998,20.64,3.542757417102933,504.64751439790558,-6.7889990312194222,-25.179531901361941,21.7,16.5,17.7,49.5,98.76543209876543,1.25,"Folded Dipole",null,null,41.31208551483418,233.73699999999999,233.04966841186734,41.31208551483418,0.98793103448275865]
["+I5MZY 9",5.19904455,14.94,3.7509999999999999,3.4980000000000002,21.04,6.0246112257038265,601.38725765404899,-7.0476017085144234,-25.438134578656943,17.25,13.88,15.78,186.3,70.701119434391032,3.36,"Bent Dipole","No",null,59.757856443903172,248.66499999999999,247.80628515512254,59.757856443903172,0.97964827586206893]
["G4CQM 9",5.2427339999999996,14.78,3.62,3.35,20.83,7.4885037141846151,573.57220551821706,-7.0502663969182819,-25.440799267060797,22.2,13.1,17.600000000000001,46.4,88.592605587474239,2.02,"Dipole","No",null,54.028121683763679,244.4,243.22249734701094,54.028121683763679,0.97482758620689658]
["+G0KSC 10 LFA",5.2635384999999992,14.76,3.48,3.18,20.69,2.6235212247738349,479.49234516353516,-6.5516039274552638,-24.942136797597783,24.3,16,22.8,48.5,99.940511600237954,1.05,"LFA Loop",null,null,36.569241475295762,229.8,229.25539318023661,36.569241475295762,0.99103448275862072]
["+*G0KSC 10 LFA",5.2635384999999992,14.76,3.4,3.1,20.63,2.5217391304347681,469.8609565217389,-6.5340077252191717,-24.924540595361698,24.3,16,22.8,48.5,99.940511600237954,1.05,"LFA Loop",null,null,34.704347826086916,228.29999999999998,227.76347826086953,34.704347826086916,0.99137931034482762]
["K1FO 12",5.2635384999999992,14.63,3.46,3.18,20.57,4.3647182359117975,549.59642982149091,-7.183285109226345,-25.573817979368872,21.6,14.7,19.600000000000001,203.26,98.852040816326536,1.24,"T Match","Yes",null,49.947497374868703,240.7,239.95799789989496,49.947497374868703,0.9851724137931035]
["Directive DSEFO144-12",5.2635384999999992,14.63,3.46,3.18,20.57,4.3647182359117975,549.59642982149091,-7.183285109226345,-25.573817979368872,21.6,14.7,19.600000000000001,203.26,98.852040816326536,1.24,"T Match","Yes",null,49.947497374868703,240.7,239.95799789989496,{"$f":"(V160-200)*1.25","v":49.947497374868703},0.9851724137931035]
["Directive DSEFO144XPOL-12H",5.2635384999999992,14.63,3.32,3.32,20.57,3.8504542278127318,557.66625611460506,-7.247729981294559,-25.638262851437084,21.6,14.7,19.600000000000001,203.3,98.852040816326536,1.24,"T Match","Yes","XPOL",51.627358490566024,241.94,241.30188679245282,51.627358490566024,0.98689655172413793]
["Directive DSEFO144XPOL-12V",5.2635384999999992,14.63,3.32,3.32,20.57,4.2102501311876956,512.0243353157249,-6.9069353124758219,-25.297468182618346,21.6,14.7,19.600000000000001,203.3,98.852040816326536,1.24,"T Match","Yes",null,42.625065593842919,234.9,234.10005247507434,42.625065593842919,0.9856896551724138]
["*YU7EF EF0210",5.388365499999999,14.59,3.38,3.09,20.48,7.0681737901801505,462.9942599788061,-6.56702762913587,-24.957560499278394,23.8,17.2,23.1,50.3,99.915166368177964,1.06,"Dipole","No",null,32.470858353938539,227.5,225.97668668315083,32.470858353938539,0.9762068965517241]
["YU7EF EF0210",5.388365499999999,14.59,3.39,3.1,20.49,7.0681737901801505,464.95721476510062,-6.57342271532311,-24.963955585465634,23.8,17.2,23.1,50.3,99.915166368177964,1.06,"Dipole","No",null,32.854998233839616,227.79999999999998,226.28399858707169,32.854998233839616,0.9762068965517241]
["Gulf Alpha 11",5.4091699999999996,14.48,3.46,3.19,20.47,5.3467954345917512,602.59507901668132,-7.6346887936466752,-26.0252216637892,17.59,13.5,16.899999999999999,187.92099999999999,99.852071005917168,1.08,"T Match","Yes",null,60.126865671641809,248.86,248.10149253731345,60.126865671641809,0.98189655172413792]
["Gulf Alpha 11 XPOL H",5.4091699999999996,14.48,3.32,3.32,20.46,5.3467954345917512,614.69487708516249,-7.7237927288707597,-26.114325599013281,17.55,13.5,16.899999999999999,187.8,99.885644939205122,1.07,"T Match","Yes","XPOL",62.494732221246707,250.72,249.99578577699737,62.494732221246707,0.98189655172413792]
["Gulf Alpha 11 XPOL V",5.4091699999999996,14.48,3.32,3.32,20.45,5.3467954345917512,567.46663301141393,-7.416514775906756,-25.807047646049277,17.53,13.5,16.899999999999999,187.673,99.885644939205122,1.07,"T Match","Yes","XPOL",53.25241439859532,243.46000000000004,242.60193151887626,53.25241439859532,0.98189655172413792]
["+G0KSC 10LFA+2",5.4091699999999996,14.6,3.39,3.09,20.5,4.1587967820916827,458.90669814620509,-6.5508020969139897,-24.941334967056513,23.8,18.899999999999999,22.6,47.4,98.852040816326536,1.24,"LFA Loop","Yes",null,32.240293809024152,226.7,225.79223504721932,32.240293809024152,0.9858620689655172]
["+YU7XL 17 twin Bm",5.4507789999999998,15.85,3.75,4.21,21.78,2.6235212247738349,542.39832985386238,-5.9446920551653575,-24.335224925307884,24.06,16.3,22.2,191.71799999999999,99.885644939205122,1.07,"Horiz Dipole","Yes",null,48.879610299234528,239.56,239.10368823938762,48.879610299234528,0.99103448275862072]
["+G0KSC 10 OWL",5.4715834999999995,14.61,3.4,3.1,20.51,7.3833097595473802,443.88021570014155,-6.369972360199454,-24.760505230341977,26.4,19.100000000000001,26.2,48.2,99.72821814424654,1.1100000000000001,"Folded Dipole","Yes",null,28.668670438472432,224.6,222.93493635077795,28.668670438472432,0.97517241379310349]
["I0JXX 12JXX2",5.5756060000000005,14.82,3.58,3.3,20.79,7.0681737901801505,531.69767749911682,-6.7969437716473085,-25.187476641789836,25.2,17,26.9,26.9,98.199059238020283,1.31,"T Match",null,null,45.915754150476857,238,236.73260332038149,45.915754150476857,0.9762068965517241]
["Antenna-Amplifiers +PA144-10-6AGP",5.6796284999999997,15.08,3.5,2.9,20.56,7.836172397917629,396.0019380599922,-5.8769801955641903,-24.267513065706705,29.06,17.75,26.21,49.9,99.318239205454091,1.18,"HairPin","No",null,19.210521655983293,217.33199999999999,215.36841732478663,19.210521655983293,0.97368965517241379]
["BQH 12J",5.8252599999999992,14.95,3.67,3.4,20.98,4.3647182359117975,585.25643157157856,-7.0219735764643563,-25.412506446606876,20.3,13.5,17.2,50,99.997524813742231,1.01,"Dipole","No",null,56.92597129856491,246.20000000000002,245.54077703885193,56.92597129856491,0.9851724137931035]
["+*InnoV 10 OWL G/T",5.8252599999999992,15.25,3.6859999999999999,3.4319999999999999,21.2,4.3647182359117975,482.16660833041652,-6.0401594224732538,-24.430692292615774,23.6,15.1,21.1,48,98.676482105098287,1.26,"Folded Dipole","Yes",null,36.751837591879593,230.3,229.40147007350367,36.751837591879593,0.9851724137931035]
["+InnoV 10 OWL G/T",5.8294208999999997,15.25,3.706,3.44,21.21,4.3647182359117975,484.1116993349666,-6.0458426751053782,-24.436375545247898,23.61,15.1,21.1,48,98.676482105098287,1.26,"Folded Dipole","Yes",null,37.132481624081173,230.6,229.70598529926494,37.132481624081173,0.9851724137931035]
["+CT1FFU 10",5.8668689999999994,14.89,3.44,3.15,20.74,4.1587967820916827,416.79254109828616,-5.9398088606871466,-24.330341730829666,25.3,20,23.3,27.97,99.247305102062086,1.19,"Dipole","No",null,23.998775795732783,220.2,219.19902063658623,23.998775795732783,0.9858620689655172]
["+CT1FFU 10C",5.8668689999999994,15.19,3.62,3.31,21.08,4.2617214835549362,434.23692267319831,-5.7559957420038614,-24.146528612146383,27.2,17.600000000000001,21.9,27.2,98.936234390395953,1.23,"Dipole","No",null,27.392407277816702,222.9,221.91392582225336,27.392407277816702,0.98551724137931029]
["M2 12",5.9084779999999997,14.84,3.48,3.2,20.7,4.4368588733676573,491.80687427791213,-6.6163831496155314,-25.006916019758055,19.899999999999999,15.1,18.3,195.86,99.627498953029601,1.1299999999999999,"T Match","Yes",null,38.624269159402047,231.79000000000002,230.89941532752164,38.624269159402047,0.98493103448275865]
["+KF2YN Boxkite12",5.9084779999999997,17.05,6,4.4000000000000004,22.99,6.0225272791270719,462.73605244632171,-4.0685295156280636,-22.459062385770583,25.2,20,27,48.5,99.017936855774693,1.22,"Dipole","Yes",null,32.624956001407952,227.4,226.09996480112636,32.624956001407952,0.97965517241379307]
["+7arrays GTV2-11LT",5.9292825000000002,15.06,3.5369999999999999,3.2610000000000001,20.95,4.7774272695408264,428.7962670872767,-5.8307425782287998,-24.221275448371323,28.91,16.670000000000002,23.44,47.37,98.676482105098287,1.26,"Bent Dipole","No",null,26.226778829302511,222.1,220.98142306344201,26.226778829302511,0.98379310344827586]
["*4Y3i 12",5.9450000000000003,14.93,3.5779999999999998,3.33,20.94,{"$f":"290*(1/X181-1)","v":2.8701272470208217},522.22608974702086,-6.6322434226388909,-25.022776292781405,20.5,13.84,16.38,50.79,99.386268555288922,1.17,"Dipole","No",null,44.883749999999999,232.5,235.90700000000001,44.883750000000013,0.99019999999999997]
["BQH 10",5.9500869999999999,15.2,3.69,3.43,20.94,7.1615944256583948,495.67231942565837,-6.3709880978845561,-24.761520968027074,23.9,14.4,20.6,22.6,96.379222737628879,1.47,"Dipole","No",null,38.847499999999997,232.5,231.078,38.847500000000004,0.97589999999999999]
["+PY1MHZ 11",5.96,15.06,3.5979999999999999,3.33,20.97,6.2811606048222401,451.45908560482218,-5.9896630886350417,-24.380195958777566,25.3,17.7,21.1,49.2,96.987910661840033,1.42,"Folded Dipole","Yes",null,30.3675,223.88,224.29400000000001,30.367500000000014,0.9788]
["WB9UWA 12",5.9708914999999996,14.88,3.48,3.2,20.76,6.9318221939766111,439.37016294177863,-6.0864682233411695,-24.477001093483686,24.2,19.600000000000001,22,200.1,96.503404058430831,1.46,"T Match","Yes",null,27.874430674716635,223.88,222.29954453977331,27.874430674716635,0.97665517241379307]
["DK7ZB 10",5.9708914999999996,15.32,3.89,3.64,21.35,5.1912951912952039,607.39184801684814,-6.7883160307217256,-25.178848900864246,20.5,12.66,16.579999999999998,26.44,94.810751181407554,1.59,"Dipole","No",null,61.095998595998608,249.6,248.87679887679889,61.095998595998608,0.98241379310344823]
["IZ7NLJ 11",5.9708914999999996,15.05,3.5569999999999999,3.2949999999999999,20.98,3.6473020062989248,437.641604078939,-5.8941429901669968,-24.28467586030952,22.29,16.47,19.37,45.46,99.097070084560102,1.21,"Dipole","Yes",null,28.178924084665375,223.381,222.5431392677323,28.178924084665375,0.9875793103448276]
["Vine 11 FD",5.9708914999999996,14.93,3.6,3.21,20.82,10.35714285714282,412.13839285714283,-5.7370722824505807,-24.127605152593109,27.9,19.7,24,48.4,99.814564684874426,1.0900000000000001,"Folded Dipole","Yes",null,21.875,220,217.5,21.875,0.96551724137931039]
["+YU7EF EF0211B",5.9708914999999996,15.07,3.58,3.3,21,4.7774272695408264,451.52081142656863,-5.979862617928446,-24.370395488070965,25.6,16.7,20.100000000000001,50.2,97.781801720235393,1.35,"Dipole","No",null,30.673852085524018,225.6,224.53908166841921,30.673852085524018,0.98379310344827586]
["+I5MZY 13 Rev2",5.9916959999999992,15.43,3.89,3.65,21.46,5.7071479555419451,562.01255480779025,-6.3635174910950338,-24.754050361237553,19.8,15.4,17.8,205.1,78.089633318243557,2.76,"Folded Dipole","Yes",null,52.114561027837247,242.624,241.6916488222698,52.114561027837247,0.98070000000000002]
["I5MZY 13",5.9916959999999992,15.36,3.82,3.56,21.36,8.0155917788802356,532.2163802267894,-6.2182649640371945,-24.608797834179718,22.8,15.1,17.8,57.2,82.335643772316729,2.4500000000000002,"Dipole","No",null,45.831856839121166,238.1,236.66548547129693,45.831856839121166,0.97310344827586204]
["+YU7XL 11 Hybrid",5.9916959999999992,15.25,3.64,3.42,21.19,4.6225258363986699,443.4739884393062,-5.7224216059156863,-24.112954476058206,26.2,17.3,20.7,195.6,99.318239205454091,1.18,"Horiz Dipole","Yes",null,29.129444736381132,224.35,223.30355578910491,29.129444736381132,0.98431034482758617]
["+*YU7XL 11 Hybrid",5.9916959999999992,15.25,3.77,3.56,21.23,4.9221489689999025,458.41087898022164,-5.8065741184956519,-24.197106988638172,26.2,17.3,20.7,195.6,99.318239205454091,1.18,"Horiz Dipole","Yes",null,31.99388062841912,226.67,225.5951045027353,31.99388062841912,0.98331034482758617]
["+InnoV 10 OWL G/T-2 2020",5.9958568999999997,15.37,3.706,3.4489999999999998,21.29,5.0152594099695058,442.58405391658187,-5.6095295860227719,-24.000062456165296,24.55,17.399999999999999,21.7,46.66,79.564646275098511,2.65,"Folded Dipole","Yes",null,28.878433367243126,224.24,223.1027466937945,28.878433367243126,0.98299999999999998]
["+*InnoV 10 OWL G/T-2 2020",5.9958568999999997,15.37,3.706,3.431,21.29,4.4162436548223161,430.44081218274118,-5.5101792348077954,-23.900712104950316,24.55,17.399999999999999,21.7,46.66,79.564646275098511,2.65,"Folded Dipole","Yes",null,26.619289340101524,222.32599999999999,221.29543147208122,26.619289340101524,0.98499999999999999]
["K1FO 13",6.0125004999999998,15.07,3.64,3.39,21.03,4.6741415557112553,539.83418009810782,-6.6485087797733158,-25.039041649915838,19.7,14.5,19.399999999999999,24.7,97.45074500388391,1.38,"T Match",null,null,47.976524176594246,239.2,238.3812193412754,47.976524176594246,0.98413793103448277]
["YU7XL TWB22205",6.0333049999999995,16.36,4.2,5.5,22.41,6.1726464663539566,343.72393038005885,-3.5142759333363562,-21.904808803478879,26.06,20.2,22.4,198.2,99.990197039505929,1.02,"Dbl Quad","Yes",null,9.3055350124667058,209.16499999999999,207.44442800997336,9.3055350124667058,0.9791586206896552]
["BQH 13X (1995)",6.0499485999999996,15.17,3.73,3.48,21.18,6.6281038374718211,533.59101650677212,-6.4267398712293557,-24.81727274137188,23.68,14.4,18.899999999999999,205,97.994068780047527,1.33,"T Match","Yes",null,46.372389954853297,238.28,237.09791196388264,46.372389954853297,0.97765517241379307]
["*InnoV/G0KSC 11 LFA3 2020",6.0849001599999992,15.19,3.62,3.3479999999999999,21.1,5.9006674477599912,430.01890720822473,-5.6770674050860173,-24.067600275228536,27.47,15.3,22.5,50.8,99.940511600237954,1.05,"LFA Loop","Yes",null,26.246230872889385,222.37299999999999,220.99698469831151,26.246230872889385,0.98005862068965521]
["+DK7ZB 11 OWL",6.0957185000000003,15.23,3.68,3.42,21.16,6.439901304194537,486.0835830102219,-6.0843110799985833,-24.4748439501411,24.34,15.23,21.57,12.47,99.814564684874426,1.0900000000000001,"Dipole","No",null,37.112266478674627,231,229.6898131829397,37.112266478674627,0.97827586206896555]
["+EAntenna 144LFA11",6.1373275000000005,15.26,3.6840000000000002,3.4209999999999998,21.2,5.5855475889216759,455.93532528468995,-5.806910564841508,-24.197443434984027,25.57,17,22.8,48.55,99.451303155006855,1.1599999999999999,"LFA Loop","Yes",null,31.379604245747217,226.32999999999998,225.10368339659777,31.379604245747217,0.98110344827586204]
["#M2 20 XPOL H ",6.1789364999999998,15.25,3.64,3.64,21.21,7.1206500618265363,550.66863186716148,-6.5142235984795764,-24.9047564686221,21.46,13.49,16.04,193.9,98.936234390395953,1.23,"T Match","Yes","XPOL",49.618000353294498,240.9,239.6944002826356,49.618000353294498,0.9760344827586207]
["#M2 20 XPOL V",6.1789364999999998,15.25,3.64,3.64,21.21,7.1206500618265363,521.2845521992582,-6.2986104395693001,-24.689143309711817,21.35,13.49,16.25,193.9,98.936234390395953,1.23,"T Match","Yes","XPOL",43.867691220632423,236.41000000000003,235.09415297650594,43.867691220632423,0.9760344827586207]
["+G0KSC 11 LFA",6.1997409999999995,15.26,3.61,3.35,21.09,3.5120231738386543,427.03134924789714,-5.6914250548227141,-24.081957924965231,27.7,16.5,24.6,48.3,99.915166368177964,1.06,"LFA Loop","Yes",null,26.129026628974259,221.73,220.90322130317941,26.129026628974259,0.98803448275862071]
["+*G0KSC 11 LFA",6.1997409999999995,15.26,3.78,3.65,21.29,3.0313588850173967,447.73349303135882,-5.6802646171516775,-24.070797487294197,27.7,16.5,24.6,48.3,99.915166368177964,1.06,"LFA Loop","Yes",null,30.274390243902438,224.9,224.21951219512195,30.274390243902438,0.98965517241379308]
["+UA9TC 11RS",6.1997409999999995,15.24,3.66,3.37,21.16,5.0877192982456299,434.4921052631579,-5.6674644933434193,-24.057997363485942,23.3,17.899999999999999,21.5,50.9,99.773242630385482,1.1000000000000001,"Dipole","No",null,27.280701754385959,223,221.82456140350877,27.280701754385959,0.98275862068965514]
["+G0KSC 11 OWL",6.2413499999999997,15.31,3.69,3.44,21.24,7.9100247963159802,{"$f":"T206/1000*H$8+(1-T206/1000)*D$8+290*(1/X206-1)","v":443.64820226709185},-5.6311339460044998,-24.021666816147025,23,16.399999999999999,22.3,49.8,96.987910661840033,1.42,"Folded Dipole","Yes",null,28.520191285866119,224.6,222.8161530286929,28.520191285866119,0.97344827586206895]
["*BVO-3WL",6.2621544999999994,15.58,3.9,3.7,21.53,8.8628287135750021,630.83577647476909,{"$f":"F207-10*LOG((T207/1000*H$8+(1-T207/1000)*D$8)+290*(10^(0.1*M$8)/X207-1))+10*LOG(1/X207)","v":-6.7099160427482563},{"$f":"10*LOG(10^(F207/10)*5E-22/X207/1.380649E-23/2500/(T207/1000*H$8+(1-T207/1000)*D$8+290*(10^(M$8/10)/X207-1)))","v":-25.100448912890784},20.5,12.9,17.7,52.7,74.009996155324885,3.08,"Dipole","No",null,64.965351812366734,253.1,251.97228144989339,64.965351812366734,0.97034482758620688]
["BVO-3WL",6.2621544999999994,15.58,4.03,3.78,21.57,8.8628287135750021,650.58391080312754,-6.7929649896395343,-25.183497859782058,20.5,12.9,17.7,52.7,{"$f":"(1-((P208-1)/(P208+1))^2)*10^2","v":74.009996155324885},3.08,"Dipole","No",null,68.82995735607679,256.10000000000002,255.06396588486143,68.82995735607679,0.97034482758620688]
["#BVO-3WL",6.2621544999999994,15.56,3.9,3.9,21.56,{"$f":"290*(1/X209-1)","v":8.8628287135750021},653.87526652452038,-6.8231384160333786,-25.213671286175906,20.5,12.9,17.7,52.7,74.009996155324885,3.08,"Dipole","No",null,69.474058280028459,256.60000000000002,255.57924662402277,69.474058280028459,0.97034482758620688]
["+G0KSC 11LFA3R",6.2621544999999994,15.15,3.6,3.33,21.07,4.0559440559440478,434.98295454545456,-5.7753014654349579,-24.165834335577479,25.7,18.2,24,50.1,99.852071005917168,1.08,"LFA Loop",null,null,27.578671328671334,223,222.06293706293707,27.578671328671334,0.98620689655172411]
["YU7EF EF0211AV",6.3,15.08,3.5379999999999998,3.2610000000000001,20.95,6.7788380102761181,396.65655745370111,-5.5067964571298926,-23.89732932727242,29.04,19.079999999999998,22.43,50.57,99.961553248750477,1.04,"Bent Dipole","Yes",null,19.54554196544521,217.33500000000001,215.63643357235617,19.54554196544521,0.9771586206896552]
["*YU7EF EF0211AV",6.3,15.08,3.45,3.25,20.92,6.7495165911560839,395.02051576547956,-5.5214451707478807,-23.911978040890403,29.04,19.079999999999998,22.43,50.57,99.961553248750477,1.04,"Bent Dipole","Yes",null,19.231115298302051,217.08199999999999,215.38489223864164,19.231115298302051,0.97725517241379312]
["+YU7EF EF0211",6.3245680000000002,15.22,3.56,3.3,21.02,4.7774272695408264,432.04263056431836,-5.7897533727991854,-24.180286242941705,22.2,17.8,22.5,49,94.400093234659991,1.62,"Dipole","No",null,26.862075008762716,222.6,221.48966000701017,26.862075008762716,0.98379310344827586]
["F9FT 16",6.3661769999999995,14.79,3.54,3.26,20.78,6.1267605633802731,553.35858274647876,-6.9766536326628081,-25.367186502805325,21.1,13.8,16.399999999999999,20.8,97.562712528262921,1.37,"HairPin",null,null,50.338908450704203,241.29999999999998,240.27112676056336,50.338908450704203,0.97931034482758617]
["#SM2CEW 14 XPOL H",6.4077859999999998,15.15,3.5,3.5,21.07,9.9286733238231157,471.16561162624828,-6.0076943844473485,-24.39822725458987,24.7,15.8,22.6,18.13,96.253902185223723,1.48,"Dipole","No","XPOL",33.510164051355211,228.9,226.80813124108417,33.510164051355211,0.96689655172413791]
["#SM2CEW 14 XPOL V",6.4077859999999998,15.15,3.5,3.5,21.07,9.9286733238231157,426.24353601997143,-5.6212996457600299,-24.011832515902547,24.71,15.8,22.7,18.2,96.253902185223723,1.48,"Dipole","No","XPOL",24.719151212553498,222.1,219.7753209700428,24.719151212553498,0.96689655172413791]
["CD15LQDver2",6.4285904999999994,15.05,3.58,3.33,21,4.4677871148459225,490.56582633053199,-6.3061143403021873,-24.696647210444709,26.1,14,17,50,98.76543209876543,1.25,"Gamma Match",null,null,38.375350140055993,231.6,230.70028011204479,38.375350140055993,0.98482758620689659]
["*CD15LQDver2",6.4285904999999994,15.05,4,3.8,21.17,4.4677871148459225,537.26435574229686,-6.4924802531056223,-24.883013123248144,26.1,14,17,50,98.76543209876543,1.25,"Gamma Match",null,null,47.514005602240879,238.8,238.0112044817927,47.514005602240879,0.98482758620689659]
["CD15LQDver1",6.449395,14.98,3.6,3.35,20.91,4.1587967820916827,595.61573102483408,-7.1644071968098961,-25.554940066952415,20.7,14.5,17.5,50,98.936234390395953,1.23,"Gamma Match",null,null,58.993529206016113,247.8,247.19482336481289,58.993529206016113,0.9858620689655172]
["*CD15LQDver1",6.449395,14.98,4,3.8,21.12,4.2617214835549362,609.23386109167291,-7.0429176810826242,-25.433450551225146,20.7,14.5,17.5,50,98.936234390395953,1.23,"Gamma Match",null,null,61.638383484954566,249.9,249.31070678796365,61.638383484954566,0.98551724137931029]
["I5MZY  13",6.449395,15.12,3.56,3.3,20.98,6.1267605633802731,452.91289612676036,-5.9941063632513494,-24.384639233393873,20.3,15.1,17.8,49.3,96,1.5,"Dipole","No",null,30.682218309859124,225.89999999999998,224.5457746478873,30.682218309859124,0.97931034482758617]
["MBI ModFT17",6.4910040000000002,15.44,3.85,3.6,21.42,8.4386089425124062,541.35854329311564,-6.219643975434594,-24.610176845577115,24.3,12.9,19.7,50.1,97.105766085294675,1.41,"Dipole","No",null,47.53814762242726,239.5,238.03051809794181,47.53814762242726,0.97172413793103452]
["*F9FT 17",6.5326129999999996,15.02,3.68,3.5,21.05,5.8871336593604067,516.87984642718925,-6.4416514875068263,-24.832184357649354,22.6,14.7,18.600000000000001,50.6,98.097502972651611,1.32,"HairPin","Yes",null,43.247106216796247,235.7,234.597684973437,43.247106216796247,0.98010344827586204]
["F9FT 17",6.5326129999999996,15.02,3.59,3.31,20.96,5.8871336593604067,503.45447788762613,-6.4286227089922345,-24.819155579134758,22.6,14.7,18.600000000000001,50.6,98.097502972651611,1.32,"HairPin","Yes",null,40.619832529993296,233.64,232.49586602399464,40.619832529993296,0.98010344827586204]
["*CC3219",6.5950264999999995,14.92,4.2699999999999996,3.66,20.95,5.8142806894125831,986.66632958142804,-9.1442492179630861,-27.534782088105612,14.9,15.1,18,18.3,96.127481814809428,1.49,"T Match",null,null,135.19609567358424,307.79999999999995,308.15687653886738,135.19609567358424,0.98034482758620689]
["CC3219",6.5950264999999995,14.92,4.07,3.82,20.94,5.8142806894125831,991.87878121702431,-9.1759111278055379,-27.566443997948053,14.9,15.1,18,18.3,96.127481814809428,1.49,"T Match",null,null,136.21614491734084,308.60000000000002,308.97291593387268,136.21614491734084,0.98034482758620689]
["CC3219 MOD",6.5950264999999995,15.41,3.87,3.62,21.42,5.1912951912952039,581.38447700947711,-6.544534460357097,-24.935067330499617,24.1,13,16,28.6,99.940511600237954,1.05,"Dipole","Yes",null,56.00649350649352,245.6,244.80519480519482,56.00649350649352,0.98241379310344823]
["BQH 13",6.6366354999999997,15.45,3.85,3.6,21.43,4.3647182359117975,576.82770388519407,-6.5144648856972989,-24.904997755839823,20.8,13.7,17.5,50,99.72821814424654,1.1100000000000001,"Dipole","No",null,55.276513825691254,244.9,244.221211060553,55.276513825691254,0.9851724137931035]
["InnoV 11 OWL G/T",6.6574400000000002,15.77,4.0190000000000001,3.7730000000000001,21.76,4.7361042966285849,555.99143565570887,-6.0339652144519871,-24.424498084594504,22.15,13.6,18.5,49.5,99.451303155006855,1.1599999999999999,"LFA-FD","Yes",null,51.126287937197716,241.69,240.90103034975817,51.126287937197716,0.98393103448275865]
["DJ9BV 3.2",6.6990490000000005,15.45,3.85,3.58,21.44,6.6490299823632988,541.55952380952385,-6.2247736676433929,-24.615306537785916,21.1,13.7,18.100000000000001,71.8,97.67308244757254,1.36,"Dipole","No",null,47.927689594356266,239.5,238.34215167548501,{"$f":"(V230-200)*1.25","v":47.927689594356266},0.97758620689655173]
["+DG7YBN GTV 2-12w Mk1",6.7198534999999993,15.6,3.87,3.62,21.56,5.6063268892794298,473.96239015817218,-5.5970181709460727,-23.987551041088597,26.2,15,20.100000000000001,46.2,97.222222222222214,1.4,"Bent Dipole","No",null,34.903339191564129,229.1,227.9226713532513,34.903339191564129,0.98103448275862071]
["*+DG7YBN GTV 2-12w Mk1",6.7198534999999993,15.6,3.99,3.83,21.62,5.7102672292545442,486.30212728551339,-5.6356627292052028,-24.026195599347723,26.2,15,20.100000000000001,46.2,97.222222222222214,1.4,"Bent Dipole","No",null,37.297819971870609,231,229.83825597749649,37.297819971870609,0.9806896551724138]
["K1FO 14",6.7822669999999992,15.49,3.8,3.56,21.44,4.7774272695408264,530.73208026638633,-6.1702239528329441,-24.560756822975467,18.100000000000001,14.4,19.3,29.6,96.987910661840033,1.42,"T Match","Yes",null,46.175078864353338,237.8,236.94006309148267,46.175078864353338,0.98379310344827586]
["+DG7YBN GTV 2-12w Mk2",6.7822669999999992,15.53,3.77,3.54,21.46,5.9183673469387816,433.44515306122446,-5.3473598211275695,-23.73789269127009,28,17.2,21.6,46.2,98.491843644198212,1.28,"Bent Dipole","No",null,26.91326530612244,222.9,221.53061224489795,26.91326530612244,0.98]
["*+DG7YBN GTV 2-12w Mk2",6.7822669999999992,15.53,3.99,3.82,21.56,5.9183673469387816,450.39158163265301,-5.3952492512588757,-23.785782121401404,28,17.2,21.6,46.2,98.491843644198212,1.28,"Bent Dipole","No",null,30.229591836734677,225.5,224.18367346938774,30.229591836734677,0.98]
["+KF2YN Boxkite 13",6.7822669999999992,17.260000000000002,4.83,4.32,23.15,6.0225272791270719,454.9118708201338,-3.8424995863042493,-22.233032456446772,28.8,20.399999999999999,28.9,52.5,99.885644939205122,1.07,"Dipole","Yes",null,31.09380499824006,226.2,224.87504399859205,31.09380499824006,0.97965517241379307]
["UR5EAZ 12",6.8030714999999997,15.46,3.71,3.44,21.36,3.8196555217832007,437.55458459979724,-5.5111142850401782,-23.901647155182701,24.01,15.3,18.3,50.15,99.961553248750477,1.04,"Dipole","No",null,28.12816616008103,223.38,222.50253292806482,28.12816616008103,0.98699999999999999]
["*WB9UWA 13",6.85,14.93,3.31,2.68,20.100000000000001,{"$f":"290*(1/X238-1)","v":7.4969224456299033},336.26265994562976,-5.7257976033532829,-24.1163304734958,27.97,19.91,26.76,24,94.400093234659991,1.62,"Dipole","No",null,7.5862499999999855,223.38,206.06899999999999,7.5862499999999855,0.9748]
["+*DG7YBN GTV 2-12n",6.8654849999999996,15.68,4.2,3.74,21.71,5.0877192982456299,437.74188596491234,-5.1461658826592176,-23.536698752801737,25.69,16.52,21.11,48.11,96.127481814809428,1.49,"Bent Dipole","No",null,27.916666666666679,223.5,222.33333333333334,27.916666666666679,0.98275862068965514]
["+DG7YBN GTV 2-12n",6.8654849999999996,15.68,3.82,3.56,21.6,5.0877192982456299,417.5932456140352,-5.075080609202252,-23.465613479344775,25.69,16.52,21.11,48.11,96.127481814809428,1.49,"Bent Dipole","No",null,23.973684210526329,220.4,219.17894736842106,23.973684210526329,0.98275862068965514]
["+*Dual PA144-12-7",6.8654849999999996,15.7,4,3.75,21.71,6.2623736217282939,423.3620803536831,-5.0024573867001685,-23.39299025684269,25.87,16.600000000000001,22.5,49.34,99.318239205454091,1.18,"Hair Pin","Yes",null,24.872741043435376,221.38,219.8981928347483,24.872741043435376,0.9788620689655172]
["+Dual PA144-12-7",6.8654849999999996,15.7,3.82,3.5880000000000001,21.62,6.5444287729195949,411.526185648801,-4.9802060294168093,-23.370738899559335,25.87,16.600000000000001,22.5,49.34,99.318239205454091,1.18,"Hair Pin","Yes",null,22.501322284908305,219.59,218.00105782792664,22.501322284908305,0.97793103448275864]
["+DK7ZB 12",6.8862895000000002,15.6,3.7509999999999999,3.4980000000000002,21.5,4.880785413744773,408.61053646563801,-5.0945312416615405,-23.485064111804061,23.04,18.38,21.2,47.76,99.097070084560102,1.21,"Bent Dipole","No",null,22.256311360448784,219,217.80504908835903,22.256311360448784,0.98344827586206895]
["+InnoV 11 G/T-2",6.8862895000000002,15.9,3.94,3.7,21.83,5.907955385102575,439.64187572569568,-5.032159299951684,-23.422692170094205,24.76,17.100000000000001,22.6,51.49,64.289155455874081,3.97,"Folded Dipole","Yes",null,28.127968755497683,223.85,222.50237500439815,28.127968755497683,0.98003448275862071]
["+PY1MHZ 12",6.907093999999999,15.61,3.8439999999999999,3.5779999999999998,21.532,5.135355180134356,438.77106768013431,-5.3325938518975464,-23.723126722040071,26.56,17.5,19.940000000000001,50.07,99.247305102062086,1.19,"Folded Dipole","Yes",null,28.108750000000001,220.66,222.48699999999999,28.108749999999993,0.98260000000000003]
["+G0KSC 12 LFA",6.907093999999999,15.54,3.78,3.52,21.49,5.2845756820336653,419.17933446859325,-5.1970557003647624,-23.587588570507279,24.4,18.100000000000001,23.1,49.9,99.885644939205122,1.07,"LFA Loop","Yes",null,24.245549664688753,220.66,219.396439731751,24.245549664688753,0.98210344827586205]
["+G0KSC 12 OWA",6.9278984999999995,15.49,3.85,3.5,21.45,5.6271091113610883,448.95135861923512,-5.4966787993234849,-23.887211669466005,25.3,16.3,23.4,49.3,99.940511600237954,1.05,"Dipole","Yes",null,30.004745500562429,225.26,224.00379640044994,30.004745500562429,0.98096551724137926]
["G4CQM 11",6.9903119999999994,15.7,3.92,3.66,21.65,8.544550940717075,492.02888711395104,-5.6141121370320777,-24.004645007174595,30.1,13.3,17.899999999999999,46.2,89.77740756166412,1.94,"Dipole","No",null,37.863862264820725,232,230.29108981185658,37.863862264820725,0.97137931034482761]
["+*InnoV 12 OWL G/T",7.0027946999999999,15.85,3.919,3.6859999999999999,21.77,6.5130627930754752,454.05998572083325,-5.2088462343197204,-23.599379104462241,23.32,15.3,22.8,50.11,97.888815837533784,1.34,"Folded Dipole","Yes",null,30.831100377252021,226.1,224.66488030180162,30.831100377252021,0.9780344827586207]
["+InnoV 12 OWL G/T",7.0027946999999999,15.85,3.9169999999999998,3.6840000000000002,21.77,6.2102000563539246,453.33523087489442,-5.2066208662314057,-23.597153736373926,23.32,15.3,22.8,50.11,97.888815837533784,1.34,"Folded Dipole","Yes",null,30.748538320653722,225.97000000000003,224.59883065652298,30.748538320653722,0.97903448275862071]
["*InnoV/G0KSC 12 LFA3 2020",7.0319209999999996,15.56,3.706,3.4590000000000001,21.45,5.8944209300444106,378.2874019695804,-4.838151489576533,-23.228684359719054,28.38,16.8,24.4,48.67,99.885644939205122,1.07,"LFA Loop","Yes",null,16.123871044918978,214.435,212.89909683593518,16.123871044918978,0.98007931034482754]
["+PY1MHZ 12",7.0444037000000002,15.58,3.7509999999999999,3.4980000000000002,21.48,5.2814653825492748,408.59924494317323,-5.109235067839073,-23.499767937981595,24.6,20.100000000000001,22.6,50.9,97.562712528262921,1.37,"Folded Dipole","Yes",null,22.175690716364755,219.03299999999999,217.7405525730918,22.175690716364755,0.98211379310344826]
["DK7ZB 11",7.0735299999999999,15.83,3.94,3.71,21.76,5.0877192982456299,507.93714912280717,-5.6738844167269233,-24.064417286869443,22.3,14.2,17.399999999999999,27.9,98.58526266762405,1.27,"Dipole","No",null,41.65350877192985,234.3,233.32280701754388,41.65350877192985,0.98275862068965514]
["+UA9TC 12RS",7.0735299999999999,15.7,3.8,3.56,21.61,5.1912951912952039,403.23398560898573,-4.9299187957869055,-23.320451665929426,32.1,18.600000000000001,21.2,51.7,99.814564684874426,1.0900000000000001,"Dipole","No",null,21.143383643383657,218.2,216.91470691470693,21.143383643383657,0.98241379310344823]
["+G0KSC 12 LFA",7.0943345000000004,15.76,4.59,3.6,21.75,5.0049109022028571,440.63937315841184,-5.1326792073169143,-23.523212077459441,26.1,17.3,22.6,50.26,99.017936855774693,1.22,"LFA Loop","Yes",null,28.499894766381395,223.94000000000003,222.79991581310512,28.499894766381395,0.98303448275862071]
["*+G0KSC 12 LFA",7.0943345000000004,15.76,3.9,3.7,21.71,5.0049109022028571,422.12082134839369,-5.0075117961871092,-23.398044666329625,26.1,17.3,22.6,50.26,99.017936855774693,1.22,"LFA Loop","Yes",null,24.875912024694884,221.09000000000003,219.90072961975591,24.875912024694884,0.98303448275862071]
["Cushcraft LFA-2M12EL",7.0984953999999991,15.55,3.7280000000000002,3.4780000000000002,21.41,7.1101533243835107,387.32856991450569,-4.9521202926049899,-23.342653162747517,25.2,17.5,23.8,48.732999999999997,99.852071005917168,1.08,"LFA Loop","Yes",null,17.655267434466175,215.94,214.12421394757294,17.655267434466175,0.97606896551724143]
["MBI 3.4",7.1151389999999992,15.77,3.89,3.64,21.58,9.5014245014244896,454.16172542735058,-5.3609557540895505,-23.751488624232067,23.24,16.010000000000002,19.86,39.340000000000003,97.45074500388391,1.38,"Dipole","No",null,30.266203703703738,226.3,224.21296296296299,30.266203703703738,0.96827586206896554]
["+G0KSC 12LFA 2R",7.1359434999999998,15.61,3.79,3.52,21.52,5.5959368739235789,400.98036975853216,-4.9933136933144393,-23.383846563456959,25,19.3,23.6,50.67,99.814564684874426,1.0900000000000001,"LFA Loop","Yes",null,20.623176689747282,217.89000000000001,216.49854135179783,20.623176689747282,0.98106896551724143]
["+*G0KSC 12LFA 2R",7.1359434999999998,15.61,3.95,3.75,21.62,5.5959368739235789,418.23387139292106,-5.0543606411792883,-23.444893511321808,25,19.3,21.6,50.67,99.814564684874426,1.0900000000000001,"LFA Loop","Yes",null,23.999595796281312,220.54000000000002,219.19967663702505,23.999595796281312,0.98106896551724143]
["InnoV 12 LFA",7.1359434999999998,15.69,3.8,3.6,21.61,6.4921558258417322,406.39588841882613,-4.9429489271263769,-23.333481797268895,23.5,17.399999999999999,23.7,49.3,99.885644939205122,1.07,"LFA Loop","Yes",null,21.507579763793423,218.8,217.20606381103474,21.507579763793423,0.97810344827586204]
["+PY1MHZ 14A",7.1598686749999993,15.63,3.7509999999999999,3.4980000000000002,21.54,3.8494275002533462,404.6420356672408,-5.0306242553555203,-23.421157125498041,26.9,16.899999999999999,20.6,50.73,98.298676748582224,1.3,"Folded Dipole","Yes",null,21.681528017022984,218.297,217.34522241361839,21.681528017022984,0.9869]
["Gulf Alpha 14",7.1567479999999994,15.4,3.71,3.44,21.29,5.5959368739235789,477.02599205651796,-5.8922013037489958,-24.282734173891516,19.91,15.3,21.9,197.98,99.097070084560102,1.21,"T Match","Yes",null,35.504903166848223,229.57,228.40392253347858,35.504903166848223,0.98106896551724143]
["Gulf Alpha 14 XPOL H",7.1567479999999994,15.4,3.57,3.57,21.28,5.5959368739235789,489.1359969772588,-5.9998166566502515,-24.390349526792775,19.920000000000002,15.3,22,198.17099999999999,99.097070084560102,1.21,"T Match","Yes","XPOL",37.874767143509835,231.42999999999998,230.29981371480787,37.874767143509835,0.98106896551724143]
["Gulf Alpha 14 XPOL V",7.1567479999999994,15.4,3.57,3.57,21.28,5.5959368739235789,460.42356595550228,-5.7647047013102846,-24.155237571452805,19.91,15.3,22,197.9,99.097070084560102,1.21,"T Match","Yes","XPOL",32.255896102070203,227.02,225.80471688165616,32.255896102070203,0.98106896551724143]
["YU7EF EF0212",7.2607705000000005,15.82,3.85,3.6,21.7,6.2310672772102871,421.55116238111998,-4.9964196608945715,-23.386952531037089,23.6,16.8,21.9,45.4,92.272804285211578,1.77,"Dipole","No",null,24.52448045086296,221.1,219.61958436069037,24.52448045086296,0.97896551724137937]
["M2 2MXP22A XPOL H",7.2896887549999994,16,3.9895,3.9849999999999999,21.93,11.14226375908618,570.04075804776755,-5.8775994871784789,-24.268132357320997,21.57,14,18.5,203,98.936234390395953,1.23,"T Match","Yes",null,52.622014537902402,243.87,242.09761163032192,52.622014537902402,0.96299999999999997]
["M2 2MXP22A XPOL V",7.2896887549999994,16,3.9895,3.9849999999999999,21.93,11.14226375908618,541.91718587746641,-5.678233391325719,-24.068766261468237,21.57,14,18.5,203,98.936234390395953,1.23,"T Match","Yes",null,47.118380062305327,239.63,237.69470404984426,47.118380062305327,0.96299999999999997]
["InnoV 12 OWL",7.4272064999999996,16.079999999999998,4.1260000000000003,3.8919999999999999,22.05,4.7670954400476839,540.01790158073675,-5.6286067316365083,-24.019139601779035,21.72,13.8,18.5,48.8,99.852071005917168,1.08,"LFA-FD","Yes",null,47.994286915986102,239.23,238.39542953278888,47.994286915986102,0.98382758620689659]
["17LQD EKM#1",7.4688154999999989,15.45,3.75,3.52,21.36,4.2617214835549362,{"$f":"T270/1000*H$8+(1-T270/1000)*D$8+290*(1/X270-1)","v":558.67918999300218},-6.4593739568904667,-24.849906827032985,20.8,15.1,18.100000000000001,50,98.936234390395953,1.23,"Gamma Match",null,null,51.745101469559138,242.1,241.39608117564731,51.745101469559138,0.98551724137931029]
["17LQD EKM#2",7.4688154999999989,15.54,3.75,3.5,21.47,4.5709281961470882,463.93476357267934,{"$f":"F271-10*LOG((T271/1000*H$8+(1-T271/1000)*D$8)+290*(10^(0.1*M$8)/X271-1))+10*LOG(1/X271)","v":-5.6176193113498334},{"$f":"10*LOG(10^(F271/10)*5E-22/X271/1.380649E-23/2500/(T271/1000*H$8+(1-T271/1000)*D$8+290*(10^(M$8/10)/X271-1)))","v":-24.008152181492356},25.6,15.3,19.600000000000001,50,98.76543209876543,1.25,"Gamma Match",null,null,33.14360770577931,227.5,226.51488616462345,33.14360770577931,0.98448275862068968]
["+DL6WU 14",7.5104244999999992,15.78,3.94,3.7,21.68,2.6235212247738349,589.70672407794018,-6.3755885824345198,-24.766121452577039,21.2,14.3,17.399999999999999,51.4,{"$f":"(1-((P272-1)/(P272+1))^2)*10^2","v":98.491843644198212},1.28,"Dipole","No",null,58.137613082811406,246.9,246.51009046624912,58.137613082811406,0.99103448275862072]
["DJ9BV 3.6",7.5104244999999992,15.82,4,3.78,21.72,5.5024595924103759,608.07699402670391,-6.4186097286845607,-24.80914259882708,21.3,13.9,18,53.5,98.298676748582224,1.3,"Dipole","No",null,61.169184820801092,249.7,248.93534785664087,61.169184820801092,0.98137931034482762]
["K1FO 15",7.572838,15.9,3.94,3.71,21.84,{"$f":"290*(1/X274-1)","v":4.2823150675344701},487.37801805584712,-5.4431438813643629,-23.833676751506886,19.7,14.4,19.3,204.9,98.491843644198212,1.28,"T Match","Yes",null,37.787808803975089,231.1,230.23024704318007,37.787808803975089,0.98544827586206896]
["Directive DSEFO144-15",7.572838,15.9,3.94,3.71,21.84,4.2823150675344701,487.37801805584712,-5.4431438813643629,-23.833676751506886,19.7,14.4,19.3,204.9,98.491843644198212,1.28,"T Match","Yes",null,37.787808803975089,231.1,230.23024704318007,37.787808803975089,0.98544827586206896]
["+PY1MHZ 13",7.8536987499999995,16.02,3.9670000000000001,3.7280000000000002,21.907999999999998,5.2555487680717068,398.11346126807172,-4.5823550876681667,-22.972887957810684,29.52,18.100000000000001,20.63,50.31,99.097070084560102,1.21,"Folded Dipole","Yes",null,20.12875,219.5,216.10300000000001,20.128750000000011,0.98219999999999996]
["+EAntenna 144LFA13",7.8536987499999995,15.97,3.9670000000000001,3.706,21.89,6.7432341836914444,410.82843318866651,-4.7011563587371947,-23.091689228879716,25.77,19.600000000000001,23.5,49.17,99.885644939205122,1.07,"LFA Loop","Yes",null,22.325870646766148,219.5,217.86069651741292,22.325870646766148,0.97727586206896555]
["+InnoV 13 OWL G/T v2",7.8849054999999995,16.22,4.08,3.9,22.15,8.3327421071301977,421.64615998581047,-4.5201824713173435,-22.910715341459866,25.5,17.2,22.7,48.3,99.097070084560102,1.21,"Folded Dipole","Yes",null,24.131784320681078,221.28,219.30542745654486,24.131784320681078,0.97206896551724142]
["+*InnoV 13 OWL G/T v2",7.8849054999999995,16.22,4.0999999999999996,3.6,22.14,8.0261525922250954,414.25470427725998,-4.466416757271892,-22.856949627414412,25.5,17.2,22.7,48.3,99.097070084560102,1.21,"Folded Dipole","Yes",null,22.745313441298407,220.13,218.19625075303873,22.745313441298407,0.97306896551724142]
["+InnoV 12 OWL G/T-2",7.9015490999999995,16.48,4.2690000000000001,4.032,22.41,6.2102000563539246,468.01487214708374,-4.6900589393926477,-23.080591809535168,23.94,16.100000000000001,21.7,48.128,57.46691871455576,4.75,"Folded Dipole","Yes",null,33.621266553958868,228.22000000000003,226.89701324316709,33.621266553958868,0.97903448275862071]
["+*InnoV 12 OWL G/T-2",7.9015490999999995,16.48,4.24,4.0190000000000001,22.4,6.2102000563539246,466.7752579952097,-4.6897698418422333,-23.080302711984757,23.94,16.100000000000001,21.7,48.128,57.46691871455576,4.75,"Folded Dipole","Yes",null,33.378680614257483,228.02999999999997,226.70294449140599,33.378680614257483,0.97903448275862071]
["+Dual PA144-13-8",7.9265144999999997,16.21,4.0449999999999999,3.82,22.13,6.9318221939766111,404.90341771704959,-4.4032509070128594,-22.79378377715538,26.26,16.7,22.6,49.48,99.017936855774693,1.22,"Hair Pin","Yes",null,21.129470748155192,218.60999999999999,216.90357659852415,21.129470748155192,0.97665517241379307]
["+*Dual PA144-13-8",7.9265144999999997,16.21,4.2,4,22.2,6.8374982352110836,416.92213751235363,-4.4462712062675349,-22.836804076410058,26.26,16.7,22.6,49.48,99.017936855774693,1.22,"Hair Pin","Yes",null,23.499929408442775,220.44000000000003,218.79994352675422,23.499929408442775,0.97696551724137937]
["DK7ZB 12",7.9681234999999999,16.32,4.21,4,22.26,7.0681737901801505,527.77176792652767,-5.2978348087281031,-23.688367678870627,25.6,13.6,17.899999999999999,26.8,96.503404058430831,1.46,"Dipole","No",null,45.147474390674667,237.4,236.11797951253973,45.147474390674667,0.9762068965517241]
["+PY1MHZ 13",7.9618821499999992,16.010000000000002,3.9169999999999998,3.6840000000000002,21.88,5.7633049527165454,389.06471229017842,-4.5163484399041174,-22.906881310046643,25.3,20.9,24.5,50.2,97.45074500388391,1.38,"Folded Dipole","Yes",null,18.258592433945573,216.07599999999999,214.60687394715646,18.258592433945573,0.98051379310344833]
["+UA9TC 13RS",7.9681234999999999,16.100000000000001,3.94,3.7,21.99,5.2949438202246757,386.26299157303356,-4.3849227373868542,-22.775455607529373,24.3,18.7,20.9,49.7,99.885644939205122,1.07,"Dipole","No",null,17.801966292134814,215.6,214.24157303370785,17.801966292134814,0.98206896551724143]
["*InnoV/G0KSC 13 LFA3 2020",7.9681234999999999,16.11,3.9670000000000001,3.7509999999999999,22.01,7.1458452580328302,380.48626097955656,-4.2841150384739315,-22.674647908616453,28.48,17.2,23.9,48.86,99.247305102062086,1.19,"LFA Loop","Yes",null,16.309279006169035,214.898,213.04742320493523,16.309279006169035,0.97595172413793108]
["+G0KSC 13 LFA",7.9889279999999996,16.23,4.07,3.85,22.16,5.0049109022028571,422.12082134839369,-4.5575117961871099,-22.948044666329626,27.4,16.5,23.6,48.56,99.51325040562466,1.1499999999999999,"LFA Loop","Yes",null,24.875912024694884,221.09000000000003,219.90072961975591,24.875912024694884,0.98303448275862071]
["+G0KSC 13 LFA",8.0097325000000001,16.13,4,3.75,22.04,7.152144724754419,393.51984400395736,-4.3818136926306011,-22.77234656277313,27.42,17.3,24.6,48.8,99.173553719008268,1.2,"LFA Loop","Yes",null,18.858649565401748,216.89000000000001,215.0869196523214,18.858649565401748,0.97593103448275864]
["*G0KSC 13 LFA",8.0097325000000001,16.13,4.0599999999999996,3.9,22.08,7.152144724754419,403.20649159070035,-4.4344023767070695,-22.824935246849591,27.42,17.3,24.6,48.8,99.173553719008268,1.2,"LFA Loop","Yes",null,20.754275316232089,218.37,216.60342025298567,20.754275316232089,0.97593103448275864]
["InnoV 13 LFA",8.0305369999999989,16.13,4.0199999999999996,3.77,22.05,7.152144724754419,395.54880397145081,-4.391371370925512,-22.781904241068037,27.38,17.3,24.6,48.7,99.173553719008268,1.2,"LFA Loop","Yes",null,19.255706310508103,217.20000000000002,215.40456504840648,19.255706310508103,0.97593103448275864]
["YU7EF EF0213M",8.0305369999999989,16,3.92,3.66,21.88,7.1731448763250754,406.0089222614842,-4.6605553197749128,-23.051088189917436,25.7,18.600000000000001,21.1,49.9,99.940511600237954,1.05,"Dipole","No",null,21.29858657243819,218.8,217.03886925795055,21.29858657243819,0.97586206896551719]
["+YU7EF EF0213",8.1553639999999987,16.27,4.05,3.82,22.15,6.1267605633802731,415.08270246478884,-4.488520358754263,-22.879053228896783,22.5,17,23.2,47.9,80.936322158301934,2.5499999999999998,"Dipole","No",null,23.279049295774676,220.10000000000002,218.62323943661974,23.279049295774676,0.97931034482758617]
["InnoV 13 OWL G/T",8.1761684999999993,16.399999999999999,4.24,4.0190000000000001,22.36,4.7154471544715708,516.33053861788608,-5.1430384718090991,-23.533571341951621,23.11,13.6,20.100000000000001,46,99.173553719008268,1.2,"LFA-FD","Yes",null,43.368902439024382,235.57999999999998,234.69512195121951,43.368902439024382,0.98399999999999999]
["IK0BZY 12",8.2177775000000004,16.190000000000001,4.0199999999999996,3.78,22.06,8.0261525922250954,486.26488801871074,-5.1649811642524295,-23.555514034394953,24.6,18.600000000000001,20.7,99.2,96.748185971513038,1.44,"Folded Dipole","Yes",null,36.837325915163532,231.1,229.46986073213083,36.837325915163532,0.97306896551724142]
["+DG7YBN GTV 2-14w",8.2801910000000003,16.239999999999998,4.05,3.82,22.15,5.9183673469387816,406.7219387755103,-4.4134082714572402,-22.803941141599758,28.3,17.399999999999999,20.399999999999999,50.4,99.885644939205122,1.07,"Bent Dipole","No",null,21.683673469387763,218.8,217.34693877551021,21.683673469387763,0.98]
["+*DG7YBN GTV 2-14w",8.2801910000000003,16.239999999999998,4.2,4,22.23,5.9183673469387816,417.15051020408168,-4.430245758037743,-22.820778628180264,28.3,17.399999999999999,20.399999999999999,50.4,99.885644939205122,1.07,"Bent Dipole","No",null,23.724489795918373,220.4,218.9795918367347,23.724489795918373,0.98]
["BVO2-4WL",8.3009955000000009,16.32,4.24,4.0199999999999996,22.29,6.9632768361582169,556.56823799435017,-5.4783429762768785,-23.868875846419396,24,13.3,17.5,45,98.76543209876543,1.25,"Dipole","No",null,50.803319209039515,241.79999999999998,240.64265536723161,50.803319209039515,0.97655172413793101]
["DJ9BV 4.0",8.3426044999999984,16.190000000000001,4.16,3.92,22.06,6.6490299823632988,606.24563492063498,-6.0512104935503066,-24.441743363692829,22.4,14.3,18.3,41.5,97.781801720235393,1.35,"Dipole","No",null,60.586419753086425,249.4,248.46913580246914,60.586419753086425,0.97758620689655173]
["K1FO 16",8.3426044999999984,16.260000000000002,4.16,3.87,22.21,4.2823150675344701,487.37801805584712,-5.0731438813643619,-23.463676751506881,23.78,14.5,19.600000000000001,202.2,98.936234390395953,1.23,"T Match","Yes",null,37.787808803975089,231.1,230.23024704318007,{"$f":"(V300-200)*1.25","v":37.787808803975089},0.98544827586206896]
["+SV 2SA13",8.3426044999999984,16.62,4.38,4.16,22.58,7.0681737901801505,545.43836100317924,-5.1073156113803204,-23.497848481522841,19.600000000000001,14.2,17.3,50.01,99.451303155006855,1.1599999999999999,"Dipole","No",null,48.604733309784542,240.1,238.88378664782763,48.604733309784542,0.9762068965517241]
["#SV 2SA13 XPOL H",8.3426044999999984,16.62,4.2699999999999996,4.2699999999999996,22.58,7.0681737901801505,544.12972447898267,-5.097855710887826,-23.48838858103035,19.559999999999999,14.2,17.3,50.01,99.451303155006855,1.1599999999999999,"Dipole","No","XPOL",48.348640056517134,239.9,238.67891204521371,48.348640056517134,0.9762068965517241]
["#SV 2SA13 XPOL V",8.3426044999999984,16.62,4.2699999999999996,4.2699999999999996,22.58,7.0681737901801505,508.79653832567999,-4.8343236939820091,-23.224856564124533,19.559999999999999,14.2,17.3,50.01,99.451303155006855,1.1599999999999999,"Dipole","No","XPOL",41.434122218297418,234.5,233.14729777463793,41.434122218297418,0.9762068965517241]
["HG VB-215DX",8.3842134999999995,16.239999999999998,4.21,3.97,22.15,5.5232272120317578,487.00906599198839,-5.1137888452371616,-23.504321715379682,19.510000000000002,14.4,18.3,194.49,97.562712528262921,1.37,"T Match","Yes",null,37.472766884531623,231.1,229.9782135076253,37.472766884531623,0.98131034482758617]
["CC3219 MOD",8.4050180000000001,16.28,4.2699999999999996,4.07,22.24,5.1912951912952039,598.28926816426815,-5.8382802743035977,-24.228813144446121,24,12.19,17.600000000000001,32.1,99.990197039505929,1.02,"Dipole","No",null,59.314671814671804,248.2,247.45173745173744,59.314671814671804,0.98241379310344823]
["KLM 16LBX",8.5090404999999993,16.309999999999999,4.26,4.0199999999999996,22.23,6.439901304194537,557.90637116672519,-5.5547828282105218,-23.945315698353042,20.5,14.9,18.7,198.1,98.396292976869248,1.29,"Dual Driven","No",null,51.167606626718332,242,240.93408530137467,51.167606626718332,0.97827586206896555]
["DK7ZB 14 OWL",8.6733960499999991,16.399999999999999,4.1539999999999999,3.9169999999999998,22.3,7.4885037141846151,408.45069862044545,-4.259396551851804,-22.649929421994329,29.96,16.989999999999998,20.79,12.38,99.885644939205122,1.07,"Dipole","No",null,21.714715245843621,219.2,217.3717721966749,21.714715245843621,0.97482758620689658]
["WB9UWA 15",8.696280999999999,15.78,3.75,3.5,21.59,8.068403331561198,340.50458532695365,-4.2753456102289569,-22.665878480371482,32.18,26.1,27.6,203.06800000000001,92.561983471074385,1.75,"T Match","Yes",null,8.3045365940102656,208.89999999999998,206.64362927520821,8.3045365940102656,0.97293103448275864]
["*CC4218XL",8.7170854999999996,16.420000000000002,4.08,3.85,22.03,10.668549569196681,485.47924189338954,-5.1543421028492631,-23.544874972991781,18.739999999999998,13.4,16.399999999999999,200.56299999999999,92.849763179433509,1.73,"T Match","Yes",null,36.166475992992737,231.1,228.93318079439419,36.166475992992737,0.96451724137931039]
["CC4218XL",8.7170854999999996,16.420000000000002,4.33,4.13,22.16,10.668549569196681,485.47924189338954,-5.0243421028492641,-23.414874972991786,18.739999999999998,13.4,16.399999999999999,200.6,92.849763179433509,1.73,"T Match","Yes",null,36.166475992992737,231.1,228.93318079439419,36.166475992992737,0.96451724137931039]
["+PY1MHZ 14 V2",8.766,16.399999999999999,4.085,3.8439999999999999,22.279,4.9552481692432675,364.38737316924323,-3.8797781528073441,-22.270311022949866,32.11,18.64,23.09,50.72,97.67308244757254,1.36,"Folded Dipole","Yes",null,13.5875,216.98,210.87,13.587500000000006,0.98319999999999996]
["+G0KSC 14 LFA 3R",8.8003035000000001,16.54,4.1900000000000004,3.97,22.44,5.8559065644128605,394.89743544642226,-4.0117344718568511,-22.402267341999369,27.7,16.899999999999999,23.7,48.8,99.885644939205122,1.07,"LFA Loop","Yes",null,19.381903890804182,216.98,215.50552311264335,19.381903890804182,0.98020689655172411]
["+*G0KSC 14 LFA 3R",8.8003035000000001,16.54,4.1849999999999996,4,22.45,5.6063268892794298,395.83057996485059,-4.0139303463637868,-22.404463216506304,27.7,16.899999999999999,23.7,48.8,99.885644939205122,1.07,"LFA Loop","Yes",null,19.613356766256587,217.1,215.69068541300527,19.613356766256587,0.98103448275862071]
["+Antennas-Amp PA144-14-9",8.8003035000000001,16.28,3.99,3.75,22.13,7.6991150442477991,343.94235398230074,-3.7774482526703443,-22.167981122812868,28.4,19.5,22.7,49.7,99.978160110655438,1.03,"Hair Pin","Yes",null,9.0495575221238767,209.38,207.2396460176991,9.0495575221238767,0.97413793103448276]
["+*Antennas-Amp PA144-14-9",8.8003035000000001,16.28,4.2,4,22.24,7.9100247963159802,350.99664364151613,-3.7407088938912278,-22.131241764033746,28.4,19.5,22.7,49.7,99.978160110655438,1.03,"Hair Pin","Yes",null,10.388770811193773,210.48,208.31101664895502,10.388770811193773,0.97344827586206895]
["+PY1MHZ 14B",8.7998874100000002,16.46,4.2110000000000003,3.9670000000000001,22.34,5.3945150050579187,431.37927110261916,-4.4557963608832853,-22.846329231025813,31.05,15.5,21.8,50.1,89.333287986486638,1.97,"Folded Dipole","Yes",null,26.611498257839763,222.54400000000001,221.28919860627181,26.611498257839763,0.9817379310344827]
["+InnoV 14 LFA Ver 3",8.8163229649999995,16.489999999999998,4.1820000000000004,3.9670000000000001,22.41,5.564771209671715,406.07655777746544,-4.1519095888054682,-22.542442458947988,31.05,15.5,21.8,49.67,99.097070084560102,1.21,"LFA Loop","Yes",null,21.626572713853953,218.67000000000002,217.30125817108316,21.626572713853953,0.98117241379310349]
["YU7EF EF0214M",8.8211080000000006,16.38,4.07,3.85,22.23,7.1731448763250754,414.51806537102476,-4.3898116937960854,-22.780344563938609,24.6,18.600000000000001,20.9,48.6,99.885644939205122,1.07,"Dipole","No",null,22.963780918727927,220.1,218.37102473498234,22.963780918727927,0.97586206896551719]
["+UA9TC 14RS",8.8211080000000006,16.48,4.13,3.8,22.37,5.2949438202246757,393.41752984550544,-4.0746694325323558,-22.465202302674882,25,18.5,20.3,49.5,99.915166368177964,1.06,"Dipole","No",null,19.202071629213471,216.7,215.36165730337078,19.202071629213471,0.98206896551724143]
["+InnoV 13 OWL G/T-2",8.8211080000000006,16.86,4.42,4.2,22.78,5.907955385102575,434.42777347735824,-4.0362093807874411,-22.426742250929962,27.04,15.7,21.4,50.21,59.927615520579081,4.45,"Folded Dipole","Yes",null,27.107596495549053,223.04999999999998,221.68607719643924,27.107596495549053,0.98003448275862071]
["+*InnoV 13 OWL G/T-2",8.8211080000000006,16.86,4.5,4.33,22.82,5.907955385102575,439.64187572569568,-4.042159299951682,-22.432692170094199,27.04,15.7,21.4,50.21,59.927615520579081,4.45,"Folded Dipole","Yes",null,28.127968755497683,223.85,222.50237500439815,28.127968755497683,0.98003448275862071]
["+DK7ZB 13",8.8585560999999995,16.7,4.5890000000000004,4.3920000000000003,22.71,5.8142806894125831,621.1431586352445,-5.5090646159036325,-23.899597486046154,22.85,12.4,15.8,27.21,99.017936855774693,1.22,"Dipole","No",null,63.66514245515301,251.7,250.93211396412241,63.66514245515301,0.98034482758620689]
["G4CQM CQM14DXL",8.9043259999999993,16.38,4.0199999999999996,3.77,22.23,3.6965252313602415,357.52691199580937,-3.8733288222178617,-22.263861692360386,26.7,19.7,23,50,98.396292976869248,1.29,"Dipole","No",null,12.491269425528202,211,209.99301554042256,12.491269425528202,0.98741379310344823]
["*InnoV/G0KSC 14 LFA3 2020",8.9396936499999988,16.489999999999998,4.3,4,22.52,7.1017564684104295,368.1209144092586,-3.6498691463561515,-22.040402016498675,29.46,17.399999999999999,25,47.8,97.45074500388391,1.38,"LFA Loop","Yes",null,13.898073961027038,213.00399999999999,211.11845916882163,13.898073961027038,0.9760965517241379]
["Cushcraft LFA-2M14EL",8.9459349999999986,16.420000000000002,4.0990000000000002,3.8679999999999999,22.27,7.7201925800056177,399.66512673463581,-4.2035073185343483,-22.594040188676871,25.8,23.8,23.9,51.5,99.67960128159487,1.1200000000000001,"LFA Loop","Yes",null,19.950084961767161,217.88,215.96006796941373,19.950084961767161,0.97406896551724143]
["+G0KSC 14 LFA",8.9459349999999986,16.66,4.24,4.0199999999999996,22.56,5.5959368739235789,402.28252082527843,-3.9656787312241075,-22.356211601366631,26.8,16.899999999999999,24.5,47.1,99.017936855774693,1.22,"LFA Loop","Yes",null,20.878000773259267,218.09,216.70240061860741,20.878000773259267,0.98106896551724143]
["+*G0KSC 14 LFA",8.9459349999999986,16.66,4.16,3.94,22.52,5.5959368739235789,395.9019805982212,-3.9447508240302707,-22.335283694172791,26.8,16.899999999999999,24.5,47.1,99.017936855774693,1.22,"LFA Loop","Yes",null,19.62936276405042,217.10999999999999,215.70349021124034,19.62936276405042,0.98106896551724143]
["+KF2YN Boxkite 16",8.9459349999999986,18,5.5,5.0999999999999996,23.98,6.3354474982381603,462.61751233262862,-3.0734422738752682,-21.463975144017795,29.4,19.100000000000001,25,50.5,99.451303155006855,1.1599999999999999,"Dipole","Yes",null,32.540521494009873,227.4,226.0324171952079,32.540521494009873,0.97862068965517246]
["InnoV 14 LFA",8.9875439999999998,16.579999999999998,4.18,3.97,22.48,7.7096534390597977,384.72065825338967,-3.8488567157464697,-22.239389585888993,27.6,17.3,25.2,48.6,99.773242630385482,1.1000000000000001,"LFA Loop","Yes",null,17.02759389712913,215.6,213.6220751177033,17.02759389712913,0.97410344827586204]
["*InnoV 14 LFA",8.9875439999999998,16.579999999999998,4,4,22.42,7.0996573285760078,378.23920761649055,-3.8522882816310409,-22.242821151773562,27.6,17.3,25.2,48.6,99.773242630385482,1.1000000000000001,"LFA Loop","Yes",null,15.878581269650596,214.54999999999998,212.70286501572048,15.878581269650596,0.97610344827586204]
["+InnoV 14 OWL G/T v2",8.9875439999999998,16.739999999999998,4.3,4.09,22.64,8.3327421071301977,426.11446434905974,-4.0706012682710222,-22.461134138413541,24.34,17.399999999999999,21.5,49.88,97.33723149104533,1.39,"Folded Dipole","Yes",null,25.006207875132986,221.95999999999998,220.00496630010639,25.006207875132986,0.97206896551724142]
["+*InnoV 14 OWL G/T v2",8.9875439999999998,16.739999999999998,4.2,4.0999999999999996,22.64,8.3327421071301977,422.8946567931892,-4.0415138795150893,-22.432046749657609,24.34,17.399999999999999,21.5,49.88,97.33723149104533,1.39,"Folded Dipole","Yes",null,24.376108549130926,221.47000000000003,219.50088683930474,24.376108549130926,0.97206896551724142]
["+*InnoV 14 OWL G/T v2",8.9875439999999998,16.739999999999998,4.1500000000000004,4,22.57,8.3327421071301977,418.42635242993958,-4.0708221878370479,-22.461355057979571,24.34,17.399999999999999,21.5,49.88,97.33723149104533,1.39,"Folded Dipole","Yes",null,23.501684994678946,220.79,218.80134799574316,23.501684994678946,0.97206896551724142]
["+*Dual PA144-14-9",9.0083485000000003,16.62,4.45,4.3,22.62,7.6043030538943235,{"$f":"T334/1000*H$8+(1-T334/1000)*D$8+290*(1/X334-1)","v":407.46821808981218},-3.928715774083734,-22.319248644226256,27.54,16.7,21.7,50.87,99.318239205454091,1.18,"Hair Pin","Yes",null,21.499787678261804,219.06,217.19983014260944,21.499787678261804,0.97444827586206895]
["+Dual PA144-14-9",9.0083485000000003,16.62,4.24,4.0199999999999996,22.53,7.878369284171038,398.19422307229132,{"$f":"F335-10*LOG((T335/1000*H$8+(1-T335/1000)*D$8)+290*(10^(0.1*M$8)/X335-1))+10*LOG(1/X335)","v":-3.9274474429469075},{"$f":"10*LOG(10^(F335/10)*5E-22/X335/1.380649E-23/2500/(T335/1000*H$8+(1-T335/1000)*D$8+290*(10^(M$8/10)/X335-1)))","v":-22.317980313089429},27.54,16.7,21.7,50.87,99.318239205454091,1.18,"Hair Pin","Yes",null,19.631282541706518,217.67,215.70502603336521,19.631282541706518,0.97355172413793101]
["YU7EF EF0214",9.091566499999999,16.63,4.21,4,22.48,9.0753911806543446,412.83285917496431,-4.0998387124873608,-22.49037158262988,22.8,17.5,22.8,41,{"$f":"(1-((P336-1)/(P336+1))^2)*10^2","v":84.481175390266287},2.2999999999999998,"Dipole","No",null,22.261735419630142,220,217.80938833570411,22.261735419630142,0.96965517241379307]
["YU7EF 14LT",9.091566499999999,16.059999999999999,3.89,3.64,21.75,12.191879266978116,351.23998383039896,-4.1799227957336074,-22.570455665876135,29.1,23.2,24.7,47.8,98.396292976869248,1.29,"Dipole","No",null,9.5984549047790324,211,207.67876392382323,9.5984549047790324,0.95965517241379306]
["K1FO 17",9.1539800000000007,16.57,4.24,4.0199999999999996,22.62,{"$f":"290*(1/X338-1)","v":4.6122048623274985},476.8973936803755,-4.5741178041144144,-22.964650674256937,23.03,14.6,19.399999999999999,200.369,96.127481814809428,1.49,"T Match","Yes",null,35.672248300987874,229.5,228.5377986407903,35.672248300987874,0.98434482758620689]
["DJ9BV 4.4",9.1747844999999995,16.47,4.2699999999999996,4.07,22.33,6.7537050105857288,619.98284227240651,-5.8689815816050546,-24.259514451747577,19.600000000000001,14.5,18.100000000000001,38.299999999999997,97.67308244757254,1.36,"Dipole","No",null,63.254234297812282,251.5,250.60338743824983,63.254234297812282,0.97724137931034483]
["SHARK 20",9.2996114999999993,16.489999999999998,4.33,4.0999999999999996,22.34,3.9531632296399688,664.87915064662718,-6.176272312234536,-24.566805182377056,22.4,13.3,18,42.8,99.940511600237954,1.05,"Dipole","No",null,72.588255854596326,258.5,258.07060468367706,72.588255854596326,0.98655172413793102]
["I0JXX 16JXX2",9.2996114999999993,16.5,4.16,3.94,22.39,7.6780404927085177,397.85408112699997,-4.0667553617275685,-22.457288231870088,25.43,17.600000000000001,21.6,199.49,99.961553248750477,1.04,"T Match","Yes",null,19.603921846240979,217.6,215.68313747699278,19.603921846240979,0.9742068965517241]
["*CC17B2",9.3412205000000004,16.66,3.66,3.51,22.09,6.012107986343322,445.46220653972074,-4.8215256684587855,-23.212058538601312,22.9,15.8,21.7,200.1,99.173553719008268,1.2,"T Match","Yes",null,29.246594628840974,224.75,223.39727570307278,29.246594628840974,0.9796896551724138]
["CC17B2",9.3412205000000004,16.66,4.2699999999999996,4.07,22.58,6.012107986343322,470.36830804969912,-4.5421233501581666,-22.932656220300686,22.9,15.8,21.7,200.1,99.173553719008268,1.2,"T Match","Yes",null,34.120587096547119,228.57,227.2964696772377,34.120587096547119,0.9796896551724138]
["RA3AQ-14",9.5908745,16.86,4.2699999999999996,4.07,22.7,5.0877192982456299,408.68884649122828,-3.8925820950618175,-22.283114965204334,28.4,15.8,20.5,50,99.247305102062086,1.19,"Folded Dipole","Yes",null,22.231140350877219,219.03,217.78491228070177,22.231140350877219,0.98275862068965514]
["G4CQM 16",9.6532879999999981,16.7,4.3899999999999997,4.18,22.62,9.0753911806543446,509.00880156472249,-4.7696173814136911,-23.160150251556214,34,12.8,17,50.9,92.127736659593197,1.78,"Dipole","No",null,41.082859174964419,234.6,232.86628733997154,41.082859174964419,0.96965517241379307]
["YU7EF EF0215M",9.7365059999999986,16.739999999999998,4.21,4,22.55,7.1731448763250754,420.40901060070684,-4.1238463052211944,-22.514379175363715,25.7,18.100000000000001,20.8,48.6,99.978160110655438,1.03,"Dipole","No",null,24.116607773851619,221,219.2932862190813,24.116607773851619,0.97586206896551719]
["+InnoV 14 OWL G/T-2",9.7365059999999986,17.21,4.5999999999999996,4.38,23.13,5.3053126865409279,446.0313827732715,-3.7956832140689536,-22.186216084211473,26.49,14.8,20.6,48.18,73.401380086651159,3.13,"Folded Dipole","Yes",null,29.496295515994255,224.79000000000002,223.5970364127954,29.496295515994255,0.98203448275862071]
["+*InnoV 14 OWL G/T-2",9.7365059999999986,17.21,4.75,4.5999999999999996,23.21,5.3053126865409279,441.608421995154,-3.677226050005141,-22.067758920147661,26.49,14.8,20.6,48.18,73.401380086651159,3.13,"Folded Dipole","Yes",null,28.630745461568132,224.10999999999999,222.90459636925451,28.630745461568132,0.98203448275862071]
["+PY1MHZ 15 V2",9.7850000000000001,16.760000000000002,4.2690000000000001,4.0190000000000001,22.620999999999999,5.7674655787863305,356.21876557878636,-3.4421486739199891,-21.832681544062513,30.43,24.68,26.36,49.42,99.318239205454091,1.18,"Folded Dipole","Yes",null,11.83,209.40899999999999,209.464,11.829999999999998,0.98050000000000004]
["DK7ZB 14",9.8405285000000013,17.07,4.59,4.3899999999999997,23.02,6.9632768361582169,499.00856285310726,-4.3197790652053287,-22.71031193534785,26.2,13,18.2,26.9,96,1.5,"Dipole","No",null,39.539194915254221,233,231.63135593220338,39.539194915254221,0.97655172413793101]
["+PY1MHZ 15",9.8363675999999991,16.73,4.1820000000000004,3.9670000000000001,22.56,6.1371879291524429,345.34313752244793,-3.3822879674616861,-21.772820837604208,28.7,20.100000000000001,27.3,50.32,97.562712528262921,1.37,"Folded Dipole","Yes",null,9.6293443431106596,209.40899999999999,207.70347547448853,9.6293443431106596,0.97927586206896555]
["+DG7YBN GTV 2-16w",9.8613330000000001,16.95,4.3899999999999997,4.21,22.86,5.9287800415215202,422.4246102959288,-3.8482749010805648,-22.238807771223087,28.9,15.8,20.6,46.6,99.318239205454091,1.18,"Bent Dipole","Yes",null,24.754565607516099,221.20999999999998,219.80365248601288,24.754565607516099,0.97996551724137926]
["*DG7YBN GTV 2-16w",9.8613330000000001,16.95,4.5999999999999996,4.45,22.94,5.9287800415215202,428.81233505753215,-3.8259023311524132,-22.216435201294935,28.9,15.8,20.6,46.6,99.318239205454091,1.18,"Bent Dipole","Yes",null,26.00460959217429,222.19000000000003,220.80368767373943,26.00460959217429,0.97996551724137926]
["G0KSC 15 LFA",9.8821374999999989,16.850000000000001,4.2699999999999996,4.07,22.72,7.404342598486453,369.1942587877503,-3.4570077425888464,-21.847540612731372,30.3,19.600000000000001,24.5,49.9,99.386268555288922,1.17,"LFA Loop","Yes",null,14.048907277742444,213.20000000000002,211.23912582219396,14.048907277742444,0.97510344827586204]
["*G0KSC 15 LFA",9.8821374999999989,16.850000000000001,4.5999999999999996,4.45,22.85,7.6991150442477991,381.44884955752212,-3.4466382047392137,-21.837171074881731,30.3,19.600000000000001,24.5,49.9,99.386268555288922,1.17,"LFA Loop","Yes",null,16.389380530973447,215.1,213.11150442477876,16.389380530973447,0.97413793103448276]
["InnoV 15 LFA",9.9029419999999995,16.850000000000001,4.3,4.0999999999999996,22.76,7.0996573285760078,358.73845691878324,-3.3127428777919059,-21.703275747934427,29.8,17.100000000000001,26.3,49,99.386268555288922,1.17,"LFA Loop","Yes",null,12.062387395343883,211.57,209.64990991627511,12.062387395343883,0.97610344827586204]
["*InnoV 15 LFA",9.9029419999999995,16.850000000000001,4.5999999999999996,4.45,22.85,7.7096534390597977,381.37642925413303,-3.4457853410097048,-21.836318211152225,29.8,17.100000000000001,26.3,49,99.386268555288922,1.17,"LFA Loop","Yes",null,16.37314595206913,215.09,213.0985167616553,16.37314595206913,0.97410344827586204]
["K1FO 18",9.9445510000000006,16.86,4.3600000000000003,4.16,22.75,4.3956313228550865,471.97649385654762,-4.4066499878765066,-22.797182858019028,20.5,14.8,19.100000000000001,199.9,98.097502972651611,1.32,"T Match","Yes",null,34.751636503658041,228.73,227.80130920292643,34.751636503658041,0.98506896551724132]
["+InnoV 15 OWL G/T",9.9445510000000006,17.059999999999999,4.42,4.2,22.94,7.730732467164656,399.26545739370556,-3.529562611042917,-21.920095481185442,27.76,18.100000000000001,22.2,49.5,98.199059238020283,1.31,"Folded Dipole","Yes",null,19.869809183276104,217.82,215.89584734662088,19.869809183276104,0.9740344827586207]
["*+InnoV 15 OWL G/T",9.9445510000000006,17.059999999999999,4.55,4.2,22.97,7.730732467164656,401.82299005204084,-3.5238850365265479,-21.914417906669073,27.8,18.100000000000001,22.2,49.5,98.199059238020283,1.31,"Folded Dipole","Yes",null,20.370304811130353,218.20999999999998,216.29624384890428,20.370304811130353,0.9740344827586207]
["*M2 28 XPOL H",10.006964499999999,17.309999999999999,4.5,4.5,23.12,15.229920516822112,571.58864733422865,-4.6450795315730486,-23.035612401715568,20.11,13.24,18.87,200.2,54.180879578036389,5.19,"T Match","Yes","XPOL",52.124995463288961,244.11,241.69999637063117,52.124995463288961,0.95010344827586202]
["*M2 28 XPOL V",10.006964499999999,17.309999999999999,4.5,4.5,23.12,15.229920516822112,541.26813323413057,-4.4305606076603494,-22.821093477802865,20.100000000000001,13.24,18.899999999999999,200.23,54.180879578036389,5.19,"T Match","Yes","XPOL",46.191431060138655,239.6,236.95314484811092,46.191431060138655,0.95010344827586202]
["#M2 28 XPOL H",10.006964499999999,17.309999999999999,4.83,4.83,23.28,15.229920516822112,560.09239919428001,-4.4049851698039637,-22.795518039946483,20.11,13.24,18.899999999999999,200.23,54.180879578036389,5.19,"T Match","Yes","XPOL",49.87524044568648,242.39999999999998,239.90019235654918,49.87524044568648,0.95010344827586202]
["#M2 28 XPOL V",10.006964499999999,17.309999999999999,4.83,4.83,23.28,15.229920516822112,529.43573748775077,-4.183884695789355,-22.574417565931878,20.100000000000001,13.2,18.899999999999999,200.23,54.180879578036389,5.19,"T Match","Yes","XPOL",43.87589373207998,237.83999999999997,235.10071498566398,43.87589373207998,0.95010344827586202]
["DJ9BV 4.8",10.027769000000001,16.78,4.4000000000000004,4.1900000000000004,22.63,6.7537050105857288,563.117413549753,-5.1873188901413227,-23.577851760283846,21,14.7,18,49.7,98.396292976869248,1.29,"Dipole","No",null,52.125970359915321,242.8,241.70077628793226,52.125970359915321,0.97724137931034483]
["*M2 5WL",10.0485735,16.809999999999999,4.2670000000000003,4.2670000000000003,22.47,7.3097182451303055,581.43119189026766,-5.4665187033009923,-23.857051573443513,20,14.3,17.600000000000001,200.9,96.987910661840033,1.42,"T Match","Yes",null,55.601071163431968,245.6,244.48085693074557,55.601071163431968,0.97541379310344822]
["M2 5WL",10.0485735,16.809999999999999,4.5599999999999996,4.3600000000000003,22.73,3.7478169752008395,597.52776807544547,-5.3626994281704805,-23.753232298313005,20,14.3,17.600000000000001,200.9,96.987910661840033,1.42,"T Match","Yes",null,59.448131330771936,248.1,247.55850506461755,59.448131330771936,0.98724137931034484]
["YU7EF EF0215",10.069377999999999,17.04,4.46,4.24,22.93,10.668549569196681,399.38694987665781,-3.5033544566512833,-21.893887326793802,25.6,17.899999999999999,22.8,41.8,72.800531123371712,3.18,"Dipole","No",null,19.318669336098075,218.1,215.45493546887846,{"$f":"(V368-200)*1.25","v":19.318669336098075},0.96451724137931039]
["+RU1AA_2",10.1734005,17.21,4.62,4.42,23.13,6.7537050105857288,495.79397494707138,-4.1873057977797989,-22.577838667922322,24.3,15,17,50,98.76543209876543,1.25,"Dipole","No",null,38.951129146083296,232.5,231.16090331686664,38.951129146083296,0.97724137931034483]
["+RA3AQ 15",10.235814,17.309999999999999,4.67,4.49,23.26,6.9632768361582169,495.08403954802259,-4.0489593484663056,-22.439492218608827,24.4,14.2,17.600000000000001,51.7,99.67960128159487,1.1200000000000001,"Dipole","No",null,38.771186440677958,232.4,231.01694915254237,38.771186440677958,0.97655172413793101]
["*+SM5BSZ 14 XPOL H",10.298227499999999,17.420000000000002,5.2,5.2,23.5,5.8142806894125831,541.65327119240249,-4.1765492784279381,-22.567082148570456,18.899999999999999,15,19.100000000000001,48.5,61.678004535147387,4.25,"Dipole","No","XPOL",48.109391487864954,239.5,238.48751319029196,48.109391487864954,0.98034482758620689]
["*+SM5BSZ 14 XPOL V",10.298227499999999,17.420000000000002,5.2,5.2,23.5,5.8142806894125831,514.28790010552257,-3.972914696695653,-22.363447566838175,18.899999999999999,15,19.100000000000001,48.5,61.678004535147387,4.25,"Dipole","No","XPOL",42.754132958142854,235.3,234.20330636651428,42.754132958142854,0.98034482758620689]
["+SM5BSZ 14",10.298227499999999,17.420000000000002,4.7300000000000004,4.5199999999999996,23.29,5.8142806894125831,554.48893334505817,-4.4788706560953244,-22.869403526237843,18.899999999999999,15,19.100000000000001,48.5,61.678004535147387,4.25,"Dipole","No",null,50.62126275061555,241.47,240.49701020049244,50.62126275061555,0.98034482758620689]
["+SM5BSZ 14 XPOL H",10.298227499999999,17.420000000000002,4.5999999999999996,4.5999999999999996,23.28,5.8142806894125831,549.47194864579672,-4.453018916127558,-22.843551786270076,18.899999999999999,15,19.100000000000001,48.5,61.678004535147387,4.25,"Dipole","No","XPOL",49.63946535349983,240.7,239.71157228279986,49.63946535349983,0.98034482758620689]
["+SM5BSZ 14 XPOL V",10.298227499999999,17.420000000000002,4.5999999999999996,4.5999999999999996,23.28,5.8142806894125831,529.92525501231125,-4.3104437643005156,-22.700976634443034,18.899999999999999,15,19.100000000000001,48.5,61.678004535147387,4.25,"Dipole","No","XPOL",45.814280689412641,237.70000000000002,236.65142455153011,45.814280689412641,0.98034482758620689]
["K5GW 17",10.360641000000001,16.98,4.43,4.21,22.88,10.142755174875081,417.54327266238397,-3.7295918789490927,-22.12012474909162,25.7,15.9,20.5,48.5,92.849763179433509,1.73,"Dipole","No",null,22.974660956459658,220.79999999999998,218.37972876516773,22.974660956459658,0.96620689655172409]
["SM2CEW 19",10.3814455,17.059999999999999,4.49,4.2699999999999996,22.97,9.2882562277580085,434.07587188612092,-3.7994058225491472,-22.189938692691666,22.1,15.3,20.2,78.400000000000006,94.400093234659991,1.62,"Folded Dipole","Yes",null,26.377224199288243,223.24,221.10177935943059,26.377224199288243,0.96896551724137936]
["#SM2CEW 19 XPOL H",10.3814455,16.82,4.38,4.38,22.75,10.282072339058089,527.65900935480408,-4.7647686547571642,-23.155301524899684,20.04,14.6,18.3,72.900000000000006,93.27846364883402,1.7,"Folded Dipole","Yes","XPOL",44.496465169421917,237.45999999999998,235.59717213553753,44.496465169421917,0.96575862068965512]
["#SM2CEW 19 XPOL V",10.3814455,17,4.38,4.38,22.9,9.277605779153788,448.71478328173362,-3.9972631911867085,-22.387796061329226,24.82,15.1,19.3,82.6,93.13598671042061,1.71,"Folded Dipole","Yes","XPOL",29.244066047471584,225.45999999999998,223.39525283797727,29.244066047471584,0.96899999999999997]
["+G0KSC 16 OWL XPOL H",10.3814455,16.91,4.25,4.25,22.79,8.9478174321057917,410.72906743210581,-3.771951812297889,-22.162484682440411,26.32,18.23,23.2,51.7,99.814564684874426,1.0900000000000001,"Folded Dipole","Yes","XPOL",21.875,219.67000000000002,217.5,21.875,0.97006896551724142]
["+G0KSC 16 OWL XPOL V",10.3814455,16.899999999999999,4.25,4.25,22.77,9.2989074344282567,390.62749564041434,-3.5964508592079172,-21.986983729350442,25.15,17.600000000000001,21.6,44.66,97.781801720235393,1.35,"Folded Dipole","Yes","XPOL",17.872522153813328,216.65,214.29801772305066,17.872522153813328,0.96893103448275864]
["*BVO-5WL",10.443858999999998,17.149999999999999,4.58,4.4000000000000004,23.07,7.0681737901801505,526.46313140233121,-4.4780883023031262,-22.86862117244565,26.3,13.3,17.100000000000001,47.4,98.676482105098287,1.26,"Dipole","No",null,44.891381137407258,237.2,235.91310490992581,44.891381137407258,0.9762068965517241]
["BVO-5WL",10.443858999999998,17.149999999999999,4.66,4.49,23.11,7.0681737901801505,524.5001766160367,-4.4234274071650308,-22.813960277307554,26.3,13.3,17.100000000000001,47.4,98.676482105098287,1.26,"Dipole","No",null,44.50724125750618,236.9,235.60579300600494,44.50724125750618,0.9762068965517241]
["+PY1MHZ 16",10.593,17.010000000000002,4.2990000000000004,4.0990000000000002,22.838999999999999,5.2555487680717068,342.09508626807173,-3.079116629812678,-21.469649499955203,28.51,20.41,25.02,50.2,97.33723149104533,1.39,"Folded Dipole","Yes",null,9.1662499999999998,224.6,207.333,9.166249999999998,0.98219999999999996]
["+InnoV 15 OWL G/T-2",10.631099499999999,17.53,4.8099999999999996,4.6100000000000003,23.48,5.3053126865409279,444.79555549703275,-3.4349720677690301,-21.82550493791155,28.51,14.2,20,48.76,74.875156249028294,3.01,"Folded Dipole","Yes",null,29.254450647845758,224.6,223.40356051827661,29.254450647845758,0.98203448275862071]
["+*InnoV 15 OWL G/T-2",10.631099499999999,17.53,4.9000000000000004,4.7,23.51,5.3053126865409279,440.95798658660743,-3.3715417524563294,-21.762074622598849,28.51,14.2,20,48.76,74.875156249028294,3.01,"Folded Dipole","Yes",null,28.503458688858423,224.01,222.80276695108674,28.503458688858423,0.98203448275862071]
["YU7EF EF0216M",10.651904,17.05,4.3600000000000003,4.16,22.85,7.1731448763250754,426.29995583038874,-3.8772168753372207,-22.267749745479737,25.1,17.899999999999999,21.3,49.9,99.978160110655438,1.03,"Dipole","No",null,25.269434628975276,221.9,220.21554770318022,25.269434628975276,0.97586206896551719]
["PY1MHZ 17",10.68,17.21,4.6239999999999997,4.423,23.113999999999997,6.7055453243298269,433.08505782432985,-3.6799426154091393,-22.070475485551661,26.89,14.88,19.649999999999999,48.68,99.814564684874426,1.0900000000000001,"Folded Dipole","Yes",null,26.688749999999999,213.92000000000002,221.351,26.688749999999999,0.97740000000000005]
["+G0KSC 16 LFA3R",10.693512999999999,17.23,4.46,4.24,23.06,6.1789047367494305,374.73874361683397,-3.1888676148460551,-21.579400484988575,25.3,17.5,23.7,49.9,99.773242630385482,1.1000000000000001,"LFA Loop","Yes",null,15.373745377707344,213.92000000000002,212.29899630216588,15.373745377707344,0.97913793103448277]
["K1FO 19",10.735122,17.16,4.49,4.2699999999999996,23,4.6638169650677881,457.53936004344615,-4.0325978297983722,-22.423130699940895,21,18.8,18.8,204.9,98.76543209876543,1.25,"T Match","Yes",null,31.873883185592646,226.52,225.49910654847412,31.873883185592646,0.9841724137931035]
["Directive DSEFO144-19",10.735122,17.16,4.49,4.2699999999999996,23,4.6638169650677881,457.53936004344615,-4.0325978297983722,-22.423130699940895,21,18.8,18.8,204.9,98.76543209876543,1.25,"T Match","Yes",null,31.873883185592646,226.52,225.49910654847412,31.873883185592646,0.9841724137931035]
["+G0KSC 16 LFA",10.8391445,17.55,4.5599999999999996,4.33,23.44,5.8975441559354973,362.93685349377233,-2.6917432638080263,-21.082276133950547,28.5,17.5,24.4,49.2,99.627498953029601,1.1299999999999999,"LFA Loop","Yes",null,13.119238617971973,212.07999999999998,210.49539089437758,13.119238617971973,0.98006896551724143]
["+*G0KSC 16 LFA",10.8391445,17.55,4.5999999999999996,4.4000000000000004,23.46,5.8975441559354973,363.5885933431847,-2.6784979180246125,-21.069030788167137,28.5,17.5,24.4,49.2,99.627498953029601,1.1299999999999999,"LFA Loop","Yes",null,13.246780662866762,212.17999999999998,210.59742453029341,13.246780662866762,0.98006896551724143]
["+Eantenna 144LFA16 H",10.8391445,17.32,4.46,4.46,23.18,6.0433680653337003,408.47667910447757,-3.398240528208174,-21.788773398350699,27.5,17.5,24.5,49,99.627498953029601,1.1299999999999999,"LFA Loop","Yes","XPOL",22.002604900028153,219.07999999999998,217.60208392002252,22.002604900028153,0.97958620689655174]
["+EAntenna 144LFA16 V",10.8391445,17.32,4.46,4.46,23.21,5.741463586172932,385.78236979990857,-3.1544628698933472,-21.544995740035869,27.5,17.5,24.5,49,99.627498953029601,1.1299999999999999,"LFA Loop","Yes","XPOL",17.620529591729088,215.57,214.09642367338327,17.620529591729088,0.98058620689655174]
["Cushcraft LFA-2M16EL",10.84538585,17.09,4.3920000000000003,4.1820000000000004,22.92,9.5440946003704177,388.16735824191483,-3.4193803660187712,-21.809913236161293,28.01,18.95,25.06,52.36,99.814564684874426,1.0900000000000001,"LFA Loop","Yes",null,17.343104430830607,216.3,213.87448354466449,17.343104430830607,0.96813793103448276]
["+EAntenna 144LFA16",10.84538585,17.32,4.5549999999999997,4.3600000000000003,23.21,6.0329473054313549,396.28942412615709,-3.2528505342736942,-21.64338340441622,27.46,17.5,24.5,48.99,99.627498953029601,1.1299999999999999,"LFA Loop","Yes",null,19.619662782920884,217.20999999999998,215.69573022633671,19.619662782920884,0.97962068965517246]
["InnoV 16 LFA",10.880753500000001,17.25,4.5199999999999996,4.2300000000000004,23.12,8.3327421071301977,{"$f":"T398/1000*H$8+(1-T398/1000)*D$8+290*(1/X398-1)","v":371.83770840723645},-3.0721602498311595,-21.462693119973679,29.9,17.7,25.5,47.3,99.627498953029601,1.1299999999999999,"LFA Loop","Yes",null,14.384533522525693,213.7,211.50762681802055,14.384533522525693,0.97206896551724142]
["RU1AA 15",10.963971499999998,17.59,4.87,4.7,23.52,9.5014245014244896,489.78432158119642,{"$f":"F399-10*LOG((T399/1000*H$8+(1-T399/1000)*D$8)+290*(10^(0.1*M$8)/X399-1))+10*LOG(1/X399)","v":-3.713834057949382},{"$f":"10*LOG(10^(F399/10)*5E-22/X399/1.380649E-23/2500/(T399/1000*H$8+(1-T399/1000)*D$8+290*(10^(M$8/10)/X399-1)))","v":-22.104366928091899},25.2,13.9,18.600000000000001,54.6,66.99864191942055,3.7,"Dipole","No",null,37.237357549857535,231.7,229.78988603988603,37.237357549857535,0.96827586206896554]
["*M2 18XXX",11.026384999999999,17.12,4.2699999999999996,3.96,22.69,7.4358974358974734,494.82602564102569,-4.6107214940932701,-23.001254364235795,23.1,16.399999999999999,19.600000000000001,199.7,{"$f":"(1-((P400-1)/(P400+1))^2)*10^2","v":99.885644939205122},1.07,"T Match","Yes",null,38.628205128205124,232.38,230.9025641025641,38.628205128205124,0.97499999999999998]
["M2 18XXX",11.026384999999999,17.12,4.5599999999999996,4.3600000000000003,23.05,7.4358974358974734,489.06089743589746,-4.2050328598329338,-22.595565729975455,23.1,16.399999999999999,19.600000000000001,199.7,99.885644939205122,1.07,"T Match","Yes",null,37.5,231.5,230,37.5,0.97499999999999998]
["YU7EF EF0216",11.276038999999999,17.3,4.46,4.2699999999999996,23.1,{"$f":"290*(1/X402-1)","v":7.4885037141846151},406.41944198797302,-3.4403643723739918,-21.830897242516514,22.1,18.399999999999999,24.3,43.9,81.632653061224488,2.5,"Dipole","No",null,21.317209055535891,218.89000000000001,217.05376724442871,21.317209055535891,0.97482758620689658]
["+*Dual PA144-16-12",11.276038999999999,17.46,4.9000000000000004,4.8,23.47,8.7248250630483675,379.86125368521994,-2.7978401563375654,-21.188373026480086,29.18,15.5,24.2,48.91,99.017936855774693,1.22,"Hair Pin","Yes",null,15.877970376158821,214.95999999999998,212.70237630092706,15.877970376158821,0.97079310344827585]
["+Dual PA144-16-12",11.276038999999999,17.46,4.62,4.46,23.35,8.7248250630483675,386.83570578623954,-2.9867351666853685,-21.377268036827889,29.18,15.5,24.2,48.91,99.017936855774693,1.22,"Hair Pin","Yes",null,17.242833801015891,216.02,213.79426704081271,17.242833801015891,0.97079310344827585]
["+PY1MHZ 18",11.42,17.350000000000001,4.7320000000000002,4.5209999999999999,23.29,7.4664068109549468,411.06809431095496,-3.2940821878684341,-21.684615058010959,27.03,14.88,25.95,50.27,96.253902185223723,1.48,"Folded Dipole","Yes",null,22.231249999999999,213.51,217.785,22.231249999999996,0.97489999999999999]
["InnoV 16 OWL G/T",11.484083999999999,17.43,4.59,4.41,23.3,9.8858935957780876,369.52567839823121,-2.8490746107997564,-21.239607480942276,26.82,17.2,25.7,49.49,96.127481814809428,1.49,"Folded Dipole","Yes",null,13.628137926116075,213.51,210.90251034089286,13.628137926116075,0.96703448275862069]
["InnoV 17 OWL G/T",11.733737999999999,17.71,4.7699999999999996,4.59,23.59,8.0367141540860576,418.12207633425476,-3.0518379225622798,-21.442370792704804,27.24,17.5,22,50.22,99.386268555288922,1.17,"Folded Dipole","Yes",null,23.50007087674534,220.72,218.80005670139627,23.50007087674534,0.9730344827586207]
["*InnoV 17 OWL G/T",11.733737999999999,17.71,4.9000000000000004,4.6500000000000004,23.63,8.0367141540860576,419.43497944574403,-3.023842891512599,-21.414375761655119,27.24,17.5,22,50.22,99.386268555288922,1.17,"Folded Dipole","Yes",null,23.756999078602341,220.92000000000002,219.00559926288187,23.756999078602341,0.9730344827586207]
["G0KSC 17 LFA",11.796151499999999,17.579999999999998,4.63,4.43,23.44,5.8975441559354973,367.62938040954191,-2.7401439049846537,-21.130676775127174,30.8,17.600000000000001,26.1,48.3,98.936234390395953,1.23,"LFA Loop","Yes",null,14.037541341214563,212.8,211.23003307297165,14.037541341214563,0.98006896551724143]
["*G0KSC 17 LFA",11.796151499999999,17.57,4.7,4.47,23.46,5.8975441559354973,367.62938040954191,-2.7201439049846541,-21.110676775127178,30.8,17.600000000000001,26.1,48.3,98.936234390395953,1.23,"LFA Loop","Yes",null,14.037541341214563,212.8,211.23003307297165,14.037541341214563,0.98006896551724143]
["InnoV 17 LFA",11.8377605,17.489999999999998,4.59,4.3899999999999997,23.35,8.322159554467742,359.0318452697669,-2.7103910597223835,-21.100923929864905,32,17.600000000000001,28.6,50,98.676482105098287,1.26,"LFA Loop","Yes",null,11.880564719236624,211.75,209.5044517753893,11.880564719236624,0.97210344827586204]
["*M2 19XXX",11.879369499999999,17.46,4.2699999999999996,4.04,22.98,6.5548855742445022,514.33216968158251,-4.4834558608056554,-22.873988730948174,24.5,15.07,15.29,201.1,96.987910661840033,1.42,"T match","Yes",null,42.617863817482977,235.32999999999998,234.09429105398638,42.617863817482977,0.97789655172413792]
["M2 19XXX",11.879369499999999,17.46,4.7,4.5199999999999996,23.36,6.5548855742445022,485.5919108572233,-3.8788589570718521,-22.26939182721437,24.5,15.07,15.29,201.1,96.987910661840033,1.42,"T match","Yes",null,36.993547022109361,230.92999999999998,229.59483761768749,36.993547022109361,0.97789655172413792]
["YU7EF EF0217XM",11.93970255,17.54,4.6239999999999997,4.423,23.37,8.0557268519503005,381.7029507871365,-2.9246269736510482,-21.315159843793566,29.28,21.82,23.37,50.35,99.852071005917168,1.08,"Dipole","Yes",null,16.369319752482632,215.17400000000001,213.09545580198611,16.369319752482632,0.9729724137931034]
["#M2 32 XPOL H",11.941782999999999,17.940000000000001,5.08,5.08,23.91,13.950269254400256,492.40333495970225,-3.2872012616280912,-21.677734131770606,23.2,13.4,18.3,205.47,67.522256908313111,3.65,"T Match","Yes","XPOL",36.879269218258699,232.28,229.50341537460696,36.879269218258699,0.95410344827586202]
["#M2 32 XPOL V",11.941782999999999,17.940000000000001,5.08,5.08,23.91,13.950269254400256,466.22679713759089,-3.0753048513455639,-21.465837721488082,23.2,13.4,18.3,205.49799999999999,67.522256908313111,3.65,"T Match","Yes","XPOL",31.756659076945333,228.37,225.40532726155627,31.756659076945333,0.95410344827586202]
["*M2 32 XPOL H",11.941782999999999,17.940000000000001,5,5,23.87,13.950269254400256,494.94734630814287,-3.3472540914231814,-21.737786961565703,23.2,13.4,18.3,205.49799999999999,67.522256908313111,3.65,"T Match","Yes","XPOL",37.377118797209903,232.66000000000003,229.90169503776792,37.377118797209903,0.95410344827586202]
["*M2 32 XPOL V",11.941782999999999,17.940000000000001,5,5,23.87,13.950269254400256,469.3733374896093,-3.1413292514621247,-21.531862121604647,23.2,13.4,18.3,205.49799999999999,67.522256908313111,3.65,"T Match","Yes","XPOL",32.372420398279651,228.83999999999997,225.89793631862372,32.372420398279651,0.95410344827586202]
["YU7EF EF0217X",11.941782999999999,17.510000000000002,4.59,4.3899999999999997,23.34,8.6505681818181692,386.75088778409082,-2.9968463419457922,-21.387379212088309,29.2,20,22,50,99.852071005917168,1.08,"Dipole","No",null,17.240767045454533,216,213.79261363636363,17.240767045454533,0.9710344827586207]
["*YU7EF EF0217X",11.941782999999999,17.510000000000002,4.5,4.3499999999999996,23.3,8.7566607460035701,385.36798401420947,-3.0219234385844365,-21.412456308726959,29.2,20,22,50,99.852071005917168,1.08,"Dipole","No",null,16.949378330372973,215.79999999999998,213.55950266429838,16.949378330372973,0.97068965517241379]
["RU1AA 17",11.9625875,17.79,4.8099999999999996,5,23.7,8.3327421071301977,476.31717807733224,-3.4406037381862395,-21.831136608328762,25.9,14.7,16.7,50,99.852071005917168,1.08,"Dipole","No",null,34.830613692798842,229.6,227.86449095423907,34.830613692798842,0.97206896551724142]
["+G0KSC 17 OWL G/T",12.004196499999999,17.77,5.15,5,23.82,11.131480951016906,418.01989490833557,-2.7813777554065346,-21.171910625549053,26.33,15.7,22.4,53.03,97.222222222222214,1.4,"Folded Dipole","Yes",null,22.874445001432235,220.95,218.29955600114579,22.874445001432235,0.96303448275862069]
["+G0KSC 17 OWL G/T",12.004196499999999,17.77,5,4.9000000000000004,23.77,11.131480951016906,421.20358153108003,-2.8604023823687648,-21.25093525251129,26.33,15.7,22.42,53,97.222222222222214,1.4,"Folded Dipole","Yes",null,23.497475651675757,221.43,218.79798052134061,23.497475651675757,0.96303448275862069]
["+G0KSC 17 OWL G/T H",12.004196499999999,17.77,5.08,5.08,23.79,11.14226375908618,446.80114226375917,-3.0668366100134707,-21.457369480155993,24.93,15.5,21.8,57.68,97.45074500388391,1.38,"Folded Dipole","Yes","XPOL",28.504672897196279,225.29,222.80373831775702,28.504672897196279,0.96299999999999997]
["+G0KSC 17 OWL G/T V",12.004196499999999,17.77,5.08,5.08,23.76,11.131480951016906,455.09657870237771,-3.1679348299787691,-21.558467700121291,24.93,15.5,21.83,50.16,95.480190960381918,1.54,"Folded Dipole","Yes","XPOL",30.130156115726194,226.54000000000002,224.10412489258096,30.130156115726194,0.96303448275862069]
["DK7ZB 17",12.108219,17.760000000000002,5.01,4.8499999999999996,23.74,8.8628287135750021,464.29317697228134,-3.2945485596418447,-21.685081429784368,24.8,12.7,17.7,26.8,99.247305102062086,1.19,"Dipole","No",null,32.373845060412201,227.79999999999998,225.89907604832976,32.373845060412201,0.97034482758620688]
["YU7EF EF0217M",12.233046,17.36,4.5199999999999996,4.33,23.15,7.3833097595473802,427.50490629420085,-3.5853386208989049,-21.975871491041428,25.61,17.25,21.58,49.12,99.961553248750477,1.04,"Dipole","No",null,25.464108910891099,222.1,220.37128712871288,25.464108910891099,0.97517241379310349]
["BVO-6WL",12.482699999999999,17.8,4.93,4.7699999999999996,23.7,7.1731448763250754,461.64562720848073,-3.3343592067953325,-21.724892076937856,24.9,14.3,18.2,44.9,99.572015023146136,1.1399999999999999,"Dipole","No",null,32.186395759717357,227.3,225.74911660777389,32.186395759717357,0.97586206896551719]
["+G0KSC 18 LFA",12.732353999999999,17.82,4.7699999999999996,4.5599999999999996,23.7,6.1893357751637872,354.96450394449539,-2.3445568853717358,-20.735089755514252,30.8,17.7,25.4,47.9,97.994068780047527,1.33,"LFA Loop","Yes",null,11.501989857012056,210.89000000000001,209.20159188560964,11.501989857012056,0.97910344827586204]
["*G0KSC 18 LFA",12.732353999999999,17.82,4.7699999999999996,4.5999999999999996,23.7,6.1893357751637872,354.96450394449539,-2.3445568853717358,-20.735089755514252,30.8,17.7,25.4,47.9,97.994068780047527,1.33,"LFA Loop","Yes",null,11.501989857012056,210.89000000000001,209.20159188560964,11.501989857012056,0.97910344827586204]
["InnoV 18 LFA",12.773962999999998,17.8,4.7300000000000004,4.5599999999999996,23.66,8.9371911989478843,353.25353232858242,-2.3318208762937576,-20.722353746436283,32.700000000000003,17.600000000000001,25.3,48.7,97.781801720235393,1.35,"LFA Loop","Yes",null,10.629420964703442,210.94000000000003,208.50353677176275,10.629420964703442,0.97010344827586203]
["AF9Y 22",12.773962999999998,17.920000000000002,5.01,4.8499999999999996,23.8,13.71975442397979,419.68206031058128,-2.7838316020320866,-21.174364472174609,24.9,12.2,18,49.9,79.564646275098511,2.65,"Folded Dipole","Yes",null,22.693210545323197,221.39999999999998,218.15456843625856,22.693210545323197,0.95482758620689656]
["+RA3AQ 18",13.065225999999999,18.239999999999998,5.13,4.97,24.16,8.2269503546099401,435.62615248226962,-2.6367724930062182,-21.027305363148741,26.9,15.2,19.600000000000001,54.9,99.627498953029601,1.1299999999999999,"Dipole","No",null,26.888297872340452,223.4,221.51063829787236,26.888297872340452,0.97241379310344822]
["*RA3AQ 18",13.065225999999999,18.239999999999998,5.3,5.3,24.27,8.3327421071301977,428.34861653068475,-2.4606704732171876,-20.851203343359714,26.9,15.2,19.600000000000001,54.9,99.627498953029601,1.1299999999999999,"Dipole","No",null,25.443419652359012,222.3,220.35473572188721,25.443419652359012,0.97206896551724142]
["MBI 6.6",13.689361,18.329999999999998,5.5,5.36,24.35,12.713987473903995,440.66531837160761,-2.4335721492246147,-20.824105019367138,27.5,12.21,18.46,47,91.982374327154076,1.79,"Folded Dipole","Yes",null,26.996346555323605,224.47,221.59707724425888,{"$f":"(V435-200)*1.25","v":26.996346555323605},0.95799999999999996]
["DK7ZB 19",13.710165499999999,18.3,5.41,5.22,24.3,8.4386089425124062,480.22622427253378,-2.870986048545956,-21.261518918688477,24,13.4,17.899999999999999,27.7,89.333287986486638,1.97,"Dipole","No",null,35.574875798438619,230.20000000000002,228.4599006387509,35.574875798438619,0.97172413793103452]
["InnoV 19 LFA",13.772579,18.010000000000002,4.84,4.7,23.88,9.554764024933224,341.97504452359755,-1.9828664384577748,-20.373399308600298,32.5,17.5,26.9,48.3,95.347943098808159,1.55,"LFA Loop","Yes",null,8.3014247551202303,209.3,206.64113980409618,8.3014247551202303,0.96810344827586203]
["*InnoV 19 LFA",13.772579,18.010000000000002,4.84,4.75,23.89,9.554764024933224,341.31524933214615,-1.9656688267902018,-20.356201696932715,32.5,17.5,26.9,48.3,95.347943098808159,1.55,"LFA Loop","Yes",null,8.1723063223508774,209.20000000000002,206.5378450578807,8.1723063223508774,0.96810344827586203]
["#BQH 25",15.187284999999999,18.53,5.27,5.09,24.43,9.0753911806543446,393.7294185633001,-1.9693192379487658,-20.359852108091285,25.5,15.2,20.8,27.9,99.451303155006855,1.1599999999999999,"Dipole","No",null,18.523293029871972,217.1,214.81863442389758,18.523293029871972,0.96965517241379307]
["InnoV 21 LFA",15.707397499999999,18.38,5.04,4.88,24.23,9.8645083077800955,334.33687513370893,-1.5449638493368099,-19.935496719479332,32.5,19,26.6,49,93.27846364883402,1.7,"LFA Loop","Yes",null,6.7460600442130669,208.17999999999998,205.39684803537045,6.7460600442130669,0.96710344827586203]
["K2GAL 21",15.915442499999999,19.05,5.71,5.55,24.96,13.939284423563461,436.30619804842786,-1.7698581089950083,-20.160390979137532,26.3,15.7,19.100000000000001,17.2,35.968027976019989,9.01,"Dipole","No",null,25.903505601734729,223.9,220.72280448138778,25.903505601734729,0.95413793103448274]
["M2 8WL(old)",16.061073999999998,18.649999999999999,5.31,5.13,24.48,8.7142146764225075,426.45060204589055,-2.22872394618377,-20.619256816326295,21.3,16.3,19.100000000000001,201.5,86.818937887946774,2.14,"T Match","Yes",null,24.997336080130736,222.04000000000002,219.99786886410459,24.997336080130736,0.97082758620689658]
["+InnoV 22 LFA",16.6644045,18.809999999999999,5.31,5.13,24.68,6.8060702311628845,329.99131374625028,-1.0844492055470971,-19.474982075689621,31.7,17.2,25.6,49.7,99.173553719008268,1.2,"LFA Loop","Yes",null,6.4941768131286537,207.14000000000001,205.19534145050292,6.4941768131286537,0.97706896551724143]
["*+InnoV 22 LFA",16.6644045,18.809999999999999,5.4,5.25,24.72,6.8060702311628845,331.95253661549339,-1.0664627723218187,-19.456995642464339,31.7,17.2,25.6,49.7,99.173553719008268,1.2,"LFA Loop","Yes",null,6.8779777660137853,207.44000000000003,205.50238221281103,6.8779777660137853,0.97706896551724143]
["M2 8WLHLD",16.747622500000002,19.14,6.05,5.87,25.11,13.610108303249097,508.67883574007232,-2.2182915281072821,-20.608824398249801,25.4,13.2,19.399999999999999,200,59.252670784705487,4.53,"T Match","Yes",null,40.130866425992799,234.70000000000002,232.10469314079424,40.130866425992799,0.95517241379310347]
["+G0KSC 22 LFA 3R",16.997276499999998,18.489999999999998,6.1,5.9,24.56,7.7201925800056177,340.51608078448027,-1.3098293152792693,-19.700362185421792,29.7,20.7,29.6,46.3,99.451303155006855,1.1599999999999999,"LFA Loop","Yes",null,8.3749291985273189,208.86,206.69994335882186,8.3749291985273189,0.97406896551724143]
["+G0KSC 22 LFA 3R",16.997276499999998,18.489999999999998,5.9,5.7,24.55,7.7201925800056177,334.74544215519666,-1.2561800283408353,-19.646712898483358,29.65,20.7,29.6,46.3,99.451303155006855,1.1599999999999999,"LFA Loop","Yes",null,7.2456457094307325,207.98,205.79651656754459,7.2456457094307325,0.97406896551724143]
["+InnoV 24 LFA",18.557613999999997,19.29,5.6539999999999999,5.5010000000000003,25.17,7.0996573285760078,332.23575882290606,-0.61595796437259853,-19.006490834515116,33.1,16,22.4,48.1,96,1.5,"LFA Loop","Yes",null,6.8759494118062747,207.52,205.50075952944502,6.8759494118062747,0.97610344827586204]
["+*InnoV 24 LFA",18.557613999999997,19.29,7,7,25.36,7.0996573285760078,341.20086904299291,-0.52510352803514682,-18.915636398177668,33.08,16,22.4,48.12,96,1.5,"LFA Loop","Yes",null,8.6303741124103439,208.89,206.90429928992828,8.6303741124103439,0.97610344827586204]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(U459-G459)/(1-G459/290)","v":0},-250,1]
["Only Antennas that have actually been built are posted in these Tables, except for the F5FOD Isotropic Lossless Radiator."]
[]
["Thanks to Vladimir, UR5EAZ for establishing the Interactive Mode in the 144 and 432 Tables"]
["Thanks to Hartmut,  DG7YBN for his ongoing support and many inputs to the Tables"]
[]
["Legend:"]
[]
["1. L       = Length in Wavelengths"]
[]
["2. Gain  = Gain in dBd of a single antenna"]
[]
["3. E      = E plane (Horizontal) stacking in Meters. "]
[]
["4. H      = H plane (Vertical) stacking in Meters."]
[]
["5. Ga     = Gain in dBd of a 4 bay array"]
[]
["6. Tloss = Noise temperature due to ohmic losses in the antenna (K) at an actual antenna temperature of 290 K."]
[]
["7. Ta     = Noise temperature of the antenna array (K) is the mixture of the antenna array pattern, the sky temperature, "]
["               ground and the ohmic losses in the antenna array."]
[]
["8. F/R    = Front to Rear in dB over the rear 180 degrees of an antenna using either E or H plane. "]
[]
["9. Z ohms = The natural impedence of a single antenna in free space.  "]
[]
["10. VSWR  = VSWR Bandwidth is based a single antenna over 144.000 - 145.000 MHz with a "]
["                    reference at 144.100 MHz. This parameter gives an indicator of the"]
["                    antenna \"Q\" and what to expect with with stacking and wet weather.  "]
[" "]
["11. G/T = Figure of merit; a system parameter used to determine the receive capability of the antenna or array"]
["               as part of the radio receiving system. The more positive level the better."]
[]
["12. S/N = Figure of merit: a system parameter used to determine the receive capability of the antenna or array"]
["                as part of the radio receiving system.The more positive level the better."]
[]
["13. e   = Radiation Efficiency; a system parameter which describes how efficiently an antenna transmits and receives signals."]
[]
["   Notes:"]
["        "]
["1. The programs used to calculate E/H Stacking,G,Ta,Tlos and Ant G/T are"]
["    EZNEC Pro+ V.7.0 by Roy Lewallen W7EL,4NEC2 by Arie Voors and Tant.exe by Sinisa, YT1NT/VE3EA (DOS) or AGTC_lite by F5FOD/DG7YBN (Windows)"]
["    This combination of software provides excellent accuracy."]
[]
["2. Temperatures initially used for producing Antenna Temperature: Tsky=200 Kelvin;Tearth=1000 Kelvin"]
["    Temperatures now adjustable to Tsky=290 Kelvin. Tearth: Rural = 1600 Kelvin, Residential = 5400 Kelvin, City = 14,500 Kelvin"]
[]
["3. Dipole Z is measured at 144.1 MHz"]
[]
["4. F/R, 1st and 2nd Side Lobes (SL) have been calculated on a single antenna"]
[]
["5. No stacking harness losses or H frame effects are included in the 4 bay gain figures."]
[]
["6. All stacking dimensions EXCEPT those marked with a \"*\" and \"#\" are"]
["    calculated from the DL6WU stacking formula:"]
["    D = W/(2* sin(B/2))"]
["    Where:"]
["    D = stacking distance,vertical or horizontal"]
["    W = wavelength, in the same units as D"]
["    B - beamwidth between -3dB points."]
["    Use vertical beamwidth for vertical stacking (as above),"]
["    Use horizontal beamwidth for horizontal stacking."]
[]
["7. Antennas marked with a \"*\" have stacking dimensions recommended by "]
["   the manufacturer or designer."]
[]
["8. Antennas marked with a \"#\" have stacking dimensions for XPOL"]
["   antennas by VE7BQH."]
[]
["9. Antennas marked with a \"+\" have some or all elements over 6mm. All others"]
["   are 4MM to 6MM."]
[]
["10. FD = Folded Dipole"]
[]
["11. XPOL Antennas: Any offset of elements or feedsystems from the zero axis results in degredation in pattern. "]
["      This affects VSWR, Antenna Temp and G/T. To show the exact amount of degradation two separate rows "]
["      are given for the vertical polarized plane an the horizontally polarized plane"]
[]
["12.  Convergence Correction: NEC2 and NEC 4 are incapable of handling complex "]
["      feed systems accurately like Folded Dipoles, T Matches, LFAs etc."]
["      Convergence Correction using the KF2YN Excel program is required. "]
["      See DUBUS 4/2010 \"The Correction of Convergence Errors in Antenna "]
["      Temperature Calculations by Brian Cake, KF2YN for details."]
[]
["13. Earth Temperature Definition"]
["       Rural: Open countryside with largely agricultural activity, building density < 1/ha, no major roads, no electrified railways."]
["       Residential: Villages and pure residential areas with no commercial or industrial activities. No electrified railways and no major roads and no high voltage overhead lines or facilities within 1 km."]
["       City: Dense commercial or industrial buildings and offices. Major roads and railways can be in the vicinity, but should not be dominating."]
[]
["14. Manufacturer/Designer Legend: Single Click on Sites with Links in blue."]
[]
["    7Arrays = 7Arrays"]
["   AF9Y = AF9Y"]
["    Antennas-Amplifiers=Antennas-Amplifiers"]
["    Ant-Amp=Antennas-Amplifiers",null,null,"K1FO = K1FO"]
["    BVO = Eagle/DJ9BV",null,null,"K2GAL = K2GAL"]
["   BQH = VE7BQH",null,null,"K5GW = Texas Towers/K5GW"]
["   CC = Cushcraft",null,null,"KF2YN = KF2YN"]
["   CC MOD = VE7BQH",null,null,"M2inc = M2inc"]
["   CD = CUE DEE ",null,null,"MBI = F/G8MBI/F5VHX"]
["   CD MOD = VE7BQH",null,null,"OZ5HF = Vargarda"]
["   CT1FFU = CT1FFU",null,null,"RA3AQ = RA3AQ"]
["   DD0VF = DD0VF",null,null,"RA3RF ="]
["   DG7YBN = DG7YBN",null,null,"RU1AA = RU1AA","R3RAV"]
["   DJ9BV = DJ9BV",null,null,"SHARK = SHARK (Italian)"]
["   DJ9BV OPT = DJ9BV",null,null,"SM2CEW = SM2CEW/VE7BQH"]
["   DK7ZB = DK7ZB",null,null,"SV = Svenska Antennspecialisten AB"]
["   Dual = Antennas-Amplifiers",null,null,"UR5CSZ = UR5CSZ"]
["   EAntenna = EAntenna",null,null,"UR5CSZ = UR5CSZ"]
["   EKM MOD = SM2EKM",null,null,"Vine = G0KSC Design"]
["   F9FT = F9FT",null,null,"WB9UWA = WB9UWA"]
["   Flexa = FlexaYagi",null,null,"YU7EF = YU7EF"]
["   G0KSC LFA = G0KSC",null,null,"YU7XL = YU7XL"]
["   G4CQM = G4CQM",null,null,"W1JR = VE7BQH (Mininec error)"]
["   HG = HYGAIN",null,null,"WB9UWA = WB9UWA"]
["   I0JXX = I0JXX"]
["   IK0BZY = IK0BZY"]
["   InnoVAntennas = G0KSC"]
["   WiMo = WiMo"]
[]
[]
["Using this Chart:"]
[]
["Programmable Tsky and Tearth: Tsky and Tearth may be changed to meet a Stations individual characteristics."]
["                                                    Click on the Red number to change then click on the green to set."]
[]
["Antennas with good G/T can provide significant benefit with today's high noise levels. "]
["Other factors like ease of matching and wet weather performance should be considered in the the decision making. "]
["Antennas with 50 ohm feed systems and good VSWR bandwidth (Q) may be the best feed system choice. "]
[]
[null,null,null,null,"Lionel H. Edwards"]
[null,null,null,null,"VE7BQH"]
[null,null,null,null,"Issue 124, July 2, 2024"]
["       "]
[]
[null,"     "]
["Issue 51: Add YU7EF Antennas"]
["Issue 52: Update all DK7ZB antennas to latest published data. Add DK7ZB 8"]
["Issue 53: Replace BQH8A with BQH8B a 50 ohm antenna"]
["Issue 54: Add YU7EF 8"]
["Issue 55: Add YU7EF 17 & YU7EF 11B"]
["Issue 56: Add YU7EF 16"]
["Issue 57: Add a revised YU7EF 10"]
["Issue 58: Add DK7ZB 19"]
["Issue 59: Add YU7EF 10LT"]
["Issue 60: Add columns of Z and VSWR bandwidth to give indicators of Q and wet weather performance."]
["Issue 61: Add UA5EAZ 9. Add VSWR bandwidth for folded dipole to RA3AQ 9. Add RA3AQ 14"]
["Issue 62: Revised Note 1 to explain limitations in YA 3.54 and the change to EZNEC 5+ and Tant.exe software"]
["Issue 63: Add new low noise wide VSWR bandwidth YU7EF 13M,14M,15M,16M series antennas"]
["Issue 64: Add YU7EF 14LT;Add G4CQM 8,9,11,16;Add G0KSC 9LFA"]
["Issue 65: Add G0KSC 11LFA,G0KSC 14LFA;Add DK7ZB 7;Add K1FO 10,11,16"]
["Issue 66: Conversion to EZNEC 5+ & Tant.exe completed. Add G0KSC 8LFA, G0KSC 12LFA,G0KSC 13LFA: RA3AQ 9S"]
["Issue 67: Data corrected for RA3AQ 9S;"]
["Issue 68: G4CQM 8 updated to new version,Add ZL1RS 9, "]
["Issue 69: Add G0KSC 15LFA,G0KSC 17LFA. Segment Density changed to improve impedence accuracy. "]
["Issue 70: Add G0KSC 7LFA, Add Front to Rear column (F/R)"]
["Issue 71: Add G0KSC 9,G4CQM 7,G4CQM 6,8 & 9 updated versions, "]
["Issue 72: Add G0KSC 10LFA,Revised G4CQM 11,"]
["Issue 73: Add G0KSC 9,G0KSC 11"]
["Issue 74: Add G0KSC 6LFA,G0KSC 8OWL,Revised G0KSC 9OWL,G0KSC 10OWL,"]
["Issue 75: Add CT1FFU 7,CT1FFU 8,CT1FFU 9,CT1FFU 10,CT1FFU 10C"]
["Issue 76: Add G0KSC 16LFA, I5MZY 11, I5MZY 13, G0KSC 11LFA 3R, G0KSC 14LFA 3R, G0KSC 16LFA 3R,"]
["Issue 77: Add G4CQM 16 Revised,KF2YN Boxkite6, KF2YN Boxkite9,KF2YN Boxkite12,G0KSC 12OWA,G0KSC 17OWA"]
["Issue 78: Add DD0VF 9,G0KSC 12LFA 2R,UA9TC 11RS,UA9TC 12RS, UA9TC 14RS"]
["Issue 79: Add Vine 6 FD,Vine 7 FD,Vine 8 FD,Vine 9 FD,Vine 10 FD,Vine 11 FD,G0KSC 12 LFA,G0KSC 22 LFA 3R,G0KSC 16 OWL FD"]
["Issue 80: Add Revised G0KSC 15 LFA,Revised G0KSC 16 LFA,"]
["Issue 81: Add G0KSC 10 LFA,Revised G0KSC 11 LFA,Revised G0KSC 13 LFA,Revised G0KSC 14 LFA,Revised G0KSC 17 LFA, "]
["Issue 81: Add G0KSC 18 LFA,Revised G0KSC 14 LFA 3R,Revised IK0BZY 12,DG7YBN 16,"]
["Issue 82: Add KF2YN Boxkite4,KF2YN Boxkite7, YU7EF 17X,Corrected DG7YBN 16, "]
["Issue 83: Add Revised DK7ZB 11,Add KF2YN Boxkite 10,KF2YN Boxkite 13,KF2YN Boxkite 16  "]
["Issue 84: Add M2 2M7,DG7YBN 12"]
["Issue 85: Add G4CQM CQM12UC,"]
["Issue 86: Add WiMo WX220,InnoV 22 LFA,InnoV 21 LFA,InnoV 19 LFA,InnoV 18 LFA,InnoV 17 LFA,InnoV 16 LFA,InnoV 15 LFA,"]
["Issue 86: Add InnoV 14 LFA,InnoV 13 LFA,InnoV 12 LFA,"]
["Issue 87: Add SM2CEW 14 XPOL,KF2YN Boxkite 9,10,12.13,16 updated,Add DL6WU 14,Add G4CQM 12UX,Add DG7YBN 8"]
["Issue 88: Add YU7XL 8 Hybrid,YU7XL 11 Hybrid,UA9TC 13RS,"]
["Issue 89: Add YU7XL 17 Twin Boom,RU1AA 15_2,RU1AA 17,G4CQM 10 UZ2,"]
["Issue 90: Add KLM 16LBX,DD0VF6,InnoV 15 OWL,"]
["Issue 91: Add DG7YBN 7, "]
["Issue 92: Revised the stock CC4218XL,Removed the modified CC4318XL,Revised G4CQM 8,"]
["Issue 93: Add I4GBZ 7,UR5EAZ 12,Gulf Alpha 9,Gulf Alpha 11,Gulf Alpha 14,"]
["Issue 94: Add InnoV 9 XPOL, G4CQM 9 UZ22, I0JXX 8 XPOL,DK7ZB 10 revised, BQH13X,DK7ZB 11 OWL,DG7YBN 12 Ver2,"]
["Issue 94: Add DK7ZB 12,DG7YBN 12 Ver3,DK7ZB 14 OWL,"]
["Issue 95: Add InnoV 11 LFA-FD,InnoV 12 LFA-FD,InnoV 13 LFA-FD,InnoV 14 LFA-FD,InnoV 7 FD,InnoV 8 FD,InnoV 10 FD,"]
["Issue 95: Add InnoV 12 FD,InnoV 13 FD,EAntenna 144LFA4,EAntenna 144LFA5,EAntenna 144LFA7,EAntenna 144LFA8,"]
["Issue 95: Add EAntenna 144LFA9,EAntenna 144LFA11,Eantenna 144LFA13,EAntenna 144LFA16,Eantenna 144LFA16 XPOL,"]
["Issue 96: Add WiMo WY209,revised InnoV 22 LFA,InnoV 24 LFA,revised InnoV 15 OWL,InnoV 16 OWL,InnoV 17 OWL,"]
["Issue 97: Add InnoV 14 OWL G/T v2,InnoV 13 OWL G/T v2,InnoV 12 OWL G/T-2,InnoV 14 OWL G/T-2Q,InnoV 11 OWL G/T-2,"]
["Issue 97: Add InnoV 13 OWL G/T-2,InnoV 15 OWL G/T-2,InnoV 10 OWL G/T-2,G4CQM WA9C4X,G4CQM WA9UXO,"]
["Issue 97: Add G4CQM WA20675,G4CQM WA 27116, G4CQM WAX8,G4CQM WAXXX10,"]
["Issue 98: Add Directive DSEFO144-12,Directive DSEFO144-12 XPOL,Directive DSEFO144-15,Directive DSEFO144-19,"]
["Issue 99: Add DG7YBN GTV-10LT,Antennas-Amp PA144-14-9,Antennas-Amp PA144-16-12,Antennas-Amp PA144-12-7,Antennas-Amp PA144-13-8,"]
["Issue 100: Add InnoV 14LFA Ver 3,DK7ZB 13,M2 2MXP22A,"]
["Issue 101: Add YU7XL X21205XL6QQ.EZ,"]
["Issue 102: Add DG7YBN GTV2-9n,"]
["Issue 103: Add  7Arrays GTV 2-9n XPOL,I5MZY 5,I5MZY 9, Programmable Tsky and T earth,"]
["Issue 104: Add  7Arrays GTV2-11LT,"]
["Issue 105: Add DG7YBN GTV2-8w,"]
["Issue 106: Add R3RAV 9,"]
["Issue 107: Add DG7YBN GTV2-6m,G4CQM CQM14DXL,"]
["Issue 108: Tearth Kelvin updated,"]
["Issue 109: Tearth Kelvin updated,"]
["Issue 110: Add Cushcraft 9 LFA,Cushcraft 12 LFA,Cushcraft 14 LFA,Cushcraft 16 LFA,"]
["Issue 111: Add Antennas-Amplifiers PA144-14-9BGP"]
["Issue 112: Add InnoV/G0KSC 13 LFA3 2019,InnoV/G0KSC 12 LFA3 2019,InnoV/G0KSC 11 LFA3 2019,InnoV/G0KSC 10 LFA3 2019,"]
["Issue 112: Add InnoV/G0KSC 9 LFA3 2019,InnoV/G0KSC 9 OWL 2020,InnoV/G0KSC 8LFA,2019InnoV/G0KSC 7 LFA3 2019,"]
["Issue 112: Add InnoV/G0KSC 14 LFA3 2019,"]
["Issue 113: Add YU7EF 17XM,Ant-Amp PA144-XPOL-18-5AP,Antennas-Amplifiers PA144-XPOL-9-4.3AP,Antennas-Amplifiers PA144-10-6AGP,"]
["Issue 114: Add YU7XL X22205XL2Q"]
["Issue 115: Add IZ7NLJ 11,I5MZY 13 Rev2,PY1MHZ 14A,PY1MHZ 11,PY1MHZ 12,PY1MHZ 8,PY1MHZ 7,PY1MHZ 13,PY1MHZ 14B,PY1MHZ 15"]
["Issue 116: Add InnoV 9 2022,YU7EF EF0209V,YU7EF EF0211AV,"]
["Issue 117: Add Receive System NF Thanks to Vladimir UR5EAZ"]
["Issue 118: Add PY1MHZ 8,PY1MHZ 9,PY1MHZ 10,PY1MHZ 11,PY1MHZ 12,PY1MHZ12,PY1MHZ 14,PY1MHZ 16,PY1MHZ 17,PY1MHz 18,DG7YBN GTV2 9M LT,DG7YBN YBN 2-7mz,",null,null,null,null,null,null,null,null,null,null,null,null,"DG7YBN 2-7mz,"]
["Issue 119: Charts for all 3 bands have been revised to be more readable.Thanks to Hartmut,DG7YBN"]
["Issue 120: Add I0JXX 4, EA1DDO 6 Quad,EA1DDO 8 Quad,"]
["Issue 121: Add WB9UWA 13,"]
["Issue 122: Add Signal to Noise (S/N)"]
["Issue 123: Add EA1DDO Circular 8, 4Y3i 12"]
["Issue 124: Add Radiation Efficiency. Thanks to Vladimir UR5EAZ"]

{"sheet":"50.15 MHz Table","index":2,"n_rows":414,"n_cols":30,"rows_kept":414,"cut":false,"hidden":false,"merged":[[9,3,9,4],[9,12,9,13],[8,1,8,2],[8,3,8,11],[8,12,8,16]]}
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"*Hairpin"]
["Issue: July 2, 2024",null,null,null,null,null,null,"VE7BQH Antenna Table"]
[]
[null,"Old Reference: Tsky=4225K Tearth=6000K",null,null,null,null,null,"Reference: Estimated Values for man-made noise (Tearth) on 50.150 MHz ITU-R P.372-16: Part 6,Man-made Noise, p.98-100",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"*Gamma"]
[null,"New Reference: Tsky=5640K",null,null,null,null,null,"Rural =",null,29700,"K",null,null,null,null,null,null,null,null,null,null,null,null,"*Beta"]
[null,null,null,null,null,null,null,"Residential =",null,100600,"K",null,null,null,null,null,null,null,null,null,null,null,null,"*KLM Dual Dip"]
[null,null,null,null,null,null,null,"City =",null,270800,"K",null,null,null,null,null,null,null,null,null,null,null,null,"Will not calculate"]
[null,null,null,"Enter Tsky >",null,5640,"K","Enter Tearth >",null,100600,null,"   Enter Receive System NF >",null,null,null,0.75,null,null,null,null,null,null,null,"accurately"]
[null,null,null,"DL6WU Optimal Stacking",null,null,null,null,null,null,null,null,"Compromise 75% Stacking",null,null,null,null,null,"            ! Ant","   1 Ant",null,null,"               ",null,null,null,"         Internal use only"]
[null,null,"1 Ant",null,null,"                  4 Antennas",null,null,null,null,"2E ant","2H ant","Spacing",null,"4 Ant","2E ant","2H ant","<","H Plane","        >",null,null,null,null,"KF2YN",null,"  archive"]
["TYPE OF","Length","GAIN","E","H","GA","TA","Tloss"," G/T","S/N","GA","GA","E","H","GA","GA","GA","F/R","1st SL","2nd SL","Z","e","VSWR ","      Feed"," Conver.",null,"Ta",null,"    New"]
["ANTENNA","m","(dBi)","(m)","(m)","(dBi)","(K)","(K)","(dB/K)","(dB)","(dBi)","(dBi)","(m)","(m)","(dBi)","(dBi)","(dBi)","(dB)","(dB)","(dB)","(ohms)","(%)","Bandwidth","    System"," Corr Req.",null,"      Old","Tpat","     \"S\""," ave gain"]
[]
["Isotropic Lossless Radiator",0,0,"-","-","-",{"$f":"Z14/9000*J$8+(1-Z14/9000)*F$8+290*(1/AD14-1)","v":53119.917722055849},{"$f":"290*(1/AD14-1)","v":7.0001689696130853E-3},{"$f":"C14-10*LOG((Z14/9000*J$8+(1-Z14/9000)*F$8)+290*(10^(0.1*P$8)/AD14-1))+10*LOG(1/AD14)","v":-47.256936234966986},{"$f":"10*LOG(10^(C14/10)*1E-20/AD14/1.380649E-23/2500/(Z14/9000*J$8+(1-Z14/9000)*F$8+290*(10^(P$8/10)/AD14-1)))","v":-52.637169148469702},"-","-","-","-","-","-","-","-","-","-","-",null,"-","-","No",4499.9915385107624,5349.8710000000001,5349.9931377653947,{"$f":"(AB14-1700)*1.232876712","v":4499.9915385107624},0.99997586206896549]
["PY1MHZ 2",0.4,6.63,5.39,3.34,13.26,17776.259083253095,{"$f":"290*(1/AD15-1)","v":1.8345322492773097},{"$f":"F15-10*LOG((Z15/9000*J$8+(1-Z15/9000)*F$8)+290*(10^(0.1*P$8)/AD15-1))+10*LOG(1/AD15)","v":-29.224436073580097},{"$f":"10*LOG(10^(F15/10)*1E-20/AD15/1.380649E-23/2500/(Z15/9000*J$8+(1-Z15/9000)*F$8+290*(10^(P$8/10)/AD15-1)))","v":-34.60466898708281},9.68,10.06,4.04,2.5099999999999998,11.83,9.16,9.1999999999999993,6.6,"none","none",50.33,{"$f":"(1-((W15-1)/(W15+1))^2)*10^2","v":98.298676748582224},1.3,"Folded Dipole","Yes",1150.061299063125,2618.1,2632.8274983777333,1150.061299063125,0.99371379310344832]
["G0KSC 2 LFA-Q",0.41845440000000006,7.49,5.17,3.7149999999999999,13.84,13929.541176938319,{"$f":"290*(1/AD16-1)","v":2.9190902441572741},-27.573052481401501,-32.953285394904206,10.34,10.67,3.9750000000000001,2.79,12.23,9.7799999999999994,9.73,9.18,"none","none",28.1,{"$f":"(1-((W16-1)/(W16+1))^2)*10^2","v":97.33723149104533},1.39,"LFA Vert Loop","Yes",785.37909414750902,2316.63,2337.0297098672986,785.37909414750902,0.99003448275862072]
["InnoV 2 LFA-Q",0.41845440000000006,6.53,5.25,3.36,13.13,19643.667395539032,{"$f":"290*(1/AD17-1)","v":1.4269873172084346},-29.793036374702265,-35.173269288204978,9.59,9.89,3.9375,2.52,11.73,9.33,9.1,6.57,"none","none",48.9,99.173553719008268,1.2,"LFA Vert Loop","Yes",1327.0868120682014,2764.24,2776.4148589645852,1327.0868120682014,0.99510344827586206]
["PY1MHZ 2 V2",0.5,6.99,5.4729999999999999,3.4980000000000002,13.64,15221.066785707228,2.6337033299697166,-28.160898114648564,-33.54113102815127,10.02,10.47,4.0999999999999996,2.63,12.08,9.43,9.5,9,"none","none",49.42,96.379222737628879,1.47,"Folded Dipole","Yes",907.81273948394391,2634.15,2436.337,907.81273948394391,0.99099999999999999]
["InnoV 2 LFA",0.83690880000000012,6.35,5.17,3.22,13,17943.101253036504,1.4269873172084346,-29.530933446707284,-34.911166360209997,9.4,9.74,3.88,2.42,11.39,8.8699999999999992,8.81,6.37,"none","none",48.5,99.247305102062086,1.19,"LFA Loop","Yes",1165.9126831452577,2634.15,2645.6847321366695,1165.9126831452577,0.99510344827586206]
["InnoV 3 OWL G/T",1.2553631999999999,7.61,5.609,3.67,14.02,13736.523387407347,2.3183872088981872,-27.341573371920301,-32.721806285423007,10.65,10.89,4.2074999999999996,2.7524999999999999,12.54,10.15,10.02,9.25,"none","none",55.02,98.936234390395953,1.23,"Dipole","Yes",767.14242840970985,2306.12,2322.2377476538059,767.14242840970985,0.99206896551724133]
["G0KSC 3el-Q",1.6738176000000002,8.66,5.8369999999999997,4.2750000000000004,14.95,10755.936719851727,1.4471860271693693,-25.36698983860212,-30.747222752104832,11.7,11.86,4.38,3.21,13.76,11.22,11.2,13.9,"none","none",48.8,99.173553719008268,1.2,"LFA Vert Loop","Yes",484.73468623021284,2084.2199999999998,2093.1736900471301,484.73468623021284,0.99503448275862072]
["Cushcraft A50-3S",1.7335967999999999,7.44,5.5620000000000003,3.613,13.99,13308.36869873306,1.3563138749350356,-27.24886957594321,-32.62910248944592,10.5,10.86,4.17,2.7075,12.73,10.02,10.16,8.7899999999999991,"none","none",37.42,99.885644939205122,1.07,"*Gamma","No",726.65450151351229,2280.09,2289.3975402736883,726.65450151351229,0.9953448275862069]
["YU7EF EF0603",1.7933760000000001,7.08,5.4290000000000003,3.4420000000000002,13.59,15774.419064271602,1.5077989601386355,-28.382114208683632,-33.762347122186348,10.130000000000001,10.45,4.07,2.58,12.34,9.67,9.76,7.61,"none","none",50.2,99.961553248750477,1.04,"Dipole","No",960.36437855732072,2467.64,2478.9622183708834,960.36437855732072,0.9948275862068966]
["PY1MHZ 3",1.8,8.4600000000000009,5.88,4.0999999999999996,14.73,11868.633797951257,2.5420898845136919,-25.996235429881843,-31.376468343384548,11.49,11.66,4.41,3.0750000000000002,13.63,11.05,11.08,13,"none","none",50.46,97.888815837533784,1.34,"Folded Dipole","Yes",590.08872549074022,2162.2159999999999,2178.6275219145678,590.08872549074022,0.99131034482758618]
["DK7ZB 3 28 ohm",1.8531552,7.89,5.6559999999999997,3.78,14.15,14020.170146869066,1.9530653336110504,-27.305396549587066,-32.685629463089768,10.92,11.07,4.2450000000000001,2.835,13.01,10.49,10.45,10.46,"none","none",27.96,99.67960128159487,1.1200000000000001,"Dipole","No",794.06016990121191,2330.33,2344.071026869402,794.06016990121191,0.99331034482758618]
["DK7ZB 3 12.5 ohm",1.8531552,8.49,5.8710000000000004,4.1059999999999999,14.66,12394.692609981925,4.0353821411090145,-26.231719046252781,-31.611951959755487,11.5,11.6,4.4000000000000004,3.08,13.55,11.07,11,13.7,"none","none",12.94,98.396292976869248,1.29,"Dipole","No",639.80533962265542,2192.48,2218.9532200545414,639.80533962265542,0.98627586206896556]
["Moxon GW3YDX",1.8531552,8.82,5.6559999999999997,4.4749999999999996,15.03,10702.82683462545,2.9190902441572741,-25.243835864299484,-30.624068777802194,11.84,11.94,4.242,3.3559999999999999,13.73,11.31,11.22,16.600000000000001,"none","none",49.97,97.888815837533784,1.34,"Bent Dipole","Yes",479.56160172105763,2071.0500000000002,2088.9777437219186,479.56160172105763,0.99003448275862072]
["InnoV 3 LFA-Q 1.91m",1.9129344000000001,9.5399999999999991,6.165,4.96,15.71,12575.491271853671,3.2152569555819044,-25.256410198395244,-30.63664311189795,12.58,12.67,4.6275000000000004,3.72,14.64,12.09,12.1,18,"none","none",27.8,97.105766085294675,1.41,"LFA Vert Loop","Yes",657.01857765462103,2211.61,2232.9150686841922,657.01857765462103,0.98903448275862071]
["G0KSC 3 1.94m LFA",1.9129344000000001,8.4700000000000006,5.8630000000000004,4.03,14.65,12065.146927142752,2.3387096774193528,-26.150233728396007,-31.530466641898713,11.44,11.59,4.4000000000000004,3.02,13.53,11.02,11,13.6,"none","none",49.35,99.51325040562466,1.1499999999999999,"LFA Loop","Yes",608.73287655000001,2178.52,2193.75,608.73287655000001,0.99199999999999999]
["EAntenna 50LFA3",1.9129344000000001,8.65,5.9420000000000002,4.1059999999999999,14.79,11477.618746964945,2.3082270341663369,-25.794886882810452,-31.175119796313165,11.6,11.81,4.46,3.08,13.53,11.07,11.2,13.98,"none","none",51.9,98.936234390395953,1.23,"LFA Loop","Yes",553.05175525881441,2133.91,2148.5864238295503,553.05175525881441,0.99210344827586205]
["M² 6M3",2.0324928,8.56,5.95,4.1900000000000004,14.81,12919.130010860437,3.2357043235704408,-26.272686194297616,-31.652919107800326,11.53,11.67,4.49,3.18,13.7,11.1,11.13,13.1,"none","none",198.18,98.852040816326536,1.24,"T Match","Yes",689.58560192535606,2237.6,2259.3305439330547,689.58560192535606,0.98896551724137927]
["DK7ZB 4 28 ohm",2.1520511999999998,9,6.1260000000000003,4.4450000000000003,15.22,11116.433003364533,2.6031591399345944,-25.222339505162417,-30.602572418665126,12.01,12.16,4.38,3.04,13.76,11.45,11.34,14.91,"none","none",28.6,99.990197039505929,1.02,"Dipole","No",518.79179231277772,2104.5100000000002,2120.7977872103547,518.79179231277772,0.99110344827586205]
["G0KSC 3 Quad",2.2716096000000001,9.33,5.71,4.9800000000000004,15.47,10832.528528945477,7.6569689247540174,-24.786554838438388,-30.166787751941094,12.36,12.41,4.28,3.74,14.32,11.82,11.85,22.86,"none","none",51.2,98.676482105098287,1.26,"Quad","No",491.40526579808869,2052.06,2098.5842712536278,491.40526579808869,0.97427586206896555]
["YU7EF EF0604S",2.3313888,8.77,6.0229999999999997,4.3099999999999996,14.97,11562.696645999886,2.7253741733379844,-25.64064366103894,-31.020876574541649,11.77,11.83,4.58,3.17,13.83,11.32,11.3,14.32,"none","none",50,99.940511600237954,1.05,"Dipole","No",561.07562601557424,2137.73,2155.0946745562132,561.07562601557424,0.99068965517241381]
["DK7ZB 3 28 ohm",2.5107263999999998,8.7799999999999994,5.9059999999999997,4.1970000000000001,14.75,12960.200554206243,1.7808694445408424,-26.367920933212726,-31.748153846715432,11.71,11.72,4.43,3.15,13.8,11.31,11.28,15.36,"none","none",27.14,99.572015023146136,1.1399999999999999,"Dipole","No",693.61601898541835,2250.56,2262.5996599937548,693.61601898541835,0.99389655172413793]
["InnoV 5 OP-DES",2.6302848000000001,9.19,6,4.32,15.22,9587.5391055456384,1.7201429116514633,-24.596225340374193,-29.976458253876899,12.19,12.3,4.5,3.24,14.12,11.71,11.64,21.06,"none","none",50.7,99.961553248750477,1.04,"Bent Dipole","No",373.97188988738287,1993.23,2003.332755211766,373.97188988738287,0.99410344827586206]
["PY1MHZ 4",2.75,9.35,6.2640000000000002,4.6740000000000004,15.57,11564.858998456466,3.548905038150878,-25.029308976623557,-30.409541890126267,12.38,12.52,4.6980000000000004,3.5005500000000001,14.43,11.9,11.91,17.170000000000002,"none","none",50.9,99.017936855774693,1.22,"Folded Dipole","Yes",561.20251517233396,2132.6480000000001,2155.197595761168,561.20251517233396,0.98791034482758622]
["InnoV 4 LFA 2.8m",2.8096223999999999,9.2100000000000009,6.13,4.41,15.29,10313.621616559261,2.9088882697130347,-24.823954358976913,-30.204187272479626,12.2,12.27,4.5999999999999996,3.31,14.16,11.74,11.65,21.2,"none","none",47,99.773242630385482,1.1000000000000001,"LFA Loop","Yes",442.67496371741731,2041.49,2059.0585817776541,442.67496371741731,0.99006896551724133]
["DK7ZB 4 12.5 ohm",2.839512,9.68,6.5380000000000003,5.0129999999999999,15.84,13493.613014992636,7.0052267269388491,-25.375603534112944,-30.75583644761565,12.68,12.8,4.91,3.7570000000000001,14.83,12.23,12.8,14.44,"none","none",11.1,96,1.5,"Dipole","No",743.67596982299153,2255.7199999999998,2303.2038423506142,743.67596982299153,0.97641379310344822]
["G0KSC 4 Quad",2.9889600000000001,10.25,6.3250000000000002,5.6959999999999997,16.23,13640.923882776751,12.126742348038524,-24.958620428223906,-30.338853341726619,13.21,13.21,4.75,4.28,15.13,12.68,12.74,15.32,18.53,"none",52.7,99.773242630385482,1.1000000000000001,"Quad","No",757.15221423608273,2232.89,2314.1345739330363,757.15221423608273,0.95986206896551729]
["EAntenna 50LFA4",2.9889600000000001,9.27,6.165,4.4749999999999996,15.34,10804.566411980271,3.4608137343848289,-24.966730839543235,-30.346963753045941,12.26,12.3,4.6275000000000004,3.36,14.22,11.79,11.72,21.15,"none","none",50.9,99.814564684874426,1.0900000000000001,"LFA Loop","Yes",489.15280522549466,2075.4499999999998,2096.7572754553698,489.15280522549466,0.98820689655172411]
["InnoV 4 LFA 3.33m",3.3476352000000005,9.4,6.17,4.4800000000000004,15.37,10640.590437271225,2.6235212247738349,-24.883000344618335,-30.263233258121037,12.38,12.4,4.63,3.36,14.32,11.94,11.84,25.3,"none","none",49.9,99.386268555288922,1.17,"LFA Loop","Yes",473.69105143658447,2068.13,2084.2160751565762,473.69105143658447,0.99103448275862072]
["InnoV 4 LFA-Q",3.3476352000000005,10.71,6.5380000000000003,5.2629999999999999,16.29,11550.063409825396,2.3387096774193528,-24.32163175366183,-29.701864667164539,13.26,13.3,4.9050000000000002,3.9449999999999998,15.23,12.79,12.8,13.9,14.1,"none",28.6,98.199059238020283,1.31,"LFA-Vert Loop","Yes",559.9149357764511,2139.2399999999998,2154.1532258064512,559.9149357764511,0.99199999999999999]
["F9FT 5 220505",3.4074144,9.8699999999999992,6.516,5.0129999999999999,16.02,11565.87105796988,3.9531632296399688,-24.57373895399747,-29.953971867500183,12.88,12.98,4.8899999999999997,3.7574999999999998,14.97,12.42,12.46,16.760000000000002,"none","none",16.8,99.318239205454091,1.18,"*Hairpin","No",561.26012060511971,2130.16,2155.2443201677734,561.26012060511971,0.98655172413793102]
["*F9FT 5 220505",3.4074144,9.8699999999999992,5.58,4.5,15.69,9600.1764065086845,3.9120710141888382,-24.09958918312639,-29.4798220966291,12.69,12.83,4.1849999999999996,3.375,14.33,12.04,12.22,16.760000000000002,"none","none",16.8,99.318239205454091,1.18,"*Hairpin","No",374.96186835984054,1981.32,2004.1357377507513,374.96186835984054,0.9866896551724138]
["G0KSC 4el-Q",3.4074144,10.220000000000001,6.54,5.26,16.29,{"$f":"Z46/9000*J$8+(1-Z46/9000)*F$8+290*(1/AD46-1)","v":11520.427749205817},2.3387096774193528,-24.31052716356756,-29.690760077070273,13.26,13.3,4.91,3.95,15.23,12.79,12.8,12.1,"none","none",49.9,99.67960128159487,1.1200000000000001,"LFA Vert Loop","Yes",557.10616423499994,2136.98,2151.875,557.10616423499994,0.99199999999999999]
["HyGain 4 VB-64DX",3.4671935999999999,9.65,6.4729999999999999,5.0010000000000003,15.51,20683.170967310893,1.4269873172084346,-27.636373128597516,-33.016606042100221,12.58,12.43,4.8499999999999996,3.75,14.59,12.11,12.28,11.68,14.68,"none",55.75,99.978160110655438,1.03,"*Beta Match","No",1425.6075802437149,2843.76,2856.3261487282557,1425.6075802437149,0.99510344827586206]
["Telrex 4-6m",3.5269727999999998,9.68,6.5609999999999999,5.0970000000000004,15.59,21397.491482217491,2.5115648151369019,-27.687355105882855,-33.06758801938556,12.64,12.47,4.92,3.8250000000000002,14.56,12.18,12.3,11.77,"none","none",51,99.72821814424654,1.1100000000000001,"Dipole","No",1493.2057630225484,2888.65,2911.1557858857086,1493.2057630225484,0.99141379310344824]
["Cushcraft A50-5S",3.5269727999999998,9.74,6.5830000000000002,5.14,15.67,21085.416275034353,1.7606244579358044,-27.55484802005931,-32.935080933562027,12.7,12.59,4.9349999999999996,3.855,14.65,12.25,12.33,12.23,"none","none",42.1,99.978160110655438,1.03,"*Gamma","No",1463.6994614067794,2871.55,2887.2228967909805,1463.6994614067794,0.99396551724137927]
["G0KSC 4 LFA",3.5269727999999998,9.86,6.41,4.87,15.85,11700.983273594902,2.2066641186894431,-24.819698558272016,-30.199931471774729,12.83,12.81,4.8099999999999996,3.65,14.77,12.37,12.33,18.8,"none","none",50.1,99.814564684874426,1.0900000000000001,"LFA Loop","Yes",574.2311445375517,2151.6,2165.7652618046627,{"$f":"(AB50-1700)*1.232876712","v":574.2311445375517},0.99244827586206896]
["DK7ZB 4 12.5 ohm",3.5867520000000002,10.39,6.8789999999999996,5.5019999999999998,16.43,14729.164123849461,4.1485082718337836,-25.20641272557587,-30.586645639078576,13.38,13.37,5.16,4.125,15.25,12.93,12.88,13.51,13.8,"none",51.5,97.222222222222214,1.4,"Folded Dipole","No",861.04823652273205,2368.67,2398.4057920324576,861.04823652273205,0.98589655172413793]
["Directive DSEJX5-50",3.6046857599999997,9.99,6.5380000000000003,5.0599999999999996,16.13,10803.341626540436,2.2574367528495931,-24.193995750431274,-29.57422866393398,13.03,13.07,4.9050000000000002,3.7949999999999999,15.02,12.52,12.52,16.96,"none","none",200.5,99.814564684874426,1.0900000000000001,"T Match","Yes",489.15077620143501,2082.8000000000002,2096.7556296914099,489.15077620143501,0.99227586206896556]
["Directive 4 DS50-4HP",3.7063104,10.28,6.9420000000000002,5.532,16.350000000000001,14814.274941657608,5.2638415897201529,-25.294967388149942,-30.675200301652652,13.27,13.29,5.2050000000000001,4.1475,15.23,12.86,12.81,12.87,12.87,"none",200.2,94.537660926880108,1.61,"T Match","Yes",869.00905539817813,2367.16,2404.8629006775968,869.00905539817813,0.98217241379310349]
["G4CQM WS65065",3.8856480000000002,9.59,6.2240000000000002,4.6689999999999996,15.46,12680.443087845415,1.5987656461288169,-25.566252512839473,-30.946485426342182,12.54,12.42,4.665,3.5,14.51,12.1,12.06,18.7,"none","none",49.65,99.978160110655438,1.03,"Dipole","No",667.11877527162562,2230.41,2241.1074511979473,667.11877527162562,0.9945172413793103]
["EAntennas 50LFA5S",3.8856480000000002,10.59,6.6870000000000003,5.4870000000000001,16.59,12203.354453059146,3.9942669370062633,-24.235061405048754,-29.615294318551459,13.53,13.56,5.0199999999999996,4.12,15.37,13.06,13.05,15.62,15.62,"none",54.8,97.994068780047527,1.33,"LFA Loop","Yes",621.67482808655484,2178.2399999999998,2204.2473606935605,621.67482808655484,0.98641379310344823]
["Maple Leaf BFM-4e6-13",3.8856480000000002,10.58,7.1520000000000001,5.8109999999999999,16.63,15581.533566085014,5.1394981575714667,-25.235287660264479,-30.615520573767192,13.6,13.61,5.3639999999999999,4.3579999999999997,15.56,13.18,13.13,12.4,11.7,"none",50,96,1.5,"Sinclair Feed","No",941.73911764265995,2426,2463.85506229163,941.73911764265995,0.98258620689655174]
["InnoV 4 LFA 3.9m Ver3",3.9125486399999998,10.48,6.7939999999999996,5.3650000000000002,16.52,12714.957441278237,2.9190902441572741,-24.498471136891514,-29.878704050394219,13.43,13.42,5.0955000000000004,4.0229999999999997,15.32,12.98,12.97,15.24,15.3,"none",49.17,98.199059238020283,1.31,"LFA Loop","Yes",670.26479738107332,2224.19,2243.659224687402,670.26479738107332,0.99003448275862072]
["Cushcraft LFA-6M4EL",3.9274934400000001,10.55,6.8419999999999996,5.444,16.55,12711.908923990879,3.3686817595144114,-24.460802359237036,-29.841035272739745,13.51,13.49,5.13,4.08,15.32,13.06,12.99,15.06,15.23,"none",53.5,98.76543209876543,1.25,"LFA Loop","Yes",669.93325800423622,2220.96,2243.3903094150069,669.93325800423622,0.9885172413793103]
["InnoV 5 LFA",3.9274934400000001,10.56,6.8419999999999996,5.4580000000000002,16.64,11153.555857013176,3.4403349616189849,-23.804400209608588,-29.184633123111304,13.55,13.61,5.13,4.0999999999999996,15.51,13.1,13.08,17,17,"none",48.95,98.199059238020283,1.31,"LFA Loop","Yes",522.23083085998326,2102.09,2123.5872295882764,522.23083085998326,0.98827586206896556]
["InnoV 5 LFA-HG",3.9274934400000001,10.67,7.0190000000000001,5.6719999999999997,16.739999999999998,12928.0799347543,4.0662260918214006,-24.333450359726946,-29.713683273229652,13.66,13.72,5.27,4.25,15.62,13.21,13.19,14.04,13.81,"none",47.35,94.810751181407554,1.59,"LFA Loop","Yes",690.35513245537379,2232.7150000000001,2259.9547186964578,690.35513245537379,0.9861724137931035]
["DK7ZB 4 12.5 ohm",3.9454272000000001,10.71,7.02,5.7,16.75,13301.386682501308,5.2327459102716762,-24.429436567440145,-29.809669480942851,13.7,13.69,5.27,4.28,15.43,13.24,13.09,13.75,13.75,"none",12.44,96.253902185223723,1.48,"Dipole","No",725.62537309729692,2253.14,2288.5628027803132,725.62537309729692,0.98227586206896556]
["DG7YBN YBN50-5wrc vs",3.95,11.12,6.7939999999999996,5.3730000000000002,16.448,11973.061530248868,3.7303757723083342,-24.298580951672161,-29.678813865174874,14.13,13.407999999999999,5.09,4.03,15.412000000000001,12.91,12.95,16.07,16.07,"none",49.23,99.814564684874426,1.0900000000000001,"Hairpin","Yes",599.87342449756773,2253.14,2186.5639999999999,599.87342449756773,0.98729999999999996]
["G0KSC 5 Quad",4.0649856,10.9,6.819,6.2539999999999996,16.920000000000002,14658.622055222786,12.670409558770587,-24.572082537334712,-29.952315450837421,13.92,13.8,5.12,4.6900000000000004,15.65,13.35,13.33,14.05,14.05,"none",50.81,99.627498953029601,1.1299999999999999,"Quad","Yes",853.55481056209078,2304.3200000000002,2392.3277909738722,853.55481056209078,0.95813793103448275]
["YU7EF EF0605C",4.1247647999999995,10.14,6.5380000000000003,5.0720000000000001,16.12,11637.345647397464,2.9088882697130347,-24.515750406623827,-29.895983320126533,13.11,13.05,4.9050000000000002,3.8025000000000002,14.99,12.61,12.62,23.61,"none","none",49.53,99.961553248750477,1.04,"Dipole","No",568.13322274799657,2142.2399999999998,2160.8191696851491,568.13322274799657,0.99006896551724133]
["DK7ZB 5 50 ohm",4.2443232000000002,10.65,6.94,5.61,16.59,14098.151713510169,2.9905239687848417,-24.874046236743105,-30.254279150245814,13.61,13.52,5.21,4.21,15.2,13.15,12.9,12.7,12.85,"none",50.3,99.627498953029601,1.1299999999999999,"Dipole","No",801.35268224381275,2328.96,2349.9860646599777,801.35268224381275,0.98979310344827587]
["PY1MHZ 5",4.2969999999999997,10.38,6.7220000000000004,5.29,16.47,10035.152056237306,4.9469726726895047,-23.495775109100837,-28.87600802260355,13.38,13.45,5.04,3.9674999999999998,15.41,12.93,12.93,19.600000000000001,19.600000000000001,"none",48.49,98.852040816326536,1.24,"Folded Dipole","Yes",416.08936133194561,2008.1849999999999,2037.4947042814656,416.08936133194561,0.98322758620689654]
["OZ3SW 4 (OZ6FRS)",4.3638816,9.93,6.43,4.9550000000000001,15.63,15038.806280609175,1.3966945012300225,-26.137101036953094,-31.517333950455814,12.85,12.57,4.82,3.72,14.81,12.46,12.45,14.66,15.96,"none",31.2,99.814564684874426,1.0900000000000001,"Dipole","No",890.6559211770375,2412.1999999999998,2422.4209140362427,890.6559211770375,0.99520689655172412]
["G0KSC 5 4.4 LFA",4.3638816,10.6,6.88,5.48,16.68,10409.025387370579,5.2949438202246757,-23.43868319032924,-28.818916103831953,13.58,13.56,5.16,4.1100000000000003,15.62,13.14,13.15,19.38,19.38,"none",49.9,99.67960128159487,1.1200000000000001,"LFA Loop","Yes",451.49088028594349,2034.36,2066.2092696629211,451.49088028594349,0.98206896551724143]
["DG7YBN YBN 50-5w",4.38,9.8659999999999997,6.3040000000000003,4.8330000000000002,15.679,12370.997078813081,1.8973326623049935,-25.235999328801167,-30.61623224230388,12.79,12.64,5.79,4.34,15.34,12.69,12.48,19.37,"none","none",50.48,99.978160110655438,1.03,"Folded Dipole","Yes",637.76219161075176,2034.36,2217.2959999999998,637.76219161075176,0.99350000000000005]
["EAntenna 50LFA5",4.4236608000000004,10.5,6.7220000000000004,5.3170000000000002,16.57,9339.7279654128888,4.3647182359117975,-23.094190287748415,-28.474423201251131,13.46,13.52,5.04,3.99,15.45,13.02,13.02,21.33,21.33,"none",50.03,99.51325040562466,1.1499999999999999,"LFA Loop","Yes",350.23451163219039,1958.96,1984.0791039551978,350.23451163219039,0.9851724137931035]
["DK7ZB 5 28 ohm",4.4834399999999999,10.76,6.9939999999999998,5.6559999999999997,16.690000000000001,13572.441336905165,3.9428890985984144,-24.595623913633716,-29.975856827136429,13.72,13.63,5.24,4.25,15.32,13.27,13.05,13.26,13.32,"none",29.11,99.814564684874426,1.0900000000000001,"Dipole","No",751.43730023440503,2282.41,2309.499143685995,751.43730023440503,0.98658620689655174]
["YU7EF EF0605A",4.4834399999999999,10.74,6.9939999999999998,5.6719999999999997,16.68,14035.365599064708,3.3175223214285898,-24.759912211941515,-30.140145125444224,13.7,13.62,5.2424999999999997,4.2525000000000004,15.23,13.23,12.99,12.92,12.92,"none",49.66,99.915166368177964,1.06,"Dipole","No",795.37102665005796,2321.89,2345.1342773437495,795.37102665005796,0.98868965517241381]
["IZ1MYT 5",4.4834399999999999,11.04,7.2350000000000003,5.9770000000000003,17.02,14551.166314004342,4.5915650833683985,-24.557297248572961,-29.937530162075667,14.01,13.98,5.43,4.4850000000000003,15.66,13.54,13.27,14.15,13.84,"none",49.41,98.676482105098287,1.26,"Dipole","No",844.13619145207213,2352.04,2384.6882443603754,844.13619145207213,0.98441379310344823]
["JK Antennas JK65",4.4834399999999999,10.62,6.9420000000000002,5.593,16.510000000000002,15357.96722707182,2.592979160143325,-25.330247032849343,-30.710479946352052,13.58,13.39,5.2065000000000001,4.19475,15.24,13.14,12.97,13.81,13.91,"none",47.65,99.67960128159487,1.1200000000000001,"Dipole","No",920.79157783493145,2427.75,2446.8642799986083,920.79157783493145,0.99113793103448278]
["G0KSC 5el-Q",4.4953958400000005,11.39,7.319,6.2640000000000002,17.41,13103.763566542049,3.6452513966480127,-23.728017426300177,-29.108250339802883,14.37,14.38,5.49,4.6950000000000003,16.25,13.88,13.87,14.77,13.32,"none",49.1,99.386268555288922,1.17,"LFA Vert Loop","Yes",707.04575438404186,2248.87,2273.4926675977654,707.04575438404186,0.98758620689655174]
["N6CA 4",4.5133296000000005,10.88,7.0460000000000003,5.72,16.8,13150.013443092683,4.7980931015143025,-24.336309248972238,-29.716542162474951,13.83,13.75,5.2874999999999996,4.29,15.42,13.38,13.16,14.25,14.24,"none",19.45,97.888815837533784,1.34,"Dipole","No",711.31990469587743,2244.62,2276.9594784071787,711.31990469587743,0.98372413793103453]
["G0KSC 5 4.6m LFA",4.5432192000000002,10.78,6.968,5.593,16.850000000000001,10304.925193511623,5.0049109022028571,-23.229509040903253,-28.609741954405962,13.76,13.83,5.23,4.2,15.77,13.76,13.83,18.87,18.11,"none",48.5,99.773242630385482,1.1000000000000001,"LFA Loop","Yes",441.6520908117605,2028.23,2058.2289181984002,441.6520908117605,0.98303448275862071]
["G0KSC 5 4.7m  LFA",4.7225568000000004,10.98,7.0720000000000001,5.7359999999999998,16.97,{"$f":"Z78/9000*J$8+(1-Z78/9000)*F$8+290*(1/AD78-1)","v":11508.347063865616},3.5120231738386543,-23.608679691103461,-28.98891260460617,13.96,13.95,5.3,4.3049999999999997,15.8,13.5,13.37,17.079999999999998,17.079999999999998,"none",50.4,99.990197039505929,1.02,"LFA Loop","Yes",555.84999332588461,2128.59,2150.8561058178902,555.84999332588461,0.98803448275862071]
["Telrex 5",4.7823359999999999,11.03,7.2350000000000003,5.9770000000000003,16.98,15001.667025704493,3.2050343408987825,{"$f":"F79-10*LOG((Z79/9000*J$8+(1-Z79/9000)*F$8)+290*(10^(0.1*P$8)/AD79-1))+10*LOG(1/AD79)","v":-24.749632033126836},{"$f":"10*LOG(10^(F79/10)*1E-20/AD79/1.380649E-23/2500/(Z79/9000*J$8+(1-Z79/9000)*F$8+290*(10^(P$8/10)/AD79-1)))","v":-30.129864946629546},13.99,13.94,5.43,4.49,15.55,13.53,13.25,13.05,12.77,"none",19.87,98.396292976869248,1.29,"Dipole","No",886.96459480067767,2396.15,2419.4268381968413,886.96459480067767,0.98906896551724133]
["M² 6M5",4.7823359999999999,11.08,7.2350000000000003,5.95,17.03,14918.276948092907,4.880785413744773,-24.650853679660404,-30.031086593163113,14.03,14.03,5.43,4.46,15.7,13.54,13.4,13.9,14.9,"none",197.8,{"$f":"(1-((W80-1)/(W80+1))^2)*10^2","v":98.097502972651611},1.32,"T Match","Yes",878.90233218315564,2377.75,2412.8874474053296,878.90233218315564,0.98344827586206895]
["InnoV 6 OP-DES",4.7823359999999999,10.93,6.9809999999999999,5.5780000000000003,17,9872.2297521230903,{"$f":"290*(1/AD81-1)","v":3.1641510091679526},-22.921266746092762,-28.301499659595471,14,14,5.24,4.1900000000000004,15.87,13.46,13.47,17.5,17.04,"none",50.7,99.978160110655438,1.03,"Bent Dipole","No",400.81708519403213,2006.38,2025.1071914107436,400.81708519403213,0.98920689655172411]
["I0JXX 5JXX6",4.8241814400000003,11.18,7.4950000000000001,6.3140000000000001,17.13,18317.184442961534,4.0353821411090145,-25.451692788083943,-30.831925701586652,14.13,14.1,5.625,4.7320000000000002,15.39,13.64,13.26,11.98,10.8,"none",17.77,96.868702264221241,1.43,"*Hairpin","No",1201.1198562277152,2641.52,2674.241661422278,1201.1198562277152,0.98627586206896556]
["G0KSC 5 LFA 4.9m",4.8421152000000003,11.02,7.02,5.69,17.03,10094.610423136783,4.7154471544715708,-22.964681980748125,-28.344914894250838,13.98,14.02,5.27,4.2699999999999996,15.87,13.52,13.47,19.3,18.7,"none",49.7,99.852071005917168,1.08,"LFA Loop","Yes",421.74657522999991,2014.05,2042.0833333333333,421.74657522999991,0.98399999999999999]
["G4CQM WS66082",4.9018943999999998,10.66,6.7450000000000001,5.3719999999999999,16.649999999999999,9635.9387913979535,2.4200278164116673,-23.17762193920764,-28.557854852710349,13.63,13.62,5.0625,4.0274999999999999,15.43,13.16,13.05,18.77,18.8,"none",49.89,99.940511600237954,1.05,"Dipole","No",378.49272190642262,1992.79,2006.9996522948538,378.49272190642262,0.99172413793103453]
["W5WVO CC A50-5 MOD",5.2007903999999998,11.29,7.4649999999999999,6.2640000000000002,17.32,14128.215200674536,5.0980736166181462,-24.122255035134458,-29.502487948637167,14.22,14.31,5.51,4.57,15.8,13.72,13.56,12.35,11.41,"none",11.96,95.08092476797529,1.57,"*Gamma","No",804.00225509184145,2316.5100000000002,2352.1351626372852,{"$f":"(AB85-1700)*1.232876712","v":804.00225509184145},0.98272413793103452]
["M² 6M5X",5.4399072000000004,11.54,7.59,6.39,17.510000000000002,14084.302021800919,7.941687037233871,-23.877304071257207,-29.257536984759916,14.5,14.48,5.69,4.79,16.18,14.01,13.85,12.7,12.58,"none",13.7,96.253902185223723,1.48,"*Hairpin","No",799.57079836639809,2293.67,2348.5407588479115,799.57079836639809,0.97334482758620688]
["M² 6M5XHP",5.4399072000000004,11.55,7.5869999999999997,6.4080000000000004,17.52,14139.190629452507,7.5411286042809511,-23.889948877821471,-29.27018179132418,14.51,14.48,5.69,4.8079999999999998,16.190000000000001,14.02,13.86,14.43,12.53,"none",13.69,96.127481814809428,1.49,"*Hairpin","No",804.81092573329863,2300.5100000000002,2352.7910843799755,804.81092573329863,0.97465517241379307]
["InnoV 5 LFA-Q",5.4996864000000008,11.91,7.7130000000000001,6.8789999999999996,17.93,13266.275400594366,5.0049109022028571,-23.241344157130222,-28.621577070632931,14.86,14.86,5.78,5.16,16.75,14.38,14.36,19.7,14.6,"none",28.89,98.298676748582224,1.3,"LFA Vert Loop","Yes",722.31923343754704,2252.02,2285.8811561666898,722.31923343754704,0.98303448275862071]
["Directive DSEJX6-50",5.5875618239999998,11.23,7.4359999999999999,6.2140000000000004,17.27,13236.235453386675,9.2137190023837299,-23.830276704148606,-29.210509617651322,14.23,14.24,5.58,4.657,16.16,13.78,13.73,15.3,13.3,"none",200.2,94.123048668503216,1.64,"T Match","Yes",719.07324778284135,2221.87,2283.2483011349486,719.07324778284135,0.9692068965517241]
["Create CL6DX 6el",5.6192447999999997,11.08,7.0190000000000001,5.72,16.95,12169.298707182666,2.0848817420901056,-23.891149566103344,-29.271382479606057,14.09,13.93,5.27,4.29,15.51,13.51,13.29,14.78,15.13,"none",47.8,99.940511600237954,1.05,"Dipole","No",618.6281005577631,2188.13,2201.7761261417704,618.6281005577631,0.99286206896551721]
["BQH 5",5.6192447999999997,11.29,7.2629999999999999,5.9770000000000003,17.27,11404.954899952087,8.3644942704083753,-23.198808453138525,-28.579041366641242,14.25,14.25,5.4450000000000003,4.8499999999999996,16.28,13.78,13.84,17.010000000000002,16.05,"none",16.53,98.396292976869248,1.29,"Dipole","No",545.59091881987263,2090.6,2142.5348564941282,545.59091881987263,0.97196551724137925]
["EAntennas 50LFA5L",5.6790240000000001,11.22,7.0720000000000001,5.7530000000000001,17.149999999999999,9460.8754469994128,4.684466869897312,-22.565145428820607,-27.945378342323316,14.12,14.13,5.3,4.3099999999999996,16.010000000000002,13.66,13.59,21.3,22.34,"none",48.7,98.097502972651611,1.32,"LFA Loop","Yes",361.68617124226654,1966.29,1993.3676723080698,361.68617124226654,0.98410344827586205]
["Innov 6 LFA MAX5.8m",5.7985823999999999,11.19,7.05,5.74,17.16,9350.6859822620427,4.086792320872803,-22.513330847339972,-27.893563760842689,14.16,14.2,5.29,4.3099999999999996,16.11,13.69,13.67,23.7,20.8,"none",51,99.67960128159487,1.1200000000000001,"LFA Loop","Yes",351.2994177492684,1961.3889999999999,1984.9428611392802,351.2994177492684,0.98610344827586205]
["BV 6-6m",5.8583616000000003,11.63,7.7450000000000001,6.5830000000000002,17.61,16133.538677955896,4.0456627390650741,-24.422023562752027,-29.80225647625474,14.6,14.56,5.8125,4.9349999999999996,16.28,14.13,13.91,14.94,11.9,"none",46.98,99.51325040562466,1.1499999999999999,"Dipole","No",994.1600372467509,2475.88,2506.3742526485089,994.1600372467509,0.98624137931034483]
["Eantenna 50LFA5XL",5.8583616000000003,11.7,7.5869999999999997,6.3869999999999996,17.7,12870.968346603504,4.385326239148684,-23.349614672958605,-28.729847586461315,14.67,14.65,5.69,4.79,16.47,14.21,14.11,18.09,14.45,"none",54.26,98.58526266762405,1.27,"LFA Loop","Yes",684.9120385770766,2226.2600000000002,2255.5397647717728,684.9120385770766,0.98510344827586205]
["YU7EF EF0606 W1",5.9181407999999998,11.56,7.59,6.4080000000000004,17.53,14983.123490138281,3.9942669370062633,-24.182648713229252,-29.562881626731961,14.52,14.47,5.69,4.8099999999999996,16,14.02,13.73,14.1,11.73,"none",50.35,99.978160110655438,1.03,"Dipole","No",885.13229790239552,2389.0300000000002,2417.9406418233939,885.13229790239552,0.98641379310344823]
["Cushcraft A50-6S",5.9779200000000001,11.05,7.0190000000000001,5.7690000000000001,16.899999999999999,13182.865327063086,2.0645945476644845,-24.28738842221038,-29.667621335713086,13.97,13.87,5.2649999999999997,4.3274999999999997,15.4,13.48,13.18,13.52,13.26,"none",37.43,99.961553248750477,1.04,"*Gamma","No",714.69257153157969,2265.63,2279.6950859524222,714.69257153157969,0.99293103448275866]
["DK7ZB 5 18 ohm",5.9779200000000001,11.52,7.649,6.4729999999999999,17.489999999999998,14783.702720061199,5.4401742429564814,-24.143446086731213,-29.523679000233926,14.48,14.44,5.74,4.8600000000000003,15.86,13.98,13.53,11.89,10.6,"none",16.89,97.45074500388391,1.38,"Dipole","No",866.09480741748291,2363.6,2402.4991217592915,866.09480741748291,0.98158620689655174]
["DK7ZB 5 12.5 ohm",5.9779200000000001,11.72,7.6818,6.4729999999999999,17.68,13024.727986086409,5.2431104089871772,-23.408386522257118,-28.788619435759827,14.68,14.64,5.76,4.8499999999999996,16.22,14.2,13.89,14.3,12.1,"none",13,97.45074500388391,1.38,"Dipole","No",699.40357920278848,2232.1799999999998,2267.2940143935402,699.40357920278848,0.98224137931034483]
["DK7ZB 6 50 ohm",5.9779200000000001,11.62,7.78,6.61,17.63,14700.945010588404,6.1580448638941139,-23.968658149548826,-29.348891063051529,14.68,14.68,5.84,4.96,16.559999999999999,14.25,14.09,14.56,12.17,"none",50.07,98.097502972651611,1.32,"Dipole","No",858.18326339006512,2352.29,2396.081980490897,858.18326339006512,0.9792068965517241]
["G0KSC 6 6.0m LFA",5.9779200000000001,11.25,7.125,5.82,17.25,9317.3245876232595,4.086792320872803,-22.407900019903845,-27.788132933406551,14.23,14.25,5.35,4.37,16.170000000000002,13.77,13.76,20.75,18.72,"none",50.8,99.773242630385482,1.1000000000000001,"LFA Loop","Yes",348.13753325317475,1958.86,1982.3782214917649,348.13753325317475,0.98610344827586205]
["OptiBeam OB6-6",6.0376992000000005,11.65,7.53,6.37,17.62,13345.532826301313,3.3584484442584239,-23.601311459041149,-28.981544372543858,14.6,14.58,5.65,4.78,16.22,14.12,13.9,14.58,12.54,"none",26,99.247305102062086,1.19,"Dipole","No",729.98704086682278,2269.1799999999998,2292.1005999720942,729.98704086682278,0.98855172413793102]
["EAntenna 50LFA6S",6.0974784,11.85,7.649,6.4939999999999998,17.84,12162.748567471761,4.6431699541043052,-22.961120293280185,-28.341353206782895,14.8,14.81,5.74,4.87,16.62,14.36,14.25,19.600000000000001,14.58,"none",53.9,97.67308244757254,1.36,"LFA Loop","Yes",617.76483337888499,2170.96,2201.0759205409381,617.76483337888499,0.98424137931034483]
["PY1MHZ 6 V1",6.15,11.55,7.56,6.3250000000000002,17.57,12240.560541065564,6.2717668154483786,-23.234860104484728,-28.615093017987427,14.55,14.56,5.7,4.75,16.62,14.13,14.14,17.84,15.36,"none",51.28,97.994068780047527,1.33,"Folded Dipole","Yes",624.98524608520472,2166.3530000000001,2206.9324775154037,624.98524608520472,0.97883103448275866]
["M² 6M5XHG",6.1572576000000003,12.02,8.0500000000000007,6.95,18.010000000000002,15400.665160526138,7.6359003397508651,-23.76831433936891,-29.148547252871616,14.99,14.96,6.04,5.21,16.59,14.5,14.2,17.600000000000001,12,"none",9,94.946217174448648,1.58,"*Hairpin","No",924.3603974481623,2394.35,2449.7589892412229,924.3603974481623,0.97434482758620689]
["*M² 6M5XHG",6.1572576000000003,12.02,7.62,7.01,17.98,15197.593148041307,7.6569689247540174,-23.740572048433236,-29.120804961935946,14.92,15,5.7149999999999999,5.2575000000000003,16.45,14.39,14.22,17.600000000000001,12,"none",9,94.946217174448648,1.58,"*Hairpin","No",905.11189566184692,2378.9899999999998,2434.1463155659371,905.11189566184692,0.97427586206896555]
["InnoV 6 LFA 6.1m",6.1572576000000003,11.39,7.26,6,17.38,10359.458559414572,4.684466869897312,-22.727003296601634,-28.10723621010435,14.36,14.41,5.45,4.5,16.34,13.91,13.89,24.6,18.3,"none",49.7,99.572015023146136,1.1399999999999999,"LFA Loop","Yes",446.85095653856428,2034.27,2062.4457759557099,446.85095653856428,0.98410344827586205]
["InnoV 5 LFA 6.2m Ver 3",6.1931251200000004,11.79,7.4359999999999999,6.2240000000000002,17.77,10838.968269546458,4.086792320872803,-22.541259651252943,-27.92149256475566,14.77,14.75,5.58,4.67,16.48,14.27,14.18,21.8,15.4,"none",47.03,96,1.5,"LFA Loop","Yes",492.35397319956041,2074.21,2099.3537783683601,492.35397319956041,0.98610344827586205]
["WiMo ZX 6-6 ",6.2170368000000007,11.45,7.75,6.59,17.47,15866.593791579806,3.3686817595144114,-24.499789888529076,-29.880022802031789,14.43,14.44,5.81,4.9400000000000004,16.43,14.01,13.95,15.9,11.01,"none",21.4,99.885644939205122,1.07,"Dipole","No",968.92403104867947,2460.69,2485.9050476157258,968.92403104867947,0.9885172413793103]
["G0KSC 6 6.2m LFA",6.2170368000000007,11.22,7.1520000000000001,5.8710000000000004,17.23,{"$f":"Z110/9000*J$8+(1-Z110/9000)*F$8+290*(1/AD110-1)","v":9704.2877537548011},4.9842160645387672,-22.590442729625984,-27.970675643128693,14.19,14.24,5.36,4.4000000000000004,16.21,13.76,13.74,29.86,"none","none",46.8,99.51325040562466,1.1499999999999999,"LFA Loop","Yes",384.72758887123382,1982.96,2012.0568221676604,384.72758887123382,0.98310344827586205]
["G0KSC 6 6.4m LFA",6.2170368000000007,11.6,7.319,6.1070000000000002,17.59,9832.3242373989306,4.7051196692013892,-22.2911336433251,-27.671366556827813,14.56,14.58,5.49,4.58,16.36,14.09,14,20.36,16.989999999999998,"none",48.37,99.67960128159487,1.1200000000000001,"LFA Loop","Yes",396.88892227851272,1994.27,2021.9210148228615,396.88892227851272,0.98403448275862071]
["EAntenna 50LFA6M",6.2768160000000002,11.69,7.4059999999999997,6.165,17.77,9835.8595992021819,4.6534930978908644,-22.113442757168404,-27.493675670671109,14.67,14.7,5.56,4.63,16.61,14.23,14.18,24.64,18.399999999999999,"none",51.76,98.491843644198212,1.28,"LFA Loop","Yes",397.22888537214209,1994.84,2022.1967626655455,397.22888537214209,0.98420689655172411]
["+PY1MHZ 6 V2",6.3,11.67,7.6180000000000003,6.3869999999999996,17.677,12267.082383319681,5.1053220718428776,-23.154271979416247,-28.534504892918964,14.65,14.65,5.71,4.79,16.59,14.21,14.16,17.84,15.4,"none",51.28,97.994068780047527,1.33,"Folded Dipole","Yes",627.6094518874321,2011.88,2209.0610000000001,627.6094518874321,0.98270000000000002]
["Cushcraft LFA-6M5EL",6.3246393600000008,11.66,7.3479999999999999,6.1260000000000003,17.61,9987.0091526306041,3.7067821470978402,-22.353203940439645,-27.733436853942358,14.6,14.6,5.51,4.5999999999999996,16.38,14.14,14.02,21.51,17.95,"none",43.07,95.21484375,1.56,"LFA Loop","Yes",411.64407470884117,2011.88,2033.8890829084305,411.64407470884117,0.98737931034482762]
["InnoV 6 LFA 6.4m",6.4561536000000004,11.63,7.57,6.39,17.73,11757.224481191502,4.6741415557112553,-22.924077636192248,-28.304310549694954,14.69,14.73,5.68,4.79,16.68,14.25,14.24,24.9,15.1,"none",49.79,99.627498953029601,1.1299999999999999,"LFA Loop","Yes",579.32764381552352,2140.08,2169.8990889978977,579.32764381552352,0.98413793103448277]
["IZ1MYT 6",6.5159328000000007,12.05,7.95,6.82,18.04,13684.817235407356,5.4297959040292447,-23.259464425122189,-28.639697338624906,15.02,15,5.96,5.12,16.59,14.52,14.24,17.149999999999999,12.04,"none",53.3,99.173553719008268,1.2,"Dipole","No",761.94699826800695,2280.75,2318.0236765377454,761.94699826800695,0.98162068965517246]
["G0KSC 6el-Q",6.695270400000001,12.05,7.649,6.6630000000000003,18.059999999999999,10523.153674543273,3.5120231738386543,-22.131954263938464,-27.512187177441167,15.03,15.05,5.7374999999999998,4.9950000000000001,16.98,14.57,14.57,24.81,16.09,"none",48.59,99.773242630385482,1.1000000000000001,"LFA Vert Loop","Yes",462.47656763189661,2053.7600000000002,2075.1198827347926,462.47656763189661,0.98803448275862071]
["InnoV 6 LFA 6.83m",6.8148287999999999,11.9,7.56,6.37,17.87,10266.109591652676,4.9842160645387672,-22.193510731724565,-27.573743645227282,14.86,14.9,5.67,4.78,16.670000000000002,14.37,14.31,27.1,16.5,"none",50.6,99.915166368177964,1.06,"LFA Loop","Yes",437.97523568126832,2025.42,2055.2465801473168,437.97523568126832,0.98310344827586205]
["YU7EF EF0606W1 6.85m",6.8746079999999994,11.82,7.62,6.43,17.829999999999998,11438.177264127662,4.3544153162297334,-22.709859300084105,-28.090092213586814,14.79,14.8,5.72,4.82,16.57,14.31,14.19,19.8,14.2,"none",49,99.773242630385482,1.1000000000000001,"Dipole","No",549.11968870369526,2117.9499999999998,2145.3970809562143,{"$f":"(AB119-1700)*1.232876712","v":549.11968870369526},0.98520689655172411]
["G4CQM 6CQM7UX",6.8746079999999994,11.75,7.35,6.15,17.670000000000002,9661.665457336323,2.6948108446733632,-22.165079854728113,-27.545312768230822,14.69,14.67,5.51,4.6100000000000003,16.48,14.23,13.34,23.4,20.9,"none",50.4,99.72821814424654,1.1100000000000001,"Dipole","No",380.90496860177791,1993.13,2008.9562523927193,380.90496860177791,0.99079310344827587]
["K6STI 5",6.8746079999999994,12.47,8.2650000000000006,7.2350000000000003,18.420000000000002,14379.545308042523,5.9391934689281234,-23.086222437741714,-28.466455351244427,15.42,15.4,6.2,5.43,17,14.91,14.67,17.829999999999998,12.64,"none",12,93.13598671042061,1.71,"Dipole","No",827.74278676455731,2329.62,2371.3913716658453,827.74278676455731,0.97993103448275864]
["EAntenna 50LFA6",6.8746079999999994,11.72,7.3479999999999999,6.1449999999999996,17.66,9243.4384844507513,4.9738697344884564,-21.95052648182514,-27.330759395327853,14.62,14.64,5.51,4.6100000000000003,16.52,14.17,14.11,27.2,21.28,"none",49.58,99.773242630385482,1.1000000000000001,"LFA Loop","Yes",341.05077435179402,1948.19,1976.6300726035565,341.05077435179402,0.98313793103448277]
["YU7EF EF0606",6.9941664000000001,11.86,7.4649999999999999,6.3040000000000003,17.77,10786.960396891085,2.6948108446733632,-22.54097746292766,-27.92121037643037,14.79,14.75,5.6,4.7300000000000004,16.37,14.3,13.77,20.9,15.4,"none",49.6,99.961553248750477,1.04,"Dipole","No",487.55676363118897,2078.84,2095.4627083840878,487.55676363118897,0.99079310344827587]
["Create CL6DXX 7el",7.1137248,11.85,7.4950000000000001,6.3449999999999998,17.72,11508.759869619351,2.2980675656888616,-22.876748303126206,-28.256981216628922,14.76,14.69,5.62,4.76,16.27,14.32,14.05,17.14,13.25,"none",89.4,99.852071005917168,1.08,"Folded Dipole","No",556.00417247770588,2136.35,2150.9811622410675,556.00417247770588,0.99213793103448278]
["DK7ZB 6 50 ohm",7.1137248,12.44,8.0129999999999999,6.9169999999999998,18.21,13518.936505897169,3.6452513966480127,-23.062921162024356,-28.443154075527065,15.24,15.19,6.0075000000000003,5.19,16.8,14.75,14.5,16.57,13.72,"none",47.68,97.67308244757254,1.36,"Dipole","No",746.39449547709216,2280.39,2305.4088687150838,746.39449547709216,0.98758620689655174]
["DK7ZB 6 28 ohm",7.1735040000000003,12.34,8.048,6.968,18.29,13116.632227207383,4.3338116403597997,-22.842133505967965,-28.222366419470678,15.29,15.27,6.0374999999999996,5.2275,16.88,14.79,14.56,19.36,13.31,"none",27.49,99.67960128159487,1.1200000000000001,"Dipole","No",708.20014469358898,2245.21,2274.4290064046477,708.20014469358898,0.98527586206896556]
["W1JR 6",7.2093715199999995,12.34,7.32,6.13,17.600000000000001,11320.538763068887,2.0341690395166312,-22.929381783490285,-28.309614696992988,14.5,14.49,5.49,4.5975000000000001,15.98,14,13.71,17.600000000000001,15.4,"none",47.18,99.814564684874426,1.0900000000000001,"Dipole","No",538.19019951836924,2123.67,2136.5320508368636,538.19019951836924,0.99303448275862072]
["EAntenna 50LFA6XL",7.2332831999999998,12.32,7.944,6.8419999999999996,18.29,11483.323800682027,4.4162436548223161,-22.265977013230916,-27.646209926733626,15.27,15.27,5.96,5.13,17.010000000000002,14.79,14.66,22.42,14.03,"none",50.99,99.885644939205122,1.07,"LFA Loop","Yes",553.39267073762448,2120.98,2148.8629441624366,553.39267073762448,0.98499999999999999]
["Hygain VB-66DX",7.2571948800000001,11.11,7.3769999999999998,6.2039999999999997,16.7,19033.962168720092,1.5482215905151508,-26.084689513646207,-31.46492242714892,13.95,13.63,5.5350000000000001,4.6500000000000004,15.14,13.52,13.06,14.27,10.09,"none",37.130000000000003,99.67960128159487,1.1200000000000001,"*Beta Match","No",1269.2894431778243,2716.58,2729.5347708521113,1269.2894431778243,0.99468965517241381]
["Hygain VB-66B",7.2571948800000001,10.48,7.0460000000000003,5.8029999999999999,15.76,22222.247766230692,1.2049861495845082,-27.700586359839384,-33.080819273342087,13.27,12.69,5.29,4.3499999999999996,14.76,12.9,12.7,12.89,9.7899999999999991,"none",45.44,99.852071005917168,1.08,"*Beta Match","No",1571.4973148771057,2963.55,2974.6589335180061,1571.4973148771057,0.99586206896551721]
["Tilton 7",7.2930624000000002,12.15,7.91,6.8179999999999996,18.079999999999998,13896.212655630919,2.7865199832892462,-23.324648217197677,-28.704881130700389,15.09,15.04,5.93,5.1150000000000002,16.559999999999999,14.59,14.28,17.14,12.42,"none",25.88,99.097070084560102,1.21,"Dipole","No",782.23288985708371,2315.02,2334.4777886088286,782.23288985708371,0.99048275862068969]
["N6CA 6",7.2930624000000002,12.23,7.91,6.7939999999999996,18.2,11767.339595369145,6.900374214502607,-22.425261818233324,-27.805494731736026,15.19,15.19,5.94,5.0999999999999996,16.97,14.71,14.6,20.07,15.01,"none",21.29,99.386268555288922,1.17,"Dipole","No",580.07532635206167,2126.8000000000002,2170.5055426110293,580.07532635206167,0.97675862068965513]
["G0KSC 6 7.3m LFA",7.2930624000000002,12.3,7.8760000000000003,6.7889999999999997,18.27,11069.023080954996,5.6167176350662391,-22.109591695370479,-27.489824608873185,15.25,15.25,5.91,5.09,17.010000000000002,14.76,14.66,22.14,15.25,"none",50.15,99.885644939205122,1.07,"LFA Loop","Yes",514.01281876452572,2082.21,2116.9215086646277,514.01281876452572,0.98099999999999998]
["M² 6M6LN",7.3020292800000002,11.67,7.2629999999999999,6.069,17.489999999999998,10865.925709514455,3.6862690319877389,-22.837881451034928,-28.218114364537637,15.44,15.43,6.07,5.27,17.190000000000001,14.96,14.86,19.52,17.899999999999999,"none",24.87,99.72821814424654,1.1100000000000001,"*Hairpin","No",494.94687199180908,2078.7199999999998,2101.4569073893003,494.94687199180908,0.98744827586206896]
["I0JXX 6JXX6",7.3408857599999999,12.43,8.6560000000000006,7.649,18.399999999999999,19136.97122870223,5.0049109022028571,-24.357021188175246,-29.737254101677951,15.38,15.38,6.49,5.74,16.88,14.82,14.51,12.07,10.14,"none",15.22,95.347943098808159,1.55,"*Hairpin","No",1278.7246931360598,2695.67,2737.1878069313875,1278.7246931360598,0.98303448275862071]
["InnoV 7 OP-DES",7.4126208,12.2,7.7290000000000001,6.516,18.149999999999999,9739.2410852387893,3.4403349616189849,-21.708629081938838,-27.088861995441547,15.14,15.14,5.7975000000000003,4.8899999999999997,16.940000000000001,14.66,14.6,24.1,17.399999999999999,"none",49.5,99.961553248750477,1.04,"Bent Dipole","Yes",388.18667599509831,1994.64,2014.8625261688765,388.18667599509831,0.98827586206896556]
["N1DPM 5 HyGain mod",7.6517376000000006,11.91,7.4649999999999999,6.2839999999999998,17.66,11535.265924591107,3.2766076161249469,-22.932245893180124,-28.312478806682829,14.78,14.71,5.6,4.71,16.29,14.31,14.09,14.48,18.850000000000001,"none",14.82,96.503404058430831,1.46,"*Beta Match","No",558.42358732913692,2132.13,2152.9435765099738,558.42358732913692,0.98882758620689659]
["DK7ZB 7 50 ohm",7.7115168000000001,12.32,8.1189999999999998,7.0720000000000001,18.29,13980.244544470801,3.1845912497821249,-23.134850695314078,-28.515083608816791,15.27,15.26,6.09,5.3,16.72,14.73,14.42,19.68,11.21,"none",48.21,99.72821814424654,1.1100000000000001,"Dipole","No",790.15943111825152,2318.63,2340.907094300157,790.15943111825152,0.98913793103448278]
["UA9TC 7RV el",7.7712960000000004,12.42,7.94,6.87,18.36,11411.551807847052,2.2675933970460305,-22.20053697859889,-27.5807698921016,15.35,15.34,5.96,5.15,16.97,14.83,14.74,18.2,14.3,"none",50.6,99.990197039505929,1.02,"Dipole","No",546.79399673599471,2129.13,2143.5106863596875,546.79399673599471,0.99224137931034484]
["N1DPM 7 KLM mod",7.8310752000000008,12.09,7.827,6.7569999999999997,17.899999999999999,14293.724694049553,3.5222672064777338,-23.615802235042228,-28.996035148544944,14.98,14.89,5.87,5.07,16.37,14.5,14.22,16.91,12.88,"none","*198",99.572015023146136,1.1399999999999999,"*KLM Dual Dip","No",819.83805646153826,2340.08,2364.9797570850201,819.83805646153826,0.98799999999999999]
["YU7EF EF0607 10-14 el dia",7.9506336000000006,12.18,7.78,6.68,18.04,12097.021244353296,3.5632504886903482,-22.753568855657431,-28.133801769160144,15.09,15.02,5.84,5.01,16.489999999999998,14.57,14.32,17.07,13.72,"none",51.5,99.990197039505929,1.02,"Dipole","No",611.63776268725201,2172.9699999999998,2196.1061854230661,611.63776268725201,0.9878620689655172]
["M² 6M7",7.9506336000000006,12.32,7.91,6.8179999999999996,18.190000000000001,{"$f":"Z142/9000*J$8+(1-Z142/9000)*F$8+290*(1/AD142-1)","v":11854.759732562758},7.1941479963248618,-22.462980017438277,-27.843212930940986,15.23,15.19,5.9325000000000001,5.1150000000000002,16.97,14.77,14.65,16.920000000000002,19.71,"none",202.1,99.173553719008268,1.2,"T Match","Yes",588.33287975039923,2131.52,2177.2033359248003,588.33287975039923,0.97579310344827586]
["IZ1MYT 7",8.010412800000001,12.54,8.3800000000000008,7.38,18.47,16750.540783257627,5.2120190957596417,{"$f":"F143-10*LOG((Z143/9000*J$8+(1-Z143/9000)*F$8)+290*(10^(0.1*P$8)/AD143-1))+10*LOG(1/AD143)","v":-23.707332035974552},{"$f":"10*LOG(10^(F143/10)*1E-20/AD143/1.380649E-23/2500/(Z143/9000*J$8+(1-Z143/9000)*F$8+290*(10^(P$8/10)/AD143-1)))","v":-29.087564949477262},15.48,15.45,6.29,5.54,17.05,14.95,14.75,12.63,11.76,"none",52.6,99.017936855774693,1.22,"Dipole","No",1052.5269468982392,2513.75,2553.7163016006739,1052.5269468982392,0.98234482758620689]
["InnoV 6 LFA 8.2m Ver 3",8.2913750400000001,12.83,8.1910000000000007,7.1520000000000001,18.72,11509.50097430136,4.9842160645387672,-21.837488429236945,-27.217721342739651,15.74,15.72,6.14,5.36,17.47,15.24,15.17,24,14.2,"none",44.9,{"$f":"(1-((W144-1)/(W144+1))^2)*10^2","v":94.674556213017752},1.6,"LFA Loop","Yes",555.81982754982505,2119.39,2150.8316380217466,555.81982754982505,0.98310344827586205]
["Mosley A507LS",8.4886464000000004,10.26,6.7220000000000004,5.43,15.58,22051.843542323135,{"$f":"290*(1/AD145-1)","v":1.6392135104206429},-27.840783189607127,-33.221016103109832,13.07,12.73,5.04,4.07,15.08,12.77,12.86,13.4,13.36,"none",41.8,99.885644939205122,1.07,"*Gamma","No",1555.3058020146841,2946.51,2961.5258175260951,1555.3058020146841,0.99437931034482763]
["PY1MHZ 7 V1",8.5,12.59,8.34,7.2629999999999999,18.579999999999998,{"$f":"Z146/9000*J$8+(1-Z146/9000)*F$8+290*(1/AD146-1)","v":12444.445988562946},{"$f":"290*(1/AD146-1)","v":6.8741726529819775},{"$f":"F146-10*LOG((Z146/9000*J$8+(1-Z146/9000)*F$8)+290*(10^(0.1*P$8)/AD146-1))+10*LOG(1/AD146)","v":-22.28749749639881},{"$f":"10*LOG(10^(F146/10)*1E-20/AD146/1.380649E-23/2500/(Z146/9000*J$8+(1-Z146/9000)*F$8+290*(10^(P$8/10)/AD146-1)))","v":-27.66773040990152},15.57,15.57,6.2549999999999999,5.4450000000000003,17.440000000000001,15.11,15.02,24.2,13.5,"none",49.04,{"$f":"(1-((W146-1)/(W146+1))^2)*10^2","v":97.67308244757254},1.36,"Folded Dipole","Yes",644.25175171850969,2177.8110000000001,2222.5597543110293,{"$f":"(AB146-1700)*1.232876712","v":644.25175171850969},0.97684482758620694]
["DG7YBN GTV_50 7N MK2",8.5399999999999991,12.82,8.2799999999999994,7.18,18.745000000000001,10521.671181391164,4.3564758424685568,-21.433933963392651,-26.81416687689536,15.75,15.76,6.21,5.39,17.66,15.29,15.27,23.1,16.600000000000001,"none",49.3,98.63,1.45,"Bent Dipole","Yes",462.25602727399172,2177.8110000000001,2074.9409999999998,462.25602727399172,0.98519999999999996]
["PY1MHZ 7 V2",8.5500000000000007,12.6,8.3019999999999996,7.2350000000000003,18.579999999999998,12285.374298932922,5.8881746760534455,-22.246260158946846,-27.626493072449559,15.57,15.58,6.2264999999999997,5.4264999999999999,17.47,15.12,15.05,26.14,14.03,"none",49.04,96.626405664306532,1.45,"Folded Dipole","Yes",629.26890394178417,2177.8110000000001,2210.4070000000002,629.26890394178417,0.98009999999999997]
["PY1MHZ 7 V3",8.625,12.72,8.2650000000000006,7.2350000000000003,18.673999999999999,11539.092303852873,5.9787711777913799,-21.880038792684257,-27.260271706186966,15.67,15.66,6.2,5.43,17.39,15.18,15.04,23.1,14.27,"none",51.54,96.503404058430831,1.46,"Folded Dipole","Yes",558.53013683736026,2184.13,2153.0300000000002,558.53013683736026,0.9798]
["Directive DSEJX7-50",8.6930912639999995,12.83,8.4169999999999998,7.41,18.79,12319.074667576324,4.4368588733676573,-22.069361728190366,-27.449594641693071,15.77,15.76,6.6315,5.5575000000000001,17.52,15.36,15.03,15.94,13.5,"none",201.47,98.58526266762405,1.27,"T Match","Yes",632.60046628397868,2184.13,2213.1092672338341,632.60046628397868,0.98493103448275865]
["YU7EF 607",8.9071008000000003,12.73,8.1999999999999993,7.18,18.64,11510.613408088549,4.1176470588235414,-21.930621771119906,-27.310854684622612,15.66,15.63,6.15,5.39,17.16,15.14,14.91,16.309999999999999,14.62,"none",49.56,99.978160110655438,1.03,"Dipole","No",556.00739099902626,2124.9299999999998,2150.9837728194725,556.00739099902626,0.98599999999999999]
["G0KSC 7 8.9m LFA",8.9071008000000003,12.77,8.2650000000000006,7.2350000000000003,18.739999999999998,10883.524222328857,4.6431699541043052,-21.580818271504132,-26.961051185006838,15.73,15.73,6.2,5.43,17.62,15.23,15.3,24.99,14.86,"none",49.12,99.67960128159487,1.1200000000000001,"LFA Loop","Yes",496.52410985017667,2074.17,2102.7362225414286,496.52410985017667,0.98424137931034483]
["JK Antennas JK67 V2",9.0864384000000005,13.04,8.6150000000000002,7.5869999999999997,18.989999999999998,12054.686099646822,6.5339727090017856,-21.744886072749964,-27.125118986252676,15.99,15.68,6.4649999999999999,5.6924999999999999,17.86,15.53,15.45,20.53,16.21,20.93,51.71,95.480190960381918,1.54,"Dipole","No",607.3438199498778,2150.6999999999998,2192.6233207573782,607.3438199498778,0.97796551724137926]
["Create CL6DXZ 8el",9.1462175999999999,12.82,8.31,7.29,18.73,11943.600362367582,3.4608137343848289,-22.009899795710862,-27.390132709213574,15.77,15.71,6.23,5.47,17.149999999999999,15.21,14.95,18.260000000000002,12.8,"none",85.7,99.915166368177964,1.06,"Folded Dipole","Yes",597.10673902378676,2161.98,2184.3199106706679,597.10673902378676,0.98820689655172411]
["Directive DS50-7",9.3255552000000002,13.04,8.4550000000000001,7.45,18.96,11061.605150224314,3.8607218980397873,-21.442440057985806,-26.822672971488515,15.98,15.99,6.3449999999999998,5.5875000000000004,17.809999999999999,15.52,15.42,18.690000000000001,18.690000000000001,18.690000000000001,202.7,99.814564684874426,1.0900000000000001,"T Match","Yes",513.47619897784807,2092.4899999999998,2116.4862503930954,{"$f":"(AB155-1700)*1.232876712","v":513.47619897784807},0.9868620689655172]
["DK7ZB 7 28 ohm",9.3255552000000002,13.05,8.5739999999999998,7.5869999999999997,19.010000000000002,11896.856886627676,4.7154471544715708,-21.694506316804979,-27.074739230307689,16,15.99,6.43,5.69,17.64,15.49,15.3,20.11,13.42,"none",27.31,99.572015023146136,1.1399999999999999,"Dipole","No",592.55763432243941,2150.38,2180.6300813008133,592.55763432243941,0.98399999999999999]
["M² 6M7JHV",9.3255552000000002,13.11,8.5340000000000007,7.556,19.059999999999999,11122.812384354062,5.5543841152697588,-21.341450961797484,-26.721683875300194,16.04,16.04,6.3975,5.67,17.68,15.55,15.38,20.48,15.2,20.48,199.7,98.097502972651611,1.32,"T Match","Yes",519.11670179179771,2086.65,2121.0613248989634,519.11670179179771,0.98120689655172411]
["EAntenna 50LFA7",9.3255552000000002,12.85,8.1189999999999998,7.0990000000000002,18.77,9452.3064533514589,5.2638415897201529,-20.93275276425258,-26.312985677755286,15.8,15.8,6.09,5.3250000000000002,17.62,15.33,15.27,26.28,17.7,27.4,49.46,99.814564684874426,1.0900000000000001,"LFA Loop","Yes",360.81911863790708,1962.31,1992.6643963065685,360.81911863790708,0.98217241379310349]
["I0JXX 7JXX6",9.3793564800000002,13.53,9.4190000000000005,8.5340000000000007,19.53,14919.394915674407,7.8256250442665598,-22.108183030445552,-27.488415943948269,16.489999999999998,16.53,7.07,6.4,18.18,15.95,15.79,15.04,12.36,16.149999999999999,30.36,87.704503288918872,2.08,"*Hairpin","No",878.72918719114659,2356.9699999999998,2412.7470075784404,878.72918719114659,0.97372413793103452]
["InnoV 7el-Q",9.3853344000000014,13.62,9.3699999999999992,8.5950000000000006,19.57,13547.999990204235,5.0049109022028571,-21.692228953431432,-27.072461866934134,16.579999999999998,16.54,7.03,6.45,18.41,16.079999999999998,15.96,19.3,12.7,19,49.6,98.396292976869248,1.29,"LFA Vert Loop","Yes",749.02017390183528,2273.31,2307.5385856601656,749.02017390183528,0.98303448275862071]
["K1WHS 7 9.4m",9.3979999999999997,13.385,8.4550000000000001,7.4359999999999999,18.981999999999999,2099.8470000000002,{"$f":"290*(1/AD161-1)","v":3.0476960388035779},-21.444618394488145,-26.824851307990851,16.02,16.010000000000002,6.3449999999999998,5.58,17.82,15.55,15.45,19.079999999999998,18.18,"none",199,99.852071005917168,1.08,"T Match","NEC5",516.51862999924822,2151.1999999999998,2118.9540000000002,516.51862999924822,0.98960000000000004]
["G4CQM 6M7N50",9.6842304000000006,13.43,8.82,7.88,18.98,{"$f":"Z162/9000*J$8+(1-Z162/9000)*F$8+290*(1/AD162-1)","v":11882.418606221936},{"$f":"290*(1/AD162-1)","v":4.4162436548223161},-21.723647755292671,-27.103880668795377,16.350000000000001,16.329999999999998,6.62,5.91,17.95,15.84,15.68,18.8,15.3,20,52.1,95.61155462513085,1.53,"Dipole","No",591.21757859208117,2151.1999999999998,2179.5431472081218,{"$f":"(AB162-1700)*1.232876712","v":591.21757859208117},0.98499999999999999]
["InnoV 7 9.54m LFA2 WOS",9.5389999999999997,12.92,8.2279999999999998,7.1520000000000001,18.829999999999998,9417.3201475183068,{"$f":"290*(1/AD163-1)","v":4.7154471544715708},-20.864768896871425,-26.245001810374134,15.86,15.34,6.17,5.3639999999999999,17.71,15.4,15.68,24.37,20.3,"none",49.17,99.852071005917168,1.08,"LFA Loop","No",357.55520538410406,2151.1999999999998,1990.0170000000001,357.55520538410406,0.98399999999999999]
["G4CQM 6M7N50",9.6842304000000006,13.43,8.82,7.88,19.32,11882.418606221936,4.4162436548223161,-21.383647755292671,-26.76388066879538,16.350000000000001,16.329999999999998,6.62,5.91,17.95,15.84,15.68,18.8,15.3,20,52.1,95.61155462513085,1.53,"Dipole","No",591.21757859208117,2151.1999999999998,2179.5431472081218,591.21757859208117,0.98499999999999999]
["K6STI 6-6",9.6842304000000006,13.33,8.9540000000000006,8.0129999999999999,19.260000000000002,13264.951470163796,4.746433953667708,-21.914703510512826,-27.294936424015539,16.260000000000002,16.260000000000002,6.7119999999999997,6.0075000000000003,17.62,15.69,15.4,17.2,12.11,17.18,17.14,96.379222737628879,1.47,"Dipole","No",722.21825322126347,2253.66,2285.799249991238,722.21825322126347,0.98389655172413792]
["G0KSC 7 9.7m LFA",9.7440096,13.15,8.5,7.5,19.079999999999998,10231.162183983748,5.907955385102575,-20.955276264992285,-26.335509178494988,16.09,16.079999999999998,6.38,5.63,17.809999999999999,15.6,15.49,23.9,15.3,24.1,50.2,99.885644939205122,1.07,"LFA Loop","Yes",434.5754850188269,2017.3,2052.4890046092678,434.5754850188269,0.98003448275862071]
["G0KSC 8 OWL",9.8037887999999995,13.27,8.6560000000000006,7.68,19.149999999999999,10912.394109048442,9.2989074344282567,-21.114524839048659,-26.494757752551369,16.170000000000002,16.149999999999999,6.4950000000000001,5.76,17.91,15.69,15.58,19.899999999999999,16,20,12.4,99.67960128159487,1.1200000000000001,"Folded Dipole","Yes",498.81904817319008,2048.2199999999998,2104.5976725150358,498.81904817319008,0.96893103448275864]
["InnoV 8 OP-DES",9.863567999999999,13.16,8.2279999999999998,7.125,18.829999999999998,9406.5899046436953,4.220542961097113,-20.867102959153165,-26.247335872655874,16.07,16.05,6.17,5.34,17.82,15.59,15.53,23.82,18.64,23.82,50.5,99.961553248750477,1.04,"Bent Dipole","No",356.58513326814864,1964.855,1989.2301637279597,356.58513326814864,0.98565517241379308]
["*InnoV 8 OP-DES",9.863567999999999,13.16,9.0879999999999992,8.0830000000000002,19.010000000000002,11778.622485877642,4.3060012528127167,-21.657341082278933,-27.037573995781639,16.16,16.18,6.8174999999999999,6.06,18.39,15.78,15.76,23.82,18.64,23.82,50.5,99.961553248750477,1.04,"Bent Dipole","No",581.39056825635498,2144.0430000000001,2171.572349933685,581.39056825635498,0.9853689655172414]
["YU7EF EF0608E",9.9233472000000003,13.1,8.3780000000000001,7.3769999999999998,18.989999999999998,10283.26357525085,4.3544153162297334,-21.08995478722564,-26.470187700728353,16.02,16,6.2850000000000001,5.5350000000000001,15.54,15.53,15.41,20.350000000000001,17.899999999999999,20.399999999999999,50.29,99.915166368177964,1.06,"Dipole","No",439.6607249306191,2030.48,2056.613699205488,439.6607249306191,0.98520689655172411]
["G4CQM 6M7N50LY",9.9233472000000003,13.25,8.7799999999999994,7.68,19.16,11741.140544191763,2.8171024685770063,-21.515487382549153,-26.895720296051863,16.190000000000001,16.149999999999999,6.59,5.76,17.66,15.66,15.4,19.2,13.5,19.5,50.4,99.67960128159487,1.1200000000000001,"Dipole","No",577.97926469575282,2150.73,2168.8054037115699,577.97926469575282,0.99037931034482762]
["CC 617-6B mod G4CQM 7",9.9831263999999997,13.32,8.7390000000000008,7.7770000000000001,19.23,11830.069398890701,2.8884864526014931,-21.477050985436541,-26.857283898939247,16.239999999999998,16.23,6.59,5.76,17.690000000000001,15.71,15.46,19.2,13.38,19.2,50.4,99.627498953029601,1.1299999999999999,"Dipole","No",586.40088681489999,2157.04,2175.6362749878108,586.40088681489999,0.99013793103448278]
["Cushcraft 617-6B",10.1026848,12.34,8.1549999999999994,7.1120000000000001,18.12,16357.52367010237,1.3058538275025855,-24.012218175984476,-29.392451089487189,15.23,15.13,6.12,5.36,16.23,14.7,14.17,18.29,10.35,"none",197.36,99.386268555288922,1.17,"T Match","Yes",1015.6482766056636,2513.79,2523.8036023553859,1015.6482766056636,0.9955172413793103]
["N1DPM 7 CC617-6B mod",10.1026848,13.12,8.3780000000000001,7.3769999999999998,19.02,10188.637971199654,3.0313588850173967,-21.03948170709171,-26.419714620594416,16.04,16.04,6.29,5.54,17.79,15.56,15.47,20.71,17.149999999999999,22.28,20.7,98.58526266762405,1.27,"Dipole","No",430.81781287733497,2031.24,2049.4411149825783,430.81781287733497,0.98965517241379308]
["InnoV 8 OP-DES 4bay",10.19833152,13.55,9.0879999999999992,8.0830000000000002,19.5,11999.675171896819,4.0353821411090145,-21.25169275627097,-26.631925669773683,15.15,15.12,6.8174999999999999,6.06,16.899999999999999,14.67,14.6,20.5,14.1,19,50.2,99.885644939205122,1.07,"Bent Dipole","Yes",602.36687139639207,2162.5300000000002,2188.5864624851411,602.36687139639207,0.98627586206896556]
["InnoV 7 LFA 10.3m Ver 3",10.262893056000001,13.46,8.7390000000000008,7.7770000000000001,19.37,11238.68696513045,4.6741415557112553,-21.089127406756486,-26.469360320259195,16.39,16.38,6.56,5.84,18.05,15.88,15.76,21.53,13.9,21,47.06,98.491843644198212,1.28,"LFA Loop","Yes",530.18234427309017,2100.85,2130.0367904695163,530.18234427309017,0.98413793103448277]
["Cushcraft LFA-6M7EL",10.425492480000001,13.41,8.8659999999999997,7.91,19.38,11297.814228616726,4.2823150675344701,-21.107554543737539,-26.487787457240245,16.36,16.38,6.65,5.93,18.11,15.88,15.76,21.76,13.63,22.11,66.03,96.987910661840033,1.42,"LFA Loop","Yes",535.82337007100591,2107.77,2134.6122891734904,535.82337007100591,0.98544827586206896]
["YU7EF EF0608",11.21457792,13.43,8.6969999999999992,7.7130000000000001,19.34,10272.986873588892,4.3647182359117975,-20.735484568455711,-26.115717481958423,16.36,16.350000000000001,6.5220000000000002,5.7839999999999998,18,15.85,15.73,20.88,15.37,20.78,49.67,99.72821814424654,1.1100000000000001,"Dipole","No",438.68575608863551,2029.64,2055.8228911445572,438.68575608863551,0.9851724137931035]
["InnoV 8 LFA 11.71m",11.716723200000001,13.36,8.4600000000000009,7.47,19.22,8717.0656479388708,5.5751590341967683,-20.12867414502843,-25.508907058531143,16.28,16.25,6.35,5.6,18.02,15.8,15.73,29.1,20.9,25.1,50.5,99.978160110655438,1.03,"LFA Loop","Yes",291.1058803721786,1905.07,1936.1192141426211,291.1058803721786,0.98113793103448277]
["K5GW 8-6",11.716723200000001,13.92,9.5190000000000001,8.6969999999999992,19.920000000000002,12123.928591359279,5.4816948914342074,-20.855014242641339,-26.235247156144045,16.87,16.91,7.14,6.53,18.41,16.3,16.100000000000001,19.920000000000002,12.02,17.690000000000001,52.5,99.51325040562466,1.1499999999999999,"Dipole","No",614.0061296146863,2162.63,2198.0271941536084,614.0061296146863,0.98144827586206895]
["YU7EF EF0609X",11.896060800000001,13.75,8.9979999999999993,8.048,19.670000000000002,9991.7387052041286,4.3399924402570438,-20.285947413264289,-25.666180326766998,16.68,16.68,6.75,6.04,18.46,16.2,16.13,23.2,17.899999999999999,20.6,49.75,99.885644939205122,1.07,"Dipole","No",412.03231270929712,2008.4860000000001,2034.2039870644398,412.03231270929712,0.98525517241379312]
["BQH 8-6",11.95584,13.92,9.3699999999999992,8.5340000000000007,19.88,11215.928365178737,6.6385665408627155,-20.541654074615447,-25.921886988118157,16.850000000000001,16.88,7.0274999999999999,6.4005000000000001,18.32,16.29,16.079999999999998,20.22,12.97,17.13,49.75,99.72821814424654,1.1100000000000001,"Dipole","No",527.83917636626848,2087,2128.1362209445874,527.83917636626848,0.97762068965517246]
["M² 6M2WLC",11.95584,13.88,9.2739999999999991,8.3780000000000001,19.79,11363.380147005266,5.2949438202246757,-20.707717297135897,-26.087950210638606,16.79,16.8,6.95,6.29,18.28,16.25,16.079999999999998,18.7,14,17,197.1,98.491843644198212,1.28,"T Match","Yes",541.94152094213757,2106.41,2139.5747893258426,541.94152094213757,0.98206896551724143]
["*JK Antennas JK68 v2",12.135177599999999,14.1,8.5,8,19.670000000000002,10367.311832260822,5.1912951912952039,-20.43285357796405,-25.813086491466759,16.850000000000001,16.87,6.375,6,18.05,16.29,16.190000000000001,20.350000000000001,14.86,20.27,49.96,98.396292976869248,1.29,"Dipole","No",447.54722866075969,2031.83,2063.0105300105301,447.54722866075969,0.98241379310344823]
["JK Antennas JK68 v2",12.141155520000002,14.1,9.4689999999999994,8.6150000000000002,19.98,10833.485070299914,7.1626444295254572,-20.284117582104084,-25.664350495606794,17.02,17.03,7.1017000000000001,6.4649999999999999,18.600000000000001,16.489999999999998,16.329999999999998,20.350000000000001,14.86,20.27,49.96,98.396292976869248,"1.29","Dipole","No",491.54277414525598,2055.1,2098.6958058019154,491.54277414525598,0.97589655172413792]
["DK7ZB 8-6",12.254735999999999,14.02,9.4689999999999994,8.5739999999999998,19.97,10993.320652953802,5.9391934689281234,-20.375226461444139,-25.755459374946852,16.97,16.97,7.1,6.43,18.52,16.420000000000002,16.23,21.29,13.27,22.08,27.76,99.451303155006855,1.1599999999999999,"Dipole","No",506.80742560408453,2074.5300000000002,2111.0771342107114,506.80742560408453,0.97993103448275864]
["K6STI 7-6",12.254735999999999,14.29,9.9949999999999992,9.1340000000000003,20.27,12383.434137510005,6.5130627930754752,-20.581510694093975,-25.961743607596688,17.239999999999998,17.260000000000002,7.5,6.8470000000000004,18.7,16.64,16.43,19.27,12.3,16.829999999999998,12.57,90.957993055895159,1.86,"Dipole","No",638.50347169810823,2175.5500000000002,2217.8972605154604,638.50347169810823,0.9780344827586207]
["InnoV 8 LFA 12.2m Ver 3",12.324677664000001,13.96,9.1340000000000003,8.2279999999999998,19.86,10565.123984525009,4.385326239148684,-20.336315572307456,-25.716548485810165,16.88,16.87,6.8470000000000004,6.1719999999999997,18.47,16.350000000000001,16.23,23.78,14.43,20.399999999999999,49.76,98.852040816326536,1.24,"LFA Loop","Yes",466.37160830426228,2051.64,2078.2791935032205,466.37160830426228,0.98510344827586205]
["N6CA 8",12.3742944,14.1,9.52,8.66,20.04,10575.003253618137,9.6401467916058046,-20.083919719916643,-25.464152633419346,17.03,17.059999999999999,7.14,6.4950000000000001,18.690000000000001,16.510000000000002,16.39,21.83,21.69,30.7,21.5,99.247305102062086,1.19,"Dipole","No",466.8098984987235,2021.09,2078.6346955499339,466.8098984987235,0.96782758620689657]
["PY1MHZ 8",12.4,13.98,9.2279999999999998,8.34,19.899999999999999,9731.70791460285,6.7620822041553712,-19.906679405393163,-25.28691231889588,16.920000000000002,16.920000000000002,6.9210000000000003,6.2549999999999999,18.66,16.420000000000002,16.170000000000002,23.44,16.239999999999998,20.83,51.57,99.097070084560102,1.21,"LFA Loop","Yes",387.15788217763549,1974.7439999999999,2014.0280600722674,387.15788217763549,0.97721379310344825]
["InnoV 9 OP-DES",12.434073600000001,13.84,8.9499999999999993,7.98,19.690000000000001,9169.4578113753942,5.1498561100582663,-19.883262324073119,-25.263495237575832,16.739999999999998,16.71,6.71,5.99,18.45,16.260000000000002,16.18,24.45,17.7,24.7,49.3,99.72821814424654,1.1100000000000001,"Bent Dipole","Yes",334.02244731874504,1941.6,1970.9293184530077,{"$f":"(AB191-1700)*1.232876712","v":334.02244731874504},0.98255172413793102]
["G0KSC 8 12.49m LFA",12.493852799999999,14.03,9.2739999999999991,8.3780000000000001,19.95,9544.8694598971506,6.5130627930754752,-19.776599085289636,-25.156831998792342,16.96,16.96,6.95,6.29,18.71,16.48,16.399999999999999,24.37,16.329999999999998,21.24,48.8,99.627498953029601,1.1299999999999999,"LFA Loop","Yes",369.47354226976279,1962.13,1999.6840954765012,369.47354226976279,0.9780344827586207]
["EAntenna 50LFA8",12.493852799999999,13.93,9.0429999999999993,8.1549999999999994,19.8,9258.3444382235848,5.2120190957596417,-19.813998495152457,-25.194231408655167,16.84,16.829999999999998,6.78,6.12,18.489999999999998,16.329999999999998,16.239999999999998,25.58,16.2,22.38,48.69,99.51325040562466,1.1499999999999999,"LFA Loop","Yes",342.44094115575427,1947.96,1977.7576523448472,342.44094115575427,0.98234482758620689]
["M² 6M7NAN",12.493852799999999,14.04,9.6720000000000006,8.8230000000000004,19.96,{"$f":"Z194/9000*J$8+(1-Z194/9000)*F$8+290*(1/AD194-1)","v":12612.916672427411},8.5233565242084595,-20.941684965146617,-26.32191787864933,16.95,16.98,7.2525000000000004,6.6150000000000002,18.27,16.350000000000001,16.11,18.3,12.37,17.32,16.920000000000002,93.703095849289511,1.67,"*Hairpin","No",660.06255100177782,2179.84,2235.3840692886556,660.06255100177782,0.97144827586206894]
["Cushcraft LFA-6M8EL",12.595477440000002,13.96,9.4689999999999994,8.6150000000000002,20.02,9674.8804571494766,4.684466869897312,-19.791727476990825,-25.171960390493538,17.010000000000002,17.03,7.1,6.46,18.86,16.53,16.23,23.62,14.01,22.43,53.3,99.386268555288922,1.17,"LFA Loop","Yes",381.9688701823527,1982.48,2009.8191947860823,381.9688701823527,0.98410344827586205]
["YU7EF EF0609",12.912307200000001,13.99,9.1340000000000003,8.2650000000000006,19.89,9656.3442036523247,4.0251022620005266,-19.923119137978947,-25.303352051481657,16.91,16.920000000000002,6.85,6.2,18.600000000000001,16.399999999999999,16.32,21.56,16.84,19.559999999999999,49.19,99.814564684874426,1.0900000000000001,"Dipole","No",380.27455678720429,1984.92,2008.4449183652066,380.27455678720429,0.98631034482758617]
["DG7YBN 50-9w",12.912307200000001,13.99,9.0879999999999992,8.1910000000000007,19.86,9293.1899968854686,2.7559438855431995,-19.8062840852653,-25.186516998768006,16.899999999999999,16.88,6.82,6.04,18.66,16.489999999999998,16.05,24.27,17.29,20.37,50.16,99.67960128159487,1.1200000000000001,"Dipole","No",345.97626871313537,1964.71,1980.625195808821,345.97626871313537,0.99058620689655175]
["M² 6M8GJ",13.031865600000001,14.27,9.68,8.42,20.14,10545.179335145724,7.0786675615528232,-20.008807114610928,-25.389040028113634,17.2,17.14,7.26,6.32,18.63,16.649999999999999,16.420000000000002,18.850000000000001,15.05,16.739999999999998,16.399999999999999,97.222222222222214,1.4,"*Hairpin","No",464.22605316193687,2033.97,2076.5389098873147,464.22605316193687,0.97617241379310349]
["*M² 6M8GJ",13.031865600000001,14.27,9.1440000000000001,9.1440000000000001,20.2,10786.936666481761,7.1206500618265363,-20.046123989861449,-25.426356903364159,17.2,17.14,7.26,6.32,18.63,16.649999999999999,16.420000000000002,18.3,15.05,16.739999999999998,16.399999999999999,97.222222222222214,1.4,"*Hairpin","No",487.13504789152705,2051.86,2095.1206500618264,487.13504789152705,0.9760344827586207]
["ZL3NW 10",13.151424,13.81,9.18,8.3019999999999996,19.739999999999998,11279.129446317384,5.4609331084879154,-20.723127326918931,-26.103360240421637,16.68,16.78,6.89,6.2220000000000004,18.32,16.2,16.010000000000002,16.54,15.75,19.13,64.13,99.572015023146136,1.1399999999999999,"Dipole","No",533.94078158045556,2099.02,2133.0853007307478,533.94078158045556,0.98151724137931029]
["BQH 9-6D",13.611723840000002,14.34,10.050000000000001,9.2270000000000003,20.37,12075.827036170864,4.4884095524896939,-20.40238521563267,-25.782618129135379,17.37,17.39,7.46,6.82,18.95,16.809999999999999,16.649999999999999,22.62,11.75,16.2,49.96,99.67960128159487,1.1200000000000001,"Dipole","No",609.54136098952574,2165.38,2194.4057707122347,609.54136098952574,0.98475862068965514]
["DK7ZB 9 28 ohm",13.9883328,14.49,10.16,9.3699999999999992,20.51,11163.642128584617,6.7955957086391656,-19.889174846170611,-25.269407759673324,17.46,17.5,7.62,7.0270000000000001,19.190000000000001,16.920000000000002,16.809999999999999,20.100000000000001,13.25,16.98,27.95,99.885644939205122,1.07,"Dipole","No",522.86877417737776,2082.11,2124.1046725014121,522.86877417737776,0.97710344827586204]
["JK Antennas JK610 2021",14.347008000000001,14.35,9.6199999999999992,8.7810000000000006,20.28,9391.2377704664359,6.2143732653320232,-19.380892256963293,-24.761125170466009,17.28,17.3,7.2149999999999999,6.58575,19.09,16.809999999999999,16.920000000000002,21.21,20.75,21.14,48.54,98.298676748582224,1.3,"Dipole","Yes",354.941139161857,1952.2760000000001,1987.8967018413898,354.941139161857,0.97902068965517242]
["JK Antennas JK610 v8",14.579549087999998,14.57,9.7769999999999992,8.9540000000000006,20.49,8850.2907631810485,6.774648881360732,-18.906652725060418,-24.286885638563124,17.5,17.510000000000002,7.3319999999999999,6.585,19.23,17,16.920000000000002,25.84,16.899999999999999,19.55,46.43,98.76543209876543,1.25,"Dipole","No",303.61883981357613,1908.46,1946.2686145811278,303.61883981357613,0.97717241379310349]
["InnoV 10 OP-DES",14.944800000000001,14.32,9.32,8.3800000000000008,20.149999999999999,8324.6855044763724,5.4713136352457532,-19.001465164539152,-24.381698078041861,17.32,17.28,6.99,6.29,19.04,16.84,16.78,26.6,19.399999999999999,24.8,50.4,99.773242630385482,1.1000000000000001,"Bent Dipole","No",253.92720848325749,1876.04,1905.9631802691213,253.92720848325749,0.98148275862068968]
["Create CL613 13 el",15.004579199999998,14.69,10.16,9.4190000000000005,20.68,10810.298774384515,3.5120231738386543,-19.628268719863648,-25.008501633366347,17.75,17.670000000000002,7.63,7.07,19.07,17.010000000000002,16.88,19.940000000000001,12.4,16.18,90.19,99.915166368177964,1.06,"Folded Dipole","Yes",489.69124642898157,2075.5700000000002,2097.1940110983146,489.69124642898157,0.98803448275862071]
["M² 6M9KHW",15.004579199999998,14.87,10.53,9.73,20.86,10870.720587270165,7.5937721160651295,-19.41267856155326,-24.792911475055973,17.829999999999998,17.86,7.9,7.3,19.48,17.27,17.16,20.5,13.6,17.5,50,99.097070084560102,1.21,"*Hairpin","No",495.03097447753703,2055.3000000000002,2101.5251238499645,495.03097447753703,0.97448275862068967]
["PY1MHZ 9",15.004579199999998,14.65,9.9949999999999992,9.1340000000000003,20.59,9272.2976162522027,6.8280691351749905,{"$f":"F208-10*LOG((Z208/9000*J$8+(1-Z208/9000)*F$8)+290*(10^(0.1*P$8)/AD208-1))+10*LOG(1/AD208)","v":-19.006932248459133},{"$f":"10*LOG(10^(F208/10)*1E-20/AD208/1.380649E-23/2500/(Z208/9000*J$8+(1-Z208/9000)*F$8+290*(10^(P$8/10)/AD208-1)))","v":-24.387165161961839},17.59,17.600000000000001,7.18,6.56,19.18,17.03,16.96,24.2,17.29,20.68,50.25,98.097502972651611,1.32,"Folded Dipole","Yes",343.61021402751942,1939.86,1978.7060625633096,343.61021402751942,0.97699655172413791]
["G0KSC 9 LFA 15.02m",15.004579199999998,14.47,9.5690000000000008,8.7390000000000008,20.350000000000001,8334.6689162930197,6.5130627930754752,-18.791452328844287,-24.171685242346999,17.39,17.39,7.18,6.56,19.11,16.899999999999999,16.829999999999998,23.07,18.86,22.61,50.2,{"$f":"(1-((W209-1)/(W209+1))^2)*10^2","v":99.773242630385482},1.1000000000000001,"LFA Loop","Yes",254.77467019270748,1871.14,1906.6505658780807,254.77467019270748,0.9780344827586207]
["EAntenna 50LFA9",15.0643584,14.6,9.6720000000000006,8.8659999999999997,20.47,8396.7658048773246,6.1059080346454264,-18.709403398116297,-24.08963631161901,17.5,17.489999999999998,7.2519999999999998,6.6520000000000001,19.22,17.010000000000002,16.940000000000001,24.12,17.7,21.8,48.45,99.67960128159487,1.1200000000000001,"LFA Loop","Yes",260.69860016411235,1878.02,1911.4555313006126,260.69860016411235,0.97937931034482761]
["K6STI 8",15.1839168,14.88,10.61,9.8849999999999998,20.87,11633.441728754542,5.8038760507896185,-19.721789795326433,-25.102022708829143,17.82,17.89,7.9574999999999996,7.4175000000000004,19.260000000000002,17.2,17.05,19.29,12.15,16.05,15.95,92.993079584775089,1.72,"Dipole","No",567.48884450646358,2123.6,2160.296507333544,567.48884450646358,0.98037931034482761]
["M² 6m25WLC",15.363254399999999,14.78,10.4,9.6460000000000008,20.8,11183.28329461216,4.9738697344884564,-19.633377385653407,-25.013610299156113,17.739999999999998,17.78,7.8,7.24,19.420000000000002,17.18,17.09,19.920000000000002,13.6,15.84,197.1,98.491843644198212,1.28,"T Match","Yes",524.90295728621561,2094.8000000000002,2125.754621023465,524.90295728621561,0.98313793103448277]
["InnoV 10 LFA",15.4230336,14.05,9.0429999999999993,8.1549999999999994,19.86,8459.2593298501033,{"$f":"290*(1/AD213-1)","v":5.4920768771300992},-19.360347820287309,-24.740580733790019,16.940000000000001,16.91,6.78,6.12,18.739999999999998,16.46,16.41,27.9,20.6,26.4,47.86,99.67960128159487,1.1200000000000001,"LFA Loop","Yes",266.67971015961206,1886.08,1916.3068760760339,266.67971015961206,0.98141379310344823]
["YU7EF EF0610",15.4828128,14.62,9.7769999999999992,8.9540000000000006,20.53,8612.017219488398,6.6176418721123138,-18.751164307122377,-24.131397220625082,17.600000000000001,17.600000000000001,7.54,6.85,19.510000000000002,17.149999999999999,17.09,24.17,17.420000000000002,22.82,50.5,99.885644939205122,1.07,"Dipole","No",281.05092879682587,1891.42,1927.9635311959935,281.05092879682587,0.9776896551724138]
["Directive DSEJX13-50",15.506126688,14.62,10.220000000000001,9.4939999999999998,20.59,11232.21020288549,4.6741415557112553,-19.866636198406855,-25.246869111909554,17.55,17.579999999999998,7.665,7.1204999999999998,19.239999999999998,17.010000000000002,16.91,17.399999999999999,12.1,17.399999999999999,202,99.885644939205122,1.07,"T Match","Yes",529.56849780926711,2100.36,2129.5388927820604,529.56849780926711,0.98413793103448277]
["G0KSC 10LFA-HZE",17.694643200000002,15.12,10.23,9.4689999999999994,21.02,7620.5805125837223,6.7851219253978616,-17.731205504610983,-23.111438418113693,18.03,18.04,7.67,7.1,19.77,17.54,17.48,26.5,18.41,23.25,50.3,99.852071005917168,1.08,"LFA Loop","Yes",187.06990855017813,1816.03,1851.7344814200515,187.06990855017813,0.97713793103448277]
["G0KSC 11 OWL-FD",17.933759999999999,15.28,10.49,9.7240000000000002,21.18,7873.9386839425388,7.341253005232633,-17.704153702419713,-23.084386615922419,18.2,18.21,7.8674999999999997,7.29,19.96,17.71,17.64,23.4,16.27,17.98,49.08,99.572015023146136,1.1399999999999999,"Folded Dipole","Yes",211.02966384199408,1832.13,1871.168505161929,211.02966384199408,0.97531034482758616]
["EAntenna 50LFA10",18.232655999999999,15.18,10.220000000000001,9.4689999999999994,21.05,7661.1206612974293,6.774648881360732,-17.724232631277729,-23.104465544780442,18.04,18.059999999999999,7.665,7.1020000000000003,19.75,17.55,17.489999999999998,25.87,18.100000000000001,22.6,48.91,99.572015023146136,1.1399999999999999,"LFA Loop","Yes",190.91316461399137,1819.13,1854.8517891170868,190.91316461399137,0.97717241379310349]
["YU7EF EF06011",18.710889599999998,15.27,10.41,9.6300000000000008,21.15,7832.6014588972866,6.5967201551754773,-17.722266672369638,-23.102499585872344,18.18,18.18,7.81,7.22,19.91,17.690000000000001,17.62,23.4,18.22,23.2,50,99.915166368177964,1.06,"Dipole","No",207.18242047892801,1832.95,1868.0479633221655,207.18242047892801,0.97775862068965513]
["G0KSC 11 BV LFA",20.1455904,15.78,10.97,10.25,21.63,7669.6723067770581,5.5336121165266983,-17.16711025980868,-22.547343173311386,18.64,18.66,8.23,7.69,20.37,18.14,18.079999999999998,26,16,23.5,47.1,99.773242630385482,1.1000000000000001,"LFA Loop","Yes",191.84128319234188,1826.29,1855.6045964086163,191.84128319234188,0.98127586206896555]
["M² 6M11JKV",21.042278400000001,16.010000000000002,12.01,11.36,21.89,13537.654140765713,3.9942669370062633,-19.383767765297026,-24.764000678799736,18.96,18.91,9.0075000000000003,8.52,20.75,18.43,18.440000000000001,19.2,14,15.7,194.3,97.888815837533784,1.34,"T Match","Yes",748.13541348418664,2279.42,2306.8209466545482,748.13541348418664,0.98641379310344823]
["InnoV 12 LFA",22.835654399999999,16.12,11.54,10.84,22.03,7975.2399670560135,6.7118261360428688,-16.918420040194803,-22.298652953697513,19.04,19.04,8.66,8.1300000000000008,20.75,18.53,18.47,26.2,15.4,21.9,47.9,99.51325040562466,1.1499999999999999,"LFA Loop","Yes",220.6903250661303,1843.06,1879.0043748235958,220.6903250661303,0.97737931034482761]
["DK7ZB 13",25.465939199999998,16.7,13.28,12.71,22.71,10991.641701807108,7.5306021368428233,-17.611392859923985,-22.991625773426691,19.68,19.68,9.9600000000000009,9.5299999999999994,21.49,19.11,19.100000000000001,22.87,12.42,15.88,27.87,99.51325040562466,1.1499999999999999,"Dipole","No",506.49747153572429,2064.7399999999998,2110.8257270218633,506.49747153572429,0.97468965517241379]
["BVO 18 Rope Yagi",30.068937600000002,17.27,13.49,12.89,23.2,10729.255682909828,0.43063853299722732,-17.121355483070005,-22.501588396572714,20.27,20.260000000000002,10.119999999999999,9.67,21.81,19.54,19.52,25.8,12.9,16.899999999999999,51.06,99.67960128159487,1.1200000000000001,"Dipole","No",482.30228937859613,2088.5300000000002,2091.200745933626,482.30228937859613,0.99851724137931031]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"-"]
["Only Antennas that have actually been built are posted in these Tables, except for the F5FOD Isotropic Lossless Radiator."]
[]
["Thanks to Vladimir, UR5EAZ for establishing the Interactive Mode in the 50,144 and 432 Tables"]
["Thanks to Hartmut,  DG7YBN for his ongoing support and many inputs to the Tables"]
[]
["Legend:"]
[]
["1. L      = Length in Wavelengths"]
[]
["2. Gain  = Gain in dBd of a single antenna"]
[]
["3. E      = E plane (Horizontal) stacking in Meters. "]
[]
["4. H      = H plane (Vertical) stacking in Meters."]
[]
["5. Ga     = Gain in dBd of a 4 bay array"]
[]
["6. Tloss = Noise temperature due to ohmic losses in the antenna (K) at an actual antenna temperature of 290 K."]
[]
["7. Ta     = Noise temperature of the antenna array (K) is the mixture of the antenna array pattern, the sky temperature, "]
["               ground and the ohmic losses in the antenna array."]
[]
["8. F/R    = Front to Rear in dB over the rear 180 degrees of an antenna using either E or H plane. "]
[]
["9. Z ohms = The natural impedence of a single antenna in free space.  "]
[]
["10. VSWR  = VSWR Bandwidth is based a single antenna over 50.0 - 50.3 MHz with a "]
["                    reference at 50.150 MHz. This parameter gives an indicator of the"]
["                    antenna \"Q\" and what to expect with with stacking and wet weather.  "]
[]
["11. G/T = Figure of merit; a system parameter used to determine the receive capability of the antenna or array"]
["               as part of the radio receiving system.The more positive level the better."]
[]
["12. S/N = Figure of merit; a system parameter used to determine the receive capability of the antenna or array"]
["               as part of the radio receiving system.The more positive level the better."]
[]
["13. e   = Radiation Efficiency; a system parameter which describes how efficiently an antenna transmits and receives signals."]
[]
["Notes:"]
[]
["1. The programs used to calculate E/H Stacking,G,Ta,Tlos and Ant G/T are"]
["    EZNEC 5+ by Roy Lewallen W7EL,4NEC2 by Arie Voors and Tant.exe by Sinisa, YT1NT/VE3EA or AGTC_lite by F5FOD/DG7YBN "]
["    This combination of software provides excellent accuracy."]
[]
["2. Temperatures initially used for producing Antenna Temperature: Tsky=4225 Kelvin;Tearth=6000 Kelvin"]
["    Temperatures now adjustable to Tsky=5640 Kelvin. Tearth: Rural = 29640 Kelvin, Residential = 100600 Kelvin, City=271000 Kelvin"]
[]
["3. One wavelength at 50.150 MHz is 5.98M or 19.62'"]
[]
["4. \"E\" represents the horizontal plane; \"H\" represents the vertical plane."]
[]
["5. F/R is Front to Rear in dB over the rear 180 degrees of an antenna using either E or H plane. "]
[]
["6. Z ohms is the natural impedence of a single antenna in free space.  "]
["   "]
["7. VSWR Bandwidth is based a single antenna over 50.000 - 50.300 MHz with a reference of 1.00:1 at 50.150 MHz"]
[]
["8. Ant G/T = Figure of merit used to determine the receive capability of the antenna"]
["                     or array. Ant G/T (dB) = Ga - 10*log(Ta). The more positive figure the "]
["                     better. Ant G/T is modelled in Tant.exe or AGTC_2lite at 30 degrees elevation."]
[]
["9. Antennas marked with a \"*\" have stacking dimensions recommended by "]
["   the manufacturer or designer."]
[]
["10. Force 12 antennas are not included as no data is available from the manufacturer."]
[]
["11. FD = Folded Dipole"]
[]
["12.  Convergence Correction: NEC2 and NEC 4 are incapable of handling complex "]
["      feed systems like Folded Dipoles, T Matches, LFAs etc."]
["      Convergence Correction using the KF2YN Excel program is required. "]
["      See DUBUS 4/2010 \"The Correction of Convergence Errors in Antenna"]
["      Temperature Calculations by Brian Cake, KF2YN for details."]
[]
["13. Earth Temperature Definition"]
["       Rural: Open countryside with largely agricultural activity, building density < 1/ha, no major roads, no electrified railways."]
["       Residential: Villages and pure residential areas with no commercial or industrial activities. No electrified railways and no major roads and no high voltage overhead lines or facilities within 1 km."]
["       City: Dense commercial or industrial buildings and offices. Major roads and railways can be in the vicinity, but should not be dominating."]
[]
["14. Manufacturer/Designer Legend: Single click on Sites in blue"]
[]
["Antennas-Amp  = Antennas-Amplifiers"]
["BVO                 = Eagle/DJ9BV"]
["BQH             = VE7BQH"]
["Cushcraft          = Cushcraft"]
["Create          = Create"]
["Directive           = Directive"]
["DK7ZB              = DK7ZB"]
["EAntenna          = EAntenna"]
["F9FT                = F9FT"]
["G0KSC             = G0KSC"]
["G4CQM             = G4CQM"]
["HyGain              = HyGain"]
["I0JXX                = I0JXX"]
["InnoV                =   InnoVAntennas"]
["IZ1MYT         = IZ1MYT"]
["JK Antennas     = JK Antennas"]
["K5GW           = K5GW"]
["K6STI               = K6STI"]
["M²                     = M²"]
["Maple Leaf        = Maple Leaf"]
["Mosley          = Mosley"]
["N1DPM          = N1DPM"]
["N6CA                = N6CA"]
["OZ3SW         = OZ3SW"]
["Telrex           = Telrex"]
["Tilton            = Tilton (ARRL Handbook)"]
["W5WVO Mod = W5WVO"]
["WiMo            = WiMo"]
["YU7EF             = YU7EF"]
["ZL3NW            = ZL3NW"]
[]
["Using this Chart:"]
[]
["Antennas with good G/T can provide significant benefit with today's high noise levels. "]
["Other factors like ease of matching and wet weather performance should be considered in the the decision making. "]
["Antennas with 50 ohm feed systems and good VSWR bandwidth (Q) may be the best feed system choice. "]
[]
["Stacking is an issue on this band due to the large optimum spacings. While the longer antennas are very attractive "]
["because of there superior gain, if severly understacked, the gain advantage may be quickly lost.  "]
[]
[]
[null,null,null,null,"Lionel H. Edwards"]
[null,null,null,null,"VE7BQH"]
[null,null,null,null,"Issue 47, July 2, 2024"]
[]
[]
["Issue   1: Initial Issue"]
["Issue   2: Add Cushcraft 617-6B and M² 6M25WLC "]
["Issue   3: Add N1DPM 7 617-6b mod, N1DPM 7 KLM mod, N1DPM 5 Hy-gain mod"]
["Issue   4: Add G0KSC 6 6.8m LFA,G0KSC 6 7.3m LFA,G0KSC 7 9.7m LFA,G0KSC 7 8.9m LFA,G0KSC 8 12.49m LFA"]
["Issue   5: Add G4CQM 6, G0KSC 5 4.4m LFA, Add F/R column "]
["Issue   6: Add M² 6M3"]
["Issue   7: Add M² 6M5XHG, IZ1MYT 6"]
["Issue   8: Add G0KSC 8 OWL, IZ1MYT 7,G4CQM 5,Revised G4CQM 6"]
["Issue   9: Add Create CL6DX,Create CL6DXX,Create CL613"]
["Issue 10: Add G0KSC 3LFA,WiMo ZX 6-6,M² 6M5,Create CL6DXZ,"]
["Issue 11: Add G0KSC 4LFA,"]
["Issue 12: Add IZ1MYT 5, G0KSC 10LFA, G0KSC 11OWL"]
["Issue 13: Add G0KSC 5 4.6m LFA,G0KSC 5 4.7m LFA,G0KSC 6 6.0m LFA,G0KSC 6.2m LFA,G0KSC 6 6.4m LFA,G0KSC 9 15.02m LFA"]
["Issue 13: Add G0KSC 6 LFA 6.0m updated"]
["Issue 14: Add G0KSC 5 LFA 4.9m,OptiBeam OB6-6"]
["Issue 15: Add YU7EF 3, YU7EF 11"]
["Issue 16: Add F9FT 5 220505"]
["Issue 17: Add InnoV 5 OP-DES,InnoV 6 OP-DES,InnoV 7 OP-DES,InnoV 8 OP-DES,InnoV 10 LFA,InnoV 8 LFA,InnoV 6 LFA 6.83,"]
["Issue 17: Add InnoV 6 6.4m ,InnoV 6 LFA 6.1m, InnoV 4 LFA 3.33m,InnoV 4 LFA 2.8m,InnoV 3 OWL,InnoV 2 LFA,"]
["Issue 18: Add Updated DK7ZB 5 50 ohm,"]
["Issue 19: Add G4CQM 6M7UX,G4CQM 6M7N50,"]
["Issue 20: Add UA9TC 7RV,G0KSC 11 BV LFA,HyGain VB-66DX(new),HYGain VB-66B(old)"]
["Issue 21: Add InnoV 6 LFA MAX 5.8m,InnoV 9 OP-DES,Innov 10 OP-DES, G4CQM 7 LY,G0KSC 2el-Q,G0KSC 3el-Q,"]
["Issue 22: Add InnoV 12 LFA,G0KSC 4el-Q,G0KSC 5el-Q,G0KSC 6el-Q,"]
["Issue 23: Add DK7ZB 6 50ohm,"]
["Issue 24: Add YU7EF 8,G0KSC 3 Quad,G0KSC 4 Quad, G0KSC 5 Quad,"]
["Issue 25: Add DK7ZB 4"]
["Issue 26: Add EAntenna 50LFA3,EAntenna 50LFA 4,EAntenna 50LFA5S,EAntenna 50LFA5,EAntenna 50LFA5XL,EAntenna 50LFAA6S,"]
["Issue 26: Add EAntenna 50LFA6M,EAntenna 50LFA6,EAntenna 50LFA6XL,EAntenna 50LFA7,EAntenna 50LFA8,"]
["Issue 26: Add EAntenna 50LFA9,EAntenna 50LFA10,"]
["Issue 27: Add InnoV 2 LFA-Q,InnoV 3 LFA-Q,InnoV 4 LFA-Q,InnoV 5 LFA-Q,"]
["Issue 28: Add Revise InnoV 6 LFA 6.4m,InnoV 5 LFA,DK7ZB 13 (50MHz),"]
["Issue 29: Add Directive DSEJX5-50,Directive DSEJX6-50,Directive DSEJX7-50,Directive DSEJX13-50,"]
["Issue 29: Add Revise HyGain VB-66DX,HyGain 66B,HyGain VB-64DX,"]
["Issue 30: Add Super Moxon,"]
["Issue 31: Add InnoV 4 LFA 3.9m Ver 3,InnoV 5 LFA 6.2m Ver 3,InnoV 6 LFA 8.2m Ver 3,InnoV 7 LFA 10.3m Ver 3,InnoV 8 LFA 12.2m Ver 3,"]
["Issue 32: Add JK Antennas JK65,JK Antennas JK67,"]
["Issue 33: Add Maple Leaf BFM-4e6-13,"]
["Issue 34: Add JK68v2,JK610 v8,"]
["Issue 35: Add Interactive Tsky and Tearth"]
["Issue 36: Add M² 6M7NAN,BQH9-6D,DG7YBN 50-9w,",null,null,null,null,"CC617-6B mod G4CQM 7"]
["Issue 37: Add Tearth Kelvin updated,Cushcraft LFA-6M4EL,Cushcraft LFA-6M5EL,Cushcraft LFA-6M7EL,Cushcraft LFA-6M8EL,"]
["Issue 38: Add G4CQM WS66082,G4CQM WS65065,"]
["Issue 39: Add YU7EF 0609X,"]
["Issue 40: Add InnoV 5 LFA-HG,JK Antennas JK610 2021,PY1MHZ 2,PY1MHZ 3,PY1MHZ 4,PY2MHZ 5,PY1MHZ 6,PY1MHZ 7,PY1MHZ 8,PY1MHZ 9,"]
["Issue 41: Add PY1MHZ 7 V2,"]
["Issue 42: Add PY1MHZ 2 V2,PY1MHZ 7 V3,PY1MHZ 6 V2,DG7YBN YBN50-5w,DG7YBN YBN50-5wrc vs,"]
["Issue 43: Add Receive System NF Thanks to Vladimir UR5EAZ"]
["Issue 43: Charts for all 3 bands have been revised to be more readable.Thanks to Hartmut,DG7YBN"]
["Issue 44: Add Signal to Noise (S/N)"]
["Issue 45: Add InnoV 7 9.54m LFA WOS,"]
["Issue 46: Add K1WHS 7 9.4m,DG7YBN GTV_50 7N MK2,"]
["Issue 47: Add Radiation Efficiency. Thanks to Vladimir UR5EAZ"]

{"sheet":"NF Calculator","index":3,"n_rows":24,"n_cols":4,"rows_kept":24,"cut":false,"hidden":false,"merged":[[16,0,16,3]]}
[]
["       Receive System NF Calculator"]
[]
[null,"             USER INPUT"]
[]
[" *Transmission Line1 Loss:",null,0.4,"dB"]
[]
["             LNA Noise Figure:",null,0.5,"dB"]
[]
["                         LNA Gain:",null,22,"dB"]
[]
["   Transmission Line2 Loss:",null,1,"dB"]
[]
["       Receiver Noise Figure:",null,6,"dB"]
[]
[]
["CALCULATION RESULT"]
[]
["          Receive System NF:",null,{"$f":"10*LOG(10^(C6/10)+(10^(C8/10)-1)*10^(C6/10)+(10^(C12/10)-1)*10^(C6/10)/10^(C10/10)+(10^(C14/10)-1)*10^(C6/10)/10^(C10/10)*10^(C12/10))","v":0.99688976910832561},"dB"]
[]
[]
["Actual temperature of the transmission lines is 290 K."]
["*The transmission line contains all the components connected between the antenna terminals and the LNA input (connectors, relays, coaxial cables etc)."]
["If LNA is not used, set LNA Noise Figure = 0 dB, LNA Gain = 0 dB."]

{"sheet":"Convergence Correction","index":4,"n_rows":59,"n_cols":12,"rows_kept":59,"cut":false,"hidden":false,"merged":[[3,1,3,4],[29,1,29,4]]}
[]
[null,"Correction of convergence errors"]
[]
[null,"Author: Brian V. Cake KF2YN",null,null,null,"( ... formatted by DG7YBN)"]
[]
[null,"Enter the data from EZNEC or TANT in cells F11 thru F13 and M11 thru M13 (Simply type over the example data)"]
[null,"Excel will automatically compute the true gain, G and the true G/Ta"]
[null,null,null," "]
[null,"ZERO Loss:",null,null,null,null,null,"With Loss:"]
[]
[null,"Gain (Go)",null,null,20.04,"dBi",null,"Gain (Gl)",null,null,20.010000000000002,"dBi"]
[null,"Average gain (Ko)",null,null,0.99980000000000002,"/",null,"Average gain (Kl)",null,null,0.99239999999999995,"/"]
[null,"Pattern temp. (T_Pattern), (Tpo)",null,null,34.749000000000002,"K",null,"Pattern temp. (T_Pattern), (Tpl)",null,null,34.750999999999998,"K"]
[]
[]
[null,"Corrrected numbers:"]
[]
[null,"Ta, antenna temp (T_total)",null,null,{"$f":"E13*K12/E12+290*(1-K12/E12)","v":36.638235247049415},"K"]
[]
[null,null,null,"Gain",{"$f":"10*LOG(10^(0.1*E11)*K12/E12^2)","v":20.008604907670286},"dBi"]
[null,null,null,"G/T",{"$f":"10*LOG(10^(0.1*E11)*K12/E12^2)-10*LOG(E18)","v":4.3692594391876458},"dB"]
[null,null,null,"T_loss",{"$f":"((1-K12/E12))*290","v":2.1464292858571818},"K"]
[null,null,null,"Avg Gain",{"$f":"K12/E12","v":0.99259851970394075},"/"]
[null,null,null,"T_pattern",{"$f":"E13","v":34.749000000000002},"K"]
[]
[]
[]
[null,"Convergence Error Correction Algorithm ",null,null,null,null,null,null,null,null,"2012-03-11"]
[]
[null,"by Brian Cake, KF2YN"]
[]
[null,"In order to evaluate antenna performance for space communications, it is necessary to compute antenna"]
[null,"temperature, Ta, and the ratio of gain to antenna temperature; G/Ta. NEC is usually the simulation engine, "]
[null,"and YT1NT’s “TANT” software is used to compute the antenna temperature and G/T."]
[]
[null,"Unfortunately NEC, in either NEC2 or NEC4 versions suffers from convergence problems that can lead to erroneous"]
[null,"results."]
[null,"The most common problem is the use of insufficient segmentation density. This can normally be corrected of course by"]
[null,"increasing the number of segments. But in the case where element diameters are large, errors still occur if we increase"]
[null,"the density beyond a point at which it becomes too high compared with the diameter of the element. Another problem"]
[null,"occurs when elements of different diameter are joined together, as might occur with elements made of telescoping  "]
[null,"tubing. Another more serious problem occurs when elements of equal or different diameter are joined at an acute angle. "]
[null,"Folded dipoles and T-matches can suffer from this effect."]
[]
[null,"The convergence errors show up as a value of Average Gain (AG) that is not at or very close to unity (in EZNEC the AG"]
[null,"is displayed below the control console). The AG compares the total power radiated over all angles with the input power. If "]
[null,"the elements have zero loss, the returned AG should of course be 1.000. The number 1.000 equals 100 percent of fed "]
[null,"power to be found  in the sum of power radiated over all angles of the 3D pattern. For this, the simulated gain is correct. "]
[null,"When element loss is included, the AG should always be <1.000. The effect of an AG >1.000 is to give apparent higher "]
[null,"gain, lower loss temperature and higher G/T than one that is perfectly converged.  "]
[]
[null,"The KF2YN convergence error correction algorithm uses modeled data from an antenna having zero loss elements to"]
[null,"correct the gain and antenna temperatures of the same antenna with real-world lossy elements. It corrects poor "]
[null,"convergence by first running the antenna with zero loss elements. Gain and temperature data are entered in the "]
[null,"spreadsheet attached. Second, the antenna is run with actual loss resistance and data are again entered in the"]
[null,"spreadsheet. The spreadsheet calculates the true antenna performance in terms of gain, temperature and G/T."]
[]
[null,"Note that the algorithm does not correct the SWR data,"]
[null,"which for a badly converged antenna may have very significant errors."]

{"sheet":"Charts432MHz_GT","index":5,"n_rows":2,"n_cols":15,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
[]
[null,"432 MHz Charts: 4 Antennas G/T",null,null,null,null,"at Tsky =",{"$f":"' 432.1 MHz Table'!D8","v":27},"K","Tearth =",{"$f":"' 432.1 MHz Table'!H8","v":1800},"K","NF_sys. =",{"$f":"' 432.1 MHz Table'!M8","v":0.75},"K"]

{"sheet":"Charts144MHz_GT","index":6,"n_rows":2,"n_cols":15,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
[]
[null,"144 MHz Charts:",null,"4 Antennas G/T",null,null,"at Tsky =",{"$f":"'144.1 MHz Table'!D8","v":290},"K","Tearth =",{"$f":"'144.1 MHz Table'!H8","v":5400},"K","NF_sys. =",{"$f":"'144.1 MHz Table'!M8","v":0.75},"K"]

{"sheet":"Charts50MHz_Gain","index":7,"n_rows":2,"n_cols":4,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
[]
[null,"50 MHz Charts:",null,"Antenna Gain (dBd)"]

{"sheet":"Charts50MHz_GT","index":8,"n_rows":2,"n_cols":14,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
[]
[null,"50 MHz Charts: 4 Antennas G/T",null,"Antennas G/T",null,"at Tsky =",{"$f":"'50.15 MHz Table'!F8","v":5640},"K","Tearth =",{"$f":"'50.15 MHz Table'!J8","v":100600},"K","NF_sys. =",{"$f":"'50.15 MHz Table'!P8","v":0.75},"K"]